(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (layers
    (0 "F.Cu" signal "Top")
    (31 "B.Cu" signal "Bottom")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pad_to_paste_clearance -0.0508)
    (aux_axis_origin 126.4803 117.6045)
    (grid_origin 126.4803 117.6045)
    (pcbplotparams
      (layerselection 0x00010f8_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/A+")
  (net 3 "/B-")
  (net 4 "/12VswAEn")
  (net 5 "/12Vsnr")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C11-Pad1)")
  (net 8 "Net-(J10-Pad2)")
  (net 9 "Net-(J11-Pad1)")
  (net 10 "/SDA")
  (net 11 "/SCL")
  (net 12 "unconnected-(J21-Pad7)")
  (net 13 "/5Vsw")
  (net 14 "/3Von")
  (net 15 "+3V0")
  (net 16 "/RXp")
  (net 17 "/TXp")
  (net 18 "/TXb")
  (net 19 "/RXb")
  (net 20 "/D4_AL")
  (net 21 "unconnected-(J21-Pad8)")
  (net 22 "unconnected-(J21-Pad9)")
  (net 23 "unconnected-(J21-Pad11)")
  (net 24 "/12Vsw")
  (net 25 "Net-(LED1-Pad2)")
  (net 26 "Net-(LED1-Pad4)")
  (net 27 "unconnected-(J21-Pad12)")
  (net 28 "/sdiProt")
  (net 29 "unconnected-(J21-Pad13)")
  (net 30 "/12Vbst")
  (net 31 "/3.8Vbat")
  (net 32 "/12Vfd")
  (net 33 "/12Vfa")
  (net 34 "/12Vfb")
  (net 35 "/12Vfc")
  (net 36 "/12Vfe")
  (net 37 "unconnected-(J21-Pad14)")
  (net 38 "unconnected-(J21-Pad17)")
  (net 39 "Net-(R2-Pad1)")
  (net 40 "/12Vfg")
  (net 41 "/12Vfh")
  (net 42 "/12Vfm")
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 137.2641 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J1" (at -3.4662 -3.4059) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -1.7019 -1.9354 180) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "/12Vfa") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 151.0791 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J5" (at -5.3512 -2.0059) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -5.08 -3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "/12Vfb") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 164.2871 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN) ")
    (property "Question" "top:vert under:R/A?")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J6" (at -5.0432 -2.0559) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -5.08 -3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "/12Vfc") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 136.5941 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J2" (at 5.6638 1.4041) (layer "F.SilkS"))
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "/12Vfa") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 150.7141 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J7" (at -1.27 -1.397) (layer "F.SilkS") hide)
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "/12Vfb") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:OSHW-LOGO-MINI" (layer "F.Cu")
    (tedit 0)
    (at 168.7141 111.1986)
    (descr "<h3>Open-Source Hardware (OSHW) Logo - Mini - Silkscreen</h3>\n<p>Silkscreen logo for open-source hardware designs.</p>\n<p>Devices using:\n<ul><li>OSHW_LOGO</li></ul></p>")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "na")
    (property "exclude_from_bom" "")
    (attr through_hole exclude_from_bom)
    (fp_text reference "LOGO1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "OSHW-LOGOMINI" (at 0 0) (layer "F.SilkS") hide)
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 163.9841 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J8" (at -1.27 -1.397) (layer "F.SilkS") hide)
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "/12Vfc") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "Connector_Pin:Pin_D1.0mm_L10.0mm_LooseFit" (layer "F.Cu")
    (tedit 5A1DC085)
    (at 181.3303 91.1545)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.2mm (loose fit), length 10.0mm")
    (tags "solder Pin_ loose fit")
    (property "MPN" "19AWG=0.912mm 18Awg=1.024mm")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Wire 19AWG 10\"")
    (attr through_hole)
    (fp_text reference "J9" (at 0.15 2.7) (layer "B.SilkS"))
    (fp_text value "GND Wire" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm_LooseFit.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.1803 109.7045)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0603FR-07649RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-649HRCT-ND")
    (attr smd)
    (fp_text reference "R7" (at 0.05 1.55) (layer "F.SilkS"))
    (fp_text value "649R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/B-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 168.7141 107.7736 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0603FR-07649RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-649HRCT-ND")
    (attr smd)
    (fp_text reference "R8" (at -1.1309 -1.5838 90) (layer "F.SilkS"))
    (fp_text value "649R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/5Vsw") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/A+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.1141 104.5736 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0603FR-07120RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-120HRCT-ND")
    (attr smd)
    (fp_text reference "R9" (at 0 0.1 90) (layer "Dwgs.User"))
    (fp_text value "120R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/A+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.9141 114.8286 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -0.72 0.1 90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+3V0") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 161.9303 108.2045 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.13 0 90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/5Vsw") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.3803 110.5545)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0402FR-07120RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-120LRCT-ND")
    (attr smd)
    (fp_text reference "R3" (at -0.06 0.05) (layer "Dwgs.User"))
    (fp_text value "120R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/TXb") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(LED1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.8303 103.4545 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -0.02 0.2) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/12Vfb") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.9303 110.9545)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0402FR-0762RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-62.0LRCT-ND ")
    (attr smd)
    (fp_text reference "R4" (at 0.29 0.25) (layer "Dwgs.User"))
    (fp_text value "62R" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/RXb") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(LED1-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:SN74LVC2G34DBVT" (layer "F.Cu")
    (tedit 0)
    (at 140.0465 108.874401)
    (property "MPN" "SN74LVC2G34DBVT")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "296-32325-1-ND ")
    (attr through_hole)
    (fp_text reference "U3" (at 0.6338 2.530099) (layer "F.SilkS"))
    (fp_text value "SN74LVC2G34  SOT23" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -1.3716 -2.6518) (layer "F.SilkS") hide)
    (fp_text user "*" (at -1.3716 -2.6518) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User") hide)
    (fp_text user ".058in/1.473mm" (at -1.1176 3.937) (layer "Cmts.User") hide)
    (fp_text user "3.740157E-02in/.95mm" (at -4.1656 -0.475) (layer "Cmts.User") hide)
    (fp_text user ".022in/.559mm" (at 4.1656 -0.95) (layer "Cmts.User") hide)
    (fp_text user ".088in/2.235mm" (at 0 -3.937) (layer "Cmts.User") hide)
    (fp_text user "*" (at -1.3716 -2.6518) (layer "F.Fab") hide)
    (fp_text user "*" (at -1.3716 -2.6518) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -1.1176 -0.950001) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/TXp") (pintype "input"))
    (pad "2" smd rect locked (at -1.1176 0) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.1176 0.950001) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/RXb") (pintype "input"))
    (pad "4" smd rect locked (at 1.1176 0.950001) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/RXp") (pintype "output"))
    (pad "5" smd rect locked (at 1.1176 0) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+3V0") (pinfunction "VCC") (pintype "power_in"))
    (pad "6" smd rect locked (at 1.1176 -0.950001) (size 1.4732 0.5588) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/TXb") (pintype "output"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.4641 106.0486)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 0) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+3V0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical" (layer "F.Cu")
    (tedit 5FC4524B)
    (at 171.7141 104.0486)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (property "MPN" "NRPN012PAEN-RC")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "S5801-01-ND")
    (attr through_hole)
    (fp_text reference "J10" (at 2.032 1.619 90) (layer "F.SilkS"))
    (fp_text value "2mm jumper" (at 0 4.06) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:LED_Kingbright_APBD3224SURKCGKC-F01" (layer "F.Cu")
    (tedit 603E917A)
    (at 165.2641 113.4986 90)
    (descr "Kingbright, dual LED, 3.2 x 2.4 mm SMD")
    (tags "dual led smd")
    (property "MPN" "APBD3224SURKCGKC-F01")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "754-1647-1-ND")
    (attr smd)
    (fp_text reference "LED1" (at -0.7559 2.418 90) (layer "F.SilkS"))
    (fp_text value "APBD3224SURKCGKC-F01" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "*" (at 2.7941 1.5162 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.6 0.7 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+3V0") (pinfunction "A1") (pintype "input"))
    (pad "2" smd rect locked (at 1.6 0.7 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(LED1-Pad2)") (pinfunction "K1") (pintype "input"))
    (pad "3" smd rect locked (at -1.6 -0.7 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+3V0") (pinfunction "A2") (pintype "input"))
    (pad "4" smd rect locked (at 1.6 -0.7 90) (size 1.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(LED1-Pad4)") (pinfunction "K2") (pintype "input"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_Kingbright_AAA3528ESGCT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 170.2641 96.7111 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R10" (at 0.0375 -0.05 90) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/12Vfd") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 133.9941 101.8486 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -0.07 -0.05 180) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/12Vfa") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm" (layer "F.Cu")
    (tedit 5A43C851)
    (at 177.4641 90.9986 180)
    (descr "http://www.molex.com/pdm_docs/sd/022232031_sd.pdf")
    (property "MANUFACTURER" "JST Sales")
    (property "MPN" "ED10562-ND")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10562-ND")
    (attr through_hole)
    (fp_text reference "J19" (at 2.71 -4.59) (layer "F.SilkS"))
    (fp_text value "Wire2Board" (at 2.82 4.63) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0 180) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "/12Vfd") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.8641 105.2986)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC0603FR-07200KL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-200KHRCT-ND")
    (attr smd)
    (fp_text reference "R11" (at 0.05 0.05) (layer "Dwgs.User"))
    (fp_text value "200K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 179.3641 104.9361 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC1206FR-07510RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-510FRCT-ND")
    (attr smd)
    (fp_text reference "R15" (at 0.0655 2.286 90) (layer "F.SilkS"))
    (fp_text value "510R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222213333)
      (net 7 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222213333)
      (net 9 "Net-(J11-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.9581 103.2714 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "C0603C332J5RAC7867")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "399-C0603C332J5RAC7867CT-ND")
    (attr smd)
    (fp_text reference "C11" (at 0.894 0.1228) (layer "Dwgs.User"))
    (fp_text value "3300pF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.6141 113.6111 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "MPN" "RC1206FR-07510RL")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-510FRCT-ND")
    (attr smd)
    (fp_text reference "R12" (at 1.2553 -2.413) (layer "F.SilkS"))
    (fp_text value "510R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222213333)
      (net 7 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222213333)
      (net 28 "/sdiProt") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:SOD-123" (layer "F.Cu")
    (tedit 5D28A50F)
    (at 176.3891 109.4986 180)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://www.diodes.com/assets/Datasheets/ds18010.pdf")
    (property "DK_Detail_Page" "/product-detail/en/diodes-incorporated/MMSZ5231B-7-F/MMSZ5231B-FDICT-ND/755506")
    (property "Description" "DIODE ZENER 5.1V 500MW SOD123")
    (property "Family" "Diodes - Zener - Single")
    (property "MPN" "MMSZ5236BT1G")
    (property "Manufacturer" "Diodes Incorporated")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "Vendor" "MMSZ5236BT1GOSCT-ND")
    (attr smd)
    (fp_text reference "Z1" (at 0.7588 -1.7559) (layer "F.SilkS"))
    (fp_text value "7.5V" (at 0.07 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "A" smd rect locked (at 1.575 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "K" smd rect locked (at -1.575 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C11-Pad1)") (pintype "passive"))
  )
  (footprint "RS485_Mayfly:JST_S3B-PH-K-S(LF)(SN)" (layer "F.Cu")
    (tedit 608069C1)
    (at 177.6641 99.4986 180)
    (property "MPN" "B3B-PH-K-S(LF)(SN)")
    (property "Opts" "Vert: B3B-PH-K-S(LF)(SN)  R/A: S3B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "455-1705-ND")
    (attr through_hole)
    (fp_text reference "J11" (at -3.4162 0.3441) (layer "F.SilkS"))
    (fp_text value "Grove 3pin" (at 12.07775 7.19784) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 4 0 180) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "/12Vfd") (pintype "passive"))
  )
  (footprint "RS485_Mayfly:max13487eesa&plus_" (layer "F.Cu")
    (tedit 0)
    (at 157.5803 106.6545)
    (property "MPN" "max13487eesa+")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "MAX13487EESA+-ND")
    (attr through_hole)
    (fp_text reference "U2" (at -0.4 -3.4) (layer "F.SilkS"))
    (fp_text value "max13487eesa+" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -2.97815 -3.5814) (layer "F.SilkS") hide)
    (fp_text user "*" (at -2.97815 -3.5814) (layer "F.SilkS") hide)
    (fp_text user "0.05in/1.27mm" (at -5.77215 -1.27) (layer "Cmts.User") hide)
    (fp_text user "0.058in/1.46mm" (at -2.72415 4.9149) (layer "Cmts.User") hide)
    (fp_text user "0.021in/0.533mm" (at 5.77215 -1.905) (layer "Cmts.User") hide)
    (fp_text user "0.214in/5.448mm" (at 0 -4.9149) (layer "Cmts.User") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User") hide)
    (fp_text user "*" (at -1.6129 -2.4257) (layer "F.Fab") hide)
    (fp_text user "*" (at -1.6129 -2.4257) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -2.72415 -1.905) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/RXb") (pinfunction "RO") (pintype "output"))
    (pad "2" smd rect locked (at -2.72415 -0.635) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/5Vsw") (pinfunction "*RE") (pintype "input"))
    (pad "3" smd rect locked (at -2.72415 0.635) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/5Vsw") (pinfunction "*SHDN") (pintype "input"))
    (pad "4" smd rect locked (at -2.72415 1.905) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/TXb") (pinfunction "DI") (pintype "input"))
    (pad "5" smd rect locked (at 2.72415 1.905) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd rect locked (at 2.72415 0.635) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/A+") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" smd rect locked (at 2.72415 -0.635) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/B-") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" smd rect locked (at 2.72415 -1.905) (size 1.4605 0.5334) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/5Vsw") (pinfunction "VCC") (pintype "power_in"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 198.7303 97.6045)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0.45 0.1) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/12Vfh") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:B2B-PH-K-SLFSN" (layer "F.Cu")
    (tedit 0)
    (at 128.430101 115.4041 -90)
    (property "MPN" "B2B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "455-1704-ND")
    (attr through_hole)
    (fp_text reference "J4" (at -2.0996 -3.900199 180) (layer "F.SilkS"))
    (fp_text value "LiIon 2pin" (at -1 0 90) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User") hide)
    (fp_text user "*" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/3.8Vbat") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB9E0)
    (at 149.2641 104.9486)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "RC0402FR-073K01L")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "311-1.50KLRCT-ND")
    (attr smd)
    (fp_text reference "R2" (at 0.3475 -0.5) (layer "Dwgs.User"))
    (fp_text value "1.5K" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 211.8641 93.8986)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H05" (at -0.1 -2.45) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.8641 108.0286 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.32 -0.05 90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.2303 98.667 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R13" (at 0.0816 0.05 90) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/12Vfg") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "digikey-footprints:PinHeader_1x3_P2.54mm_Drill1.02mm" (layer "F.Cu")
    (tedit 5A43C851)
    (at 189.6003 114.9545)
    (descr "http://www.molex.com/pdm_docs/sd/022232031_sd.pdf")
    (property "MANUFACTURER" "JST Sales")
    (property "MPN" "ED10562-ND")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10562-ND")
    (attr through_hole)
    (fp_text reference "J13" (at -2.92 -0.95) (layer "F.SilkS"))
    (fp_text value "Wire2Board" (at 2.82 4.63) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.02 2.02) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 "/12Vfe") (pinfunction "3") (pintype "passive"))
  )
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 192.1641 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J14" (at -2.3662 2.9941) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -5.08 -3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "/12Vfg") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 198.8641 93.8986)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H03" (at -0.1 -2.4) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 197.3303 112.3845 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0.45 -1.6 -270) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/12Vfe") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:mouse-bite-2mm-slot" locked (layer "F.Cu")
    (tedit 551DB891)
    (at 184.1303 98.8045 90)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "mouse-bite-2mm-slot" (at 0 -2 90) (layer "Cmts.User") hide)
    (fp_text value "MSB02" (at 0 2.1 90) (layer "Cmts.User") hide)
    (pad "" np_thru_hole circle locked (at 0 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 219.8641 106.8986)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H06" (at -0.0838 4.6559) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.1891 104.9986)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "JMK107ABJ106MA-T ")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -0.175 -0.1) (layer "Dwgs.User"))
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:mouse-bite-2mm-slot" locked (layer "F.Cu")
    (tedit 551DB891)
    (at 184.0803 89.7545 90)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "mouse-bite-2mm-slot" (at 0 -2 90) (layer "Cmts.User") hide)
    (fp_text value "MSB01" (at 0 2.1 90) (layer "Cmts.User") hide)
    (pad "" np_thru_hole circle locked (at -0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 209.8641 113.8986)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H04" (at 3.3162 1.9059) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "RS485_Mayfly:mouse-bite-2mm-slot" locked (layer "F.Cu")
    (tedit 551DB891)
    (at 184.0803 109.0045 90)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "mouse-bite-2mm-slot" (at 0 -2 90) (layer "Cmts.User") hide)
    (fp_text value "MSB04" (at 0 2.1 90) (layer "Cmts.User") hide)
    (pad "" np_thru_hole circle locked (at 0 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "RS485_Mayfly:JST_S3B-PH-K-S(LF)(SN)" (layer "F.Cu")
    (tedit 608069C1)
    (at 190.1803 105.7045)
    (property "MPN" "B3B-PH-K-S(LF)(SN)")
    (property "Options" "Vert Top: B3B-PH-K-S(LF)(SN)  Btm R/A: S3B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "455-1705-ND")
    (attr through_hole)
    (fp_text reference "J20" (at -3.75 3.15) (layer "F.SilkS"))
    (fp_text value "Grove 3pin" (at 12.07775 7.19784) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 4 0) (size 1.308 1.308) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "/12Vfe") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 129.8641 106.8986)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H01" (at -1.4838 -2.4941) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 205.2641 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN) ")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J15" (at -2.3662 3.2441) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -5.08 -3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "/12Vfh") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:B2B-PH-K-SLFSN" (layer "F.Cu")
    (tedit 0)
    (at 128.3641 100.198601 -90)
    (property "MPN" "B2B-PH-K-S(LF)(SN)")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "455-1704-ND")
    (attr through_hole)
    (fp_text reference "J3" (at -5.294101 -0.3162) (layer "F.SilkS"))
    (fp_text value "LiIon 2pin" (at -1 0 90) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User") hide)
    (fp_text user "*" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/3.8Vbat") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.000001 0 270) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 211.7603 97.9545 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0.2559 -0.0662) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/12Vfm") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 135.8641 106.2111 -90)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Description" " Tant 250mOhm 1210 ")
    (property "MPN" "TLJA107M006R0800")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "478-11096-1-ND")
    (attr smd)
    (fp_text reference "C1" (at 3.4375 0.4338 -90) (layer "F.SilkS"))
    (fp_text value "100uF/6V3" (at 0 1.75 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 31 "/3.8Vbat") (pintype "passive"))
    (pad "2" smd roundrect (at 1.35 0 270) (size 1.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:mouse-bite-2mm-slot" locked (layer "F.Cu")
    (tedit 551DB891)
    (at 184.1303 116.3545 90)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "mouse-bite-2mm-slot" (at 0 -2 90) (layer "Cmts.User") hide)
    (fp_text value "MSB05" (at 0 2.1 90) (layer "Cmts.User") hide)
    (pad "" np_thru_hole circle locked (at 0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.8766 101.9486)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R1" (at -0.2125 0.05) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/12Vfa") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.7641 91.5786 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.16 -90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/12Vfc") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 192.0941 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J12" (at -1.27 -1.397) (layer "F.SilkS") hide)
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "/12Vfg") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 205.4441 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J16" (at -1.27 -1.397) (layer "F.SilkS") hide)
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "/12Vfh") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:mouse-bite-2mm-slot" locked (layer "F.Cu")
    (tedit 551DB891)
    (at 184.0803 102.2545 90)
    (attr through_hole board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "mouse-bite-2mm-slot" (at 0 -2 90) (layer "Cmts.User") hide)
    (fp_text value "MSB03" (at 0 2.1 90) (layer "Cmts.User") hide)
    (pad "" np_thru_hole circle locked (at -0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0.75 -0.75 90) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.3803 95.8845 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 2.38 -0.4 90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/12Vfg") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 198.7303 99.9545 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R16" (at 0.0184 -0.1662 -270) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/12Vfh") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:2.0_1X4" (layer "F.Cu")
    (tedit 0)
    (at 218.6641 98.7486 180)
    (property "MPN" "B4B-PH-K-S(LF)(SN)")
    (property "Question" "top:vert under:R/A?")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "0.1*1597-1082-ND")
    (attr through_hole)
    (fp_text reference "J17" (at -2.5162 3.2941) (layer "F.SilkS"))
    (fp_text value "Grove 4pin" (at -5.08 -3.81) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at -3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "/12Vfm") (pinfunction "3") (pintype "bidirectional") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3 0 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "bidirectional") (solder_mask_margin 0.1016))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.7141 95.4111 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R5" (at -0.1125 -0.15 -270) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/12Vfc") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 197.2303 108.542 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R14" (at -0.3375 1.9 90) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/12Vfe") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 170.3641 91.4286 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -0.18 0.05 -90) (layer "Dwgs.User"))
    (fp_text value "0.1uF" (at 0 1.16 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/12Vfd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:1X04_NOSILK" (layer "F.Cu")
    (tedit 0)
    (at 218.8441 90.7086 180)
    (descr "<h3>Plated Through Hole - 4 Pin</h3>\n<p>Specifications:\n<ul><li>Pin count:4</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_04</li>\n</ul></p>")
    (property "MPN" "OSTVN04A150")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "ED10563-ND")
    (attr through_hole)
    (fp_text reference "J18" (at -1.27 -1.397) (layer "F.SilkS") hide)
    (fp_text value "Wire2Board" (at -1.27 2.032) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at -3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/A+") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at -1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/B-") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 1.27 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "/12Vfm") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 3.81 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.6803 104.2295 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "JMK107ABJ106MA-T ")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -0.05 0 90) (layer "Dwgs.User"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/12Vbst") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.7303 103.2545)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R6" (at -0.0125 0) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/12Vfb") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:MP5036GJ-P" (layer "F.Cu")
    (tedit 0)
    (at 149.21415 107.5501 180)
    (property "MPN" " MP5036GJ-P")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "1589-MP5036GJ-PCT-ND")
    (attr through_hole)
    (fp_text reference "U1" (at -0.01615 -2.5544) (layer "F.SilkS"))
    (fp_text value "MP5036" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "0.102in/2.6mm" (at 0 3.998) (layer "Cmts.User") hide)
    (fp_text user "0.037in/0.95mm" (at -4.348 -0.475) (layer "Cmts.User") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User") hide)
    (fp_text user "0.047in/1.194mm" (at -1.3 -4.5466) (layer "Cmts.User") hide)
    (fp_text user "0.024in/0.61mm" (at 4.348 -0.95) (layer "Cmts.User") hide)
    (fp_text user "*" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -1.3 -0.950001 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/12VswAEn") (pinfunction "EN") (pintype "unspecified"))
    (pad "2" smd rect locked (at -1.3 0 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/12Vsnr") (pinfunction "SOURCE") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.3 0.950001 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.3 0.950001 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(R2-Pad1)") (pinfunction "ILIMIT") (pintype "unspecified"))
    (pad "5" smd rect locked (at 1.3 0 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/12Vbst") (pinfunction "VIN") (pintype "power_in"))
    (pad "6" smd rect locked (at 1.3 -0.950001 180) (size 1.1938 0.6096) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C5-Pad2)") (pinfunction "DV/DT") (pintype "unspecified"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 172.8641 113.8986 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H02" (at 0 -4.2 90) (layer "Dwgs.User"))
    (fp_text value "MountingHole_3.2mm_M3" (at 0 4.2 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 211.7803 100.292 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "MPN" "PRG18BC3R3MM1RB")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "490-8506-1-ND")
    (attr smd)
    (fp_text reference "R17" (at 0.0684 -0.2162 -270) (layer "Dwgs.User"))
    (fp_text value "eFuse 120mA" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/12Vfm") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/12Vsnr") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:2X10" locked (layer "B.Cu")
    (tedit 0)
    (at 136.9821 113.1266)
    (descr "<h3>Plated Through Hole - 2x10</h3>\n<p>Specifications:\n<ul><li>Pin count:20</li>\n<li>Pin pitch:0.1\"</li>\n</ul></p>\n<p>Example device(s):\n<ul><li>CONN_10x2</li>\n</ul></p>")
    (property "MPN" "67996-220HLF")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "609-3214-ND")
    (solder_paste_margin -0.5)
    (attr through_hole)
    (fp_text reference "J21" (at -3.0018 3.8779) (layer "B.SilkS"))
    (fp_text value "Mayfly 10X2" (at -1.27 -2.413) (layer "B.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle locked (at 0 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "/3Von") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle locked (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/TXp") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle locked (at 2.54 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "/D4_AL") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle locked (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "/sdiProt") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle locked (at 5.08 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/RXp") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle locked (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J21-Pad7)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle locked (at 7.62 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J21-Pad8)") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle locked (at 10.16 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J21-Pad9)") (pinfunction "9") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle locked (at 10.16 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "/12VswAEn") (pinfunction "10") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle locked (at 12.7 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J21-Pad11)") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle locked (at 12.7 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J21-Pad12)") (pinfunction "12") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "13" thru_hole circle locked (at 15.24 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J21-Pad13)") (pinfunction "13") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "14" thru_hole circle locked (at 15.24 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J21-Pad14)") (pinfunction "14") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "15" thru_hole circle locked (at 17.78 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "/SCL") (pinfunction "15") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "16" thru_hole circle locked (at 17.78 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "/SDA") (pinfunction "16") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "17" thru_hole circle locked (at 20.32 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J21-Pad17)") (pinfunction "17") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "18" thru_hole circle locked (at 20.32 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "/12Vsw") (pinfunction "18") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "19" thru_hole circle locked (at 22.86 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "/5Vsw") (pinfunction "19") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "20" thru_hole circle locked (at 22.86 2.54) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "+3V0") (pinfunction "20") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "RS485_Mayfly:Pololu4016_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A430)
    (at 143.8141 108.4486)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (property "MPN" "polou U3V40F12")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "2183-4016-ND")
    (attr through_hole)
    (fp_text reference "U4" (at 1.5662 -14.7941) (layer "B.SilkS"))
    (fp_text value "Boost +12V" (at 0 -15.47) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -6.35 90) (layer "B.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "+3V0") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "/3.8Vbat") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "/3.8Vbat") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "/12Vbst") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RS485_Mayfly:E2,5-6E" (layer "B.Cu")
    (tedit 0)
    (at 164.7641 106.1286 -90)
    (descr "<b>ELECTROLYTIC CAPACITOR</b><p>\ngrid 2.54 mm, diameter 6 mm")
    (property "Descr" "330uF/16V")
    (property "MPN" " 860020373011")
    (property "Sheetfile" "File: KNH002rev8.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "732-8798-1-ND")
    (attr through_hole)
    (fp_text reference "C17" (at 4.4259 1.75 180) (layer "B.SilkS"))
    (fp_text value "330uF/16V Elec" (at 2.667 -2.54 90) (layer "B.Fab") hide)
    (pad "+" thru_hole circle locked (at -1.27 0 270) (size 1.5748 1.5748) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "/12Vsnr") (pinfunction "+") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "-" thru_hole circle locked (at 1.27 0 270) (size 1.5748 1.5748) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (gr_line (start 224.8803 88.4045) (end 131.6041 88.4045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 126.4141 93.6486) (end 126.4141 117.6986) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 224.9141 117.7486) (end 224.8803 88.4045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 126.4141 117.6986) (end 224.9141 117.7486) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 131.6041 88.4045) (end 126.4141 93.6486) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.3803 114.9545) (end 183.3803 110.3045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.3803 110.3045) (end 184.8303 110.3045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.4053 97.3045) (end 184.8553 97.3045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8303 103.5045) (end 184.8303 107.6045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8303 114.9545) (end 183.3803 114.9545) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.3803 103.5045) (end 184.8303 103.5045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8303 107.6045) (end 183.3803 107.6045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8303 110.3045) (end 184.8303 114.9545) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8303 92.1045) (end 183.3803 92.1045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.3803 92.1045) (end 183.4053 97.3045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 184.8553 97.3045) (end 184.8303 92.1045) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 183.3803 107.6045) (end 183.3803 103.5045) (layer "Edge.Cuts") (width 0.05))
  (gr_text "+" (at 130.9803 116.7045 270) (layer "B.SilkS"))
  (gr_text "KNH002r8b4" (at 169.6141 116.7986) (layer "B.SilkS"))
  (gr_text "V G D" (at 175.3641 101.4486 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 205.3803 93.2045 180) (layer "B.SilkS"))
  (gr_text "+" (at 134.9303 115.1545 270) (layer "B.SilkS"))
  (gr_text "G V B A" (at 164.5141 92.7986 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 218.4303 93.2045 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 150.8141 92.4986 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 192.0803 93.2045 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 164.3641 101.5986 180) (layer "B.SilkS"))
  (gr_text "V G D " (at 176.2141 93.3986 180) (layer "B.SilkS"))
  (gr_text "OUT" (at 140.9303 94.7045 180) (layer "B.SilkS"))
  (gr_text "+" (at 164.6803 102.4045 270) (layer "B.SilkS"))
  (gr_text "G V B A" (at 136.7141 92.9986 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 150.8303 102.0045 180) (layer "B.SilkS"))
  (gr_text "D G V" (at 191.7803 112.6045 180) (layer "B.SilkS"))
  (gr_text "+" (at 143.2803 93.3545 270) (layer "B.SilkS"))
  (gr_text "+" (at 127.4303 101.5545 270) (layer "B.SilkS"))
  (gr_text "G V B A" (at 136.8803 100.6045 180) (layer "B.SilkS"))
  (gr_text "G V B A" (at 164.8803 102.0545) (layer "F.SilkS"))
  (gr_text "G V B A" (at 151.0303 101.6045) (layer "F.SilkS"))
  (gr_text "*" (at 134.2641 103.7834) (layer "F.SilkS"))
  (gr_text "*" (at 137.8141 107.0486) (layer "F.SilkS"))
  (gr_text "+" (at 134.9501 115.1586 270) (layer "F.SilkS"))
  (gr_text "V G D " (at 175.4141 101.5486) (layer "F.SilkS"))
  (gr_text "GND" (at 164.8803 109.3545) (layer "F.SilkS"))
  (gr_text "*" (at 155.0803 104.0045) (layer "F.SilkS"))
  (gr_text "G V B A" (at 192.5303 102.4045) (layer "F.SilkS"))
  (gr_text "Mayfly Modbus 2" (at 209.3803 109.1545) (layer "F.SilkS"))
  (gr_text "+" (at 162.8803 103.9545) (layer "F.SilkS"))
  (gr_text "KNH002r8b4" (at 168.6641 117.0486) (layer "F.SilkS"))
  (gr_text "G V B A" (at 136.9303 100.4545) (layer "F.SilkS"))
  (gr_text "+12V" (at 199.2803 105.2545) (layer "F.SilkS"))
  (gr_text "G V B A" (at 218.0803 102.6045) (layer "F.SilkS"))
  (gr_text "MM2" (at 180.9303 110.2545 90) (layer "F.SilkS"))
  (gr_text "*" (at 152.0303 108.9045) (layer "F.SilkS"))
  (gr_text "D G V " (at 192.5303 109.5545) (layer "F.SilkS"))
  (gr_text "G V B A" (at 204.9303 102.4045) (layer "F.SilkS"))
  (gr_text "*" (at 177.5303 107.9545) (layer "F.SilkS"))
  (gr_text "+12V" (at 199.2803 115.3545) (layer "F.SilkS"))
  (gr_text "*" (at 163.1803 111.2045) (layer "F.SilkS"))
  (gr_text "+" (at 130.3141 107.4986 270) (layer "Dwgs.User"))
  (gr_text " gnd +V  B  A  gnd +V  B  A   gnd +V  B  A" (at 147.32 93.98) (layer "F.Fab"))
  (gr_text "Mayfly" (at 170.0021 100.6806 90) (layer "F.Fab"))
  (gr_text "SMC\nRS-485" (at 145.8721 109.8246) (layer "F.Fab"))
  (gr_text "6 Holes\n3.2mm" (at 120.9303 103.1545) (layer "User.1"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 183.5303 117.6045) (xy 126.5141 117.6986))
    (height -3.937)
    (gr_text "57 mm" (at 154.9303 122.7545 0.09456133444) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 224.9803 120.8045) (xy 126.5303 120.604563))
    (height -3.950007)
    (gr_text "98.5 mm" (at 175.749613 123.504533 -0.1163582857) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 228.401402 117.8486) (xy 228.372503 88.851507))
    (height 4.0289)
    (gr_text "29 mm" (at 234.21585 103.344245 -89.94290004) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 196.0303 91.1045) (xy 201.7303 91.1045))
    (height -4.45)
    (gr_text "5.7 mm" (at 198.8803 85.5045) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 209.3803 90.9545) (xy 215.0803 90.9545))
    (height -4.5)
    (gr_text "5.7 mm" (at 212.2303 85.3045) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 154.4641 90.8486) (xy 160.1641 90.8486))
    (height -3.8)
    (gr_text "5.7 mm" (at 157.3141 85.8986) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 1))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 167.7641 91.0986) (xy 172.4303 91.1545))
    (height -4.35)
    (gr_text "4.7 mm" (at 170.163084 85.626945 359.3136426) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 146.9303 90.7045) (xy 140.4303 90.7045))
    (height 3.55)
    (gr_text "6.5 mm" (at 143.6803 86.0045) (layer "Cmts.User"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 129.9303 107.0545) (xy 126.3803 107.0545))
    (height -13.1)
    (gr_text "4 mm" (at 129.3303 118.7045) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 0))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 198.926169 92.10455) (xy 211.926169 92.10455))
    (height -7.6)
    (gr_text "13 mm" (at 205.426169 83.35455) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 129.9803 117.7545) (xy 129.9803 106.7545))
    (height -7.6)
    (gr_text "11 mm" (at 121.2303 112.2545 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 209.940024 113.254507) (xy 172.9803 113.1045))
    (height -7.05)
    (gr_text "37 mm" (at 191.436216 119.079455 -0.2325413336) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 206.3803 114.0545) (xy 206.3803 107.1045))
    (height 21.35)
    (gr_text "7 mm" (at 226.5803 110.5795 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 172.9803 114.8986) (xy 129.942581 114.904514))
    (height -5.25)
    (gr_text "43 mm" (at 151.462004 119.001557 0.007873262191) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 212.6303 94.1545) (xy 212.6803 107.1045))
    (height -15.000036)
    (gr_text "13 mm" (at 228.805215 100.567145 270.2212181) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 129.8803 105.4545) (xy 198.8803 105.6045))
    (height -21.1)
    (gr_text "69 mm" (at 164.428669 83.279553 359.8754442) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 132.0803 106.7045) (xy 132.0803 113.6545))
    (height 7.3)
    (gr_text "7 mm" (at 123.6303 110.6045 90) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 209.8803 114.1545) (xy 221.8803 114.1045))
    (height 6.05)
    (gr_text "12 mm" (at 215.900716 119.029457 0.2387310331) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 1) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.099171 114.564028)
        (xy 135.712671 114.310028)
        (xy 135.585671 97.546028)
        (xy 133.998171 97.546028)
        (xy 132.601171 94.244028)
        (xy 132.601171 90.434028)
        (xy 179.718171 90.434028)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 222.8803 117.0545)
        (xy 186.2303 117.0545)
        (xy 186.2303 88.7045)
        (xy 222.8803 88.7045)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 223.5803 117.0045)
        (xy 186.2303 117.0045)
        (xy 186.2303 88.9045)
        (xy 223.5803 88.9045)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.572852 89.067132)
        (xy 181.318852 113.197132)
        (xy 128.867852 113.197132)
        (xy 128.853646 94.900595)
        (xy 131.220055 94.4144)
        (xy 131.534852 91.861132)
        (xy 133.953646 89.000595)
        (xy 134.963852 89.000595)
      )
    )
  )
)
