(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 23)
    (no_connects 0)
    (area 127.940999 89.840999 151.459001 108.787001)
    (thickness 1.6)
    (drawings 9)
    (tracks 65)
    (zones 0)
    (modules 11)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 C)
  (net 2 A)
  (net 3 B)
  (net 4 GND)
  (net 5 +5V)
  (net 6 "Net-(D1-Pad2)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.15)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A)
    (add_net B)
    (add_net C)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 587A6311)
    (at 131.064 92.964 270)
    (fp_text reference J1 (at 6.604 1.524 270) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312 270) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 0 270) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 7 thru_hole circle (at 3.81 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 6 thru_hole circle (at 4.826 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole circle (at 6.858 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at 8.89 -4.318 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at 5.842 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 C))
    (pad 3 thru_hole circle (at 7.874 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 B))
    (pad 1 thru_hole circle (at 9.906 -2.54 270) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 A))
    (pad "" thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 270) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587A6302)
    (at 144.78 101.6 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference A (at -0.762 -2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 A))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587A6306)
    (at 144.78 96.52 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference B (at 0 -2.39 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 B))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 587A6308)
    (at 144.78 91.44 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference C (at 0 -2.39 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 C))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 587A637E)
    (at 142.2654 99.06 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 0.0254 270) (layer F.SilkS))
    (fp_text value C (at 0 1.2954 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 587A5835)
    (at 145.415 104.14 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.0508 -0.0762 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 587A592E)
    (at 145.415 99.06 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.0508 -0.0508 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 587A5928)
    (at 145.415 93.98 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0.0254 -0.0254 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 C))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RJ45:LED_0805_SILK (layer F.Cu) (tedit 587A58A1)
    (at 149.225 93.98 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module RJ45:LED_0805_SILK (layer F.Cu) (tedit 587A58A1)
    (at 149.225 99.06 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module RJ45:LED_0805_SILK (layer F.Cu) (tedit 587A58A1)
    (at 149.225 104.14 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text FRC2168 (at 129.286 99.314 90) (layer B.SilkS))
  (gr_line (start 151.384 89.916) (end 128.016 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.384 108.712) (end 151.384 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.016 108.712) (end 151.384 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.016 89.916) (end 128.016 108.712) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text Gnd (at 149.86 106.68 90) (layer F.SilkS))
  (gr_text "\nRJ45->\n3xDIO/PWM/ANA\nv0.2" (at 138.7348 99.2632 90) (layer B.SilkS))
  (gr_text Sig (at 144.78 106.68 90) (layer F.SilkS))
  (gr_text 5V (at 147.32 106.68 90) (layer F.SilkS))
)
