<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="110" y2="0" width="0" layer="20"/>
<wire x1="110" y1="0" x2="110" y2="5.08" width="0" layer="20"/>
<wire x1="110" y1="12.065" x2="110" y2="50" width="0" layer="20"/>
<wire x1="110" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="0" width="0" layer="20"/>
<text>AIS Ethernet IRD</text>
<text>www.open-hw.net</text>
<text>Based on a design by Alex Scafidas</text>
<text>http://www.tekmanoid.com/ais.shtml</text>
<text>v2.00a</text>
<text>5.5-18VDC</text>
<text>PZW 20-04-14</text>
<text>External
receiver</text>
<wire x1="110" y1="12.065" x2="108.585" y2="12.065" width="0" layer="20"/>
<wire x1="108.585" y1="12.065" x2="108.585" y2="5.08" width="0" layer="20"/>
<wire x1="108.585" y1="5.08" x2="110" y2="5.08" width="0" layer="20"/>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
</packages>
</library>
<library name="cmx589">
<packages>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="PZW">
<packages>
<package name="NRX1FLAT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="AUDIO-JACK">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CT6">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Copal</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="OSHW">
<packages>
<package name="OSHW_FILLX200_TNAMES.PAC">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="lantronix">
<description>&lt;b&gt;LANTRONIX&lt;/b&gt;&lt;p&gt;
WIPORT&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="XPORT">
<description>&lt;b&gt;Serial to 10/100 Ethernet transceiver&lt;/b&gt;&lt;p&gt;
Source: http://www.lantronix.com/pdf/XPort_DS.pdf</description>
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BU-SMA-G">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 193-9117</description>
</package>
</packages>
</library>
<library name="work">
<packages>
<package name="R-78EXX">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC3" library="cmx589" package="TSSOP24" value="CMX589">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="0207/2V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C025-025X050" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="crystal" package="HC49/S" value="4.9152M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="Q1" library="crystal" package="HC49/S" value="8MHZ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C12" library="rcl" package="C025-024X044" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C025-024X044" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C025-024X044" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C025-024X044" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0207/10" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="0207/2V" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C025-025X050" value="15N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C025-025X050" value="15N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="0207/2V" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="0207/2V" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="0207/2V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="0207/2V" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="POWER">
<attribute name="VALUE"/>
</element>
<element name="M1" library="PZW" package="NRX1FLAT" value="NRX1H">
<attribute name="NAME"/>
</element>
<element name="C11" library="rcl" package="E2,5-5" value="100µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun-Connectors" package="BNC" value="BNC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="atmel" package="DIL28-3" value="ATMega 8">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="0207/10" value="510k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="0207/2V" value="180k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GAIN" library="pot" package="CT6" value="500k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO41-7" value="1N4004">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C025-025X050" value="10N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="OSHW" package="OSHW_FILLX200_TNAMES.PAC" value="OSHW_LOGO_FILLX0200-NT-TN"/>
<element name="C1" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="Power">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="R3" library="rcl" package="0207/2V" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0207/2V" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="E2,5-5" value="1µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="lantronix" package="XPORT" value="XPORT">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-coax" package="BU-SMA-G" value="SMA">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="SparkFun-Connectors" package="AUDIO-JACK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PROG" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH">
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="C025-025X050" value="100N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="work" package="R-78EXX" value="R-78E3.3-0.5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="CRC">
<attribute name="VALUE"/>
</element>
<element name="IC4" library="linear" package="DIL08" value="LM358N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSSI" library="pinhead" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="E5-10,5" value="470µ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="12"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IC3" pad="17"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="M1" pad="0V"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="22"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="22"/>
<contactref element="C14" pad="2"/>
<contactref element="C11" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="X3" pad="GND"/>
<contactref element="X3" pad="GNDBREAK"/>
<contactref element="C8" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="RESET" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="3"/>
<contactref element="X5" pad="1"/>
<contactref element="X5" pad="1"/>
<contactref element="X5" pad="SH1"/>
<contactref element="X5" pad="SH2"/>
<contactref element="M1" pad="RF_GND"/>
<contactref element="X1" pad="GND"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="5"/>
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="3"/>
<contactref element="X4" pad="RSH"/>
<contactref element="X4" pad="RING"/>
<contactref element="X4" pad="SLEEVE"/>
<contactref element="PROG" pad="6"/>
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="GND"/>
<contactref element="LED2" pad="K"/>
<contactref element="IC4" pad="4"/>
<contactref element="C6" pad="-"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$19">
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="N$20">
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="N$21">
<contactref element="IC3" pad="7"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="N$28">
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$29">
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$36">
<contactref element="R1" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="PROG" pad="5"/>
</signal>
<signal name="N$37">
<contactref element="IC3" pad="20"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$38">
<contactref element="IC3" pad="21"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="IC3" pad="13"/>
<contactref element="C16" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="14"/>
<contactref element="C17" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="VCC">
<contactref element="IC3" pad="15"/>
<contactref element="IC3" pad="18"/>
<contactref element="IC3" pad="24"/>
<contactref element="IC3" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="20"/>
<contactref element="M1" pad="VCC"/>
<contactref element="C8" pad="1"/>
<contactref element="PROG" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="X5" pad="3"/>
<contactref element="C11" pad="+"/>
<contactref element="IC1" pad="OUT"/>
<contactref element="R7" pad="2"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="2"/>
<contactref element="X5" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="3"/>
<contactref element="X5" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="C13" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC3" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC3" pad="10"/>
<contactref element="C10" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SIG">
<contactref element="IC3" pad="11"/>
<contactref element="C10" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VBIAS">
<contactref element="IC3" pad="9"/>
<contactref element="C14" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="IN"/>
<contactref element="C6" pad="+"/>
</signal>
<signal name="N$12">
<contactref element="D1" pad="A"/>
<contactref element="X3" pad="PWR"/>
</signal>
<signal name="N$31">
<contactref element="LED1" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R8" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="M1" pad="RF_IN"/>
<contactref element="X1" pad="S"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R6" pad="2"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R4" pad="1"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="M1" pad="AF"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$23">
<contactref element="C9" pad="-"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="PROG" pad="3"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="N$11">
<contactref element="PROG" pad="1"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="N$24">
<contactref element="IC2" pad="17"/>
<contactref element="PROG" pad="4"/>
</signal>
<signal name="N$25">
<contactref element="IC2" pad="21"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="GAIN" pad="E"/>
</signal>
<signal name="N$27">
<contactref element="M1" pad="RSSI"/>
<contactref element="RSSI" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="GAIN" pad="S"/>
<contactref element="GAIN" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="X4" pad="TIP"/>
</signal>
<signal name="N$26">
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
