(kicad_pcb (version 4) (host pcbnew 4.0.1-3.201512221402+6198~38~ubuntu14.04.1-stable)
  (general
    (links 29)
    (no_connects 1)
    (area 97.852159 72.922 178.510001 123.265001)
    (thickness 1.6)
    (drawings 34)
    (tracks 102)
    (zones 0)
    (modules 8)
    (nets 18)
  )
  (page A4)
  (title_block
    (title "Temperature Monitor Teensy Hat")
    (date 2016-07-30)
    (rev v1.0)
    (company "Released under the CERN Open Hardware License v1.2")
    (comment 1 "wickerboxen@gmail.com - http://wickerbox.net")
    (comment 2 "Designed by Jenner at Wickerbox Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x30000_00000000)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 +3V3)
  (net 4 GND)
  (net 5 +5V)
  (net 6 "Net-(LCD1-Pad3)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "Net-(J1-Pad6)")
  (net 10 "Net-(J1-Pad8)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad10)")
  (net 13 "Net-(J1-Pad11)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad13)")
  (net 16 "Net-(J1-Pad14)")
  (net 17 "Net-(J1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(LCD1-Pad3)")
  )
  (module Wickerlib:SOIC-8-3.9x4.9MM-P1.27MM (layer F.Cu) (tedit 57903FBD)
    (at 168.656 89.916 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -0.508 90) (layer F.Fab))
    (fp_text value MAX31855 (at 0 1.27 90) (layer F.Fab) hide)
    (fp_text user %R (at 4.572 -2.032 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad13)"))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad14)"))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad12)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 168.898 100.076 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C1 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.07 -1.51 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 172.72 92.964 270)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C2 (at 0.09 0.04 270) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.54 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:CONN-ONSHORE-SCREW-GREEN-2PIN-TH (layer F.Cu) (tedit 579D849E)
    (at 169.164 106.172 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 1.27 270) (layer F.Fab))
    (fp_text value THERMO (at -2.286 1.27 360) (layer F.Fab) hide)
    (fp_text user %R (at 0.508 -2.54 360) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Wickerlib:LCD-1602A locked (layer B.Cu) (tedit 57902DAA)
    (at 170.18 79.756 180)
    (descr http://www.kamami.pl/dl/wc1602a0.pdf)
    (tags "LCD 16x2 Alphanumeric 16pin")
    (fp_text reference LCD1 (at 19.05 0 180) (layer B.Fab))
    (fp_text value LCD-MODULE-16X2-CHARACTER-1602A-CUSTOM1 (at 31.99892 -15.49908 180) (layer B.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 5 +5V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(LCD1-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole oval (at 25.4 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(J1-Pad8)"))
    (pad 12 thru_hole oval (at 27.94 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(J1-Pad9)"))
    (pad 13 thru_hole oval (at 30.48 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(J1-Pad10)"))
    (pad 14 thru_hole oval (at 33.02 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(J1-Pad11)"))
    (pad 15 thru_hole oval (at 35.56 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 5 +5V))
    (pad 16 thru_hole oval (at 38.1 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 0 thru_hole circle (at -5.4991 0 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at -5.4991 -31.0007 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at 69.49948 -31.0007 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at 69.49948 0 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module Wickerlib:RES-TRIMPOT-BOURNS-3362-SQUARE-TH-CENTER (layer F.Cu) (tedit 5790459A)
    (at 122.936 83.82)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference R1 (at 0 0 90) (layer F.Fab))
    (fp_text value 10K (at 0.508 0.254 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.54 5.08) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(LCD1-Pad3)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
  )
  (module Wickerlib:SPEAKER-CMT-1603 (layer F.Cu) (tedit 579D801C)
    (at 107.188 94.996 270)
    (fp_text reference SPK1 (at 0 0 270) (layer F.Fab))
    (fp_text value BUZZER (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at -9.144 -5.588 360) (layer F.SilkS))
    (pad 1 smd rect (at -7.65 0 270) (size 5.7 4.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad20)"))
    (pad 2 smd rect (at 7.5 0 270) (size 5.7 4.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:TEENSY-3.2-NOSILK (layer F.Cu) (tedit 579D85BE)
    (at 146.812 102.616 270)
    (fp_text reference J1 (at -2 0 270) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 25.4 270) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -10.16 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -10.16 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -10.16 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad12)"))
    (pad VBAT thru_hole circle (at -7.62 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V1 thru_hole circle (at -5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad G2 thru_hole circle (at -2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad PGM thru_hole circle (at 0 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad DAC thru_hole circle (at 2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad13)"))
    (pad 16 thru_hole circle (at 5.08 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 18 thru_hole circle (at 5.08 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 5.08 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AG thru_hole circle (at 5.08 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad VIN thru_hole circle (at 5.08 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 21 thru_hole circle (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 5.08 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 5.08 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text 7/30/2016 (at 170.942 115.824) (layer F.Fab))
  (gr_text "Temperature Monitor Teensy Hat  v1.0" (at 155.702 74.422) (layer F.Fab))
  (gr_text wickerbox.net (at 100.5078 94.615 90) (layer B.SilkS))
  (gr_text "Temperature Monitor Teensy Hat  v1.0\n7/30/2016" (at 149.3012 99.9236) (layer B.SilkS))
  (gr_text 1 (at 172.72 79.8576) (layer F.SilkS))
  (gr_text 16 (at 128.8542 79.9084) (layer F.SilkS))
  (gr_text "TEENSY 3.2" (at 152.908 110.744) (layer F.SilkS))
  (gr_text THERMO (at 168.148 110.744) (layer F.SilkS))
  (gr_line (start 98.044 77.216) (end 178.308 77.216) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.044 113.284) (end 98.044 77.216) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.308 113.284) (end 98.044 113.284) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178.308 77.216) (end 178.308 113.284) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.308 77.216) (xy 178.308 113.284) (xy 98.044 113.284) (xy 98.044 77.216)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.308 77.216) (xy 178.308 113.284) (xy 98.044 113.284) (xy 98.044 77.216)
      )
    )
  )
)
