(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 175)
    (zones 0)
    (modules 26)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x310fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbs/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VUSB)
  (net 3 VCC)
  (net 4 "Net-(D1-Pad1)")
  (net 5 /RXOKLED)
  (net 6 /SFDLED)
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 /RXLED)
  (net 10 /TXLED)
  (net 11 "Net-(D4-Pad1)")
  (net 12 "Net-(D5-Pad2)")
  (net 13 /IO4-PC12)
  (net 14 /IO3)
  (net 15 /SWCLK)
  (net 16 /SWDIO)
  (net 17 /I2C_SCL-PB6)
  (net 18 /I2C_SDA-PB7)
  (net 19 /RESET_n)
  (net 20 /IRQ)
  (net 21 /VCC_3V)
  (net 22 /UART2_RX)
  (net 23 /UART2_TX)
  (net 24 /VCOM)
  (net 25 "/SCK(PA5)")
  (net 26 "/MISO(PA6)")
  (net 27 /WKUP-P0.12)
  (net 28 /N_IO_1-P0.11)
  (net 29 "/MOSI(PA7)")
  (net 30 /LIS_SCL)
  (net 31 /LIS_SDA)
  (net 32 /LIS_INT2)
  (net 33 "Net-(U1-Pad4)")
  (net 34 "Net-(U2-Pad2)")
  (net 35 "Net-(U2-Pad6)")
  (net 36 "Net-(U2-Pad7)")
  (net 37 "Net-(U2-Pad8)")
  (net 38 "Net-(U2-Pad15)")
  (net 39 "Net-(U2-Pad19)")
  (net 40 "Net-(U2-Pad20)")
  (net 41 "Net-(U2-Pad21)")
  (net 42 "Net-(U2-Pad22)")
  (net 43 "Net-(U2-Pad23)")
  (net 44 "Net-(U2-Pad37)")
  (net 45 "Net-(U2-Pad36)")
  (net 46 "Net-(U2-Pad29)")
  (net 47 "Net-(U2-Pad35)")
  (net 48 "Net-(U2-Pad30)")
  (net 49 "Net-(D5-Pad1)")
  (net 50 "Net-(JP1-Pad1)")
  (net 51 /OW)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /I2C_SCL-PB6)
    (add_net /I2C_SDA-PB7)
    (add_net /IO3)
    (add_net /IO4-PC12)
    (add_net /IRQ)
    (add_net /LIS_INT2)
    (add_net /LIS_SCL)
    (add_net /LIS_SDA)
    (add_net "/MISO(PA6)")
    (add_net "/MOSI(PA7)")
    (add_net /N_IO_1-P0.11)
    (add_net /OW)
    (add_net /RESET_n)
    (add_net /RXLED)
    (add_net /RXOKLED)
    (add_net "/SCK(PA5)")
    (add_net /SFDLED)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /TXLED)
    (add_net /UART2_RX)
    (add_net /UART2_TX)
    (add_net /VCC_3V)
    (add_net /VCOM)
    (add_net /VUSB)
    (add_net /WKUP-P0.12)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 180.975 84.455)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VUSB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 173.115 81.915 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1uf (at 2.3635 0.1905 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 177.165 79.375)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value RXOK (at 5.5245 0.0635) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RXOKLED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 177.165 77.47)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value SFD (at 4.826 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /SFDLED))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 177.165 75.565)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value RX (at 4.5085 -0.0635) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /RXLED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 177.165 73.66)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value TX (at 4.318 -0.0635) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /TXLED))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bitcraze:CF2-DECK-SMD-HOLES (layer F.Cu) (tedit 570E483E)
    (at 185.42 66.04 180)
    (attr smd)
    (fp_text reference P1 (at 0 0.1) (layer F.SilkS))
    (fp_text value CF_EXP_LEFT (at 11.43 0 90) (layer F.SilkS))
    (fp_text user 1 (at -9 2) (layer F.SilkS))
    (fp_text user 10 (at 9 -1.9) (layer F.SilkS))
    (pad 10 smd circle (at 9 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin -0.05))
    (pad 9 smd circle (at 7 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 13 /IO4-PC12) (solder_mask_margin -0.05))
    (pad 8 smd circle (at 5 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 14 /IO3) (solder_mask_margin -0.05))
    (pad 7 smd circle (at 3 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 15 /SWCLK) (solder_mask_margin -0.05))
    (pad 6 smd circle (at 1 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 16 /SWDIO) (solder_mask_margin -0.05))
    (pad 5 smd circle (at -1 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 17 /I2C_SCL-PB6) (solder_mask_margin -0.05))
    (pad 4 smd circle (at -3 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 18 /I2C_SDA-PB7) (solder_mask_margin -0.05))
    (pad 3 smd circle (at -5 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 19 /RESET_n) (solder_mask_margin -0.05))
    (pad 2 smd circle (at -7 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 20 /IRQ) (solder_mask_margin -0.05))
    (pad 1 smd circle (at -9 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 21 /VCC_3V) (solder_mask_margin -0.05))
    (pad 10 smd rect (at 9 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /IO4-PC12))
    (pad 8 smd rect (at 5 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /IO3))
    (pad 7 smd rect (at 3 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /SWCLK))
    (pad 6 smd rect (at 1 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /SWDIO))
    (pad 5 smd rect (at -1 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /I2C_SCL-PB6))
    (pad 4 smd rect (at -3 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /I2C_SDA-PB7))
    (pad 3 smd rect (at -5 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET_n))
    (pad 2 smd rect (at -7 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /IRQ))
    (pad 1 smd rect (at -9 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /VCC_3V))
    (pad 5 thru_hole circle (at -1 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 17 /I2C_SCL-PB6))
    (pad 6 thru_hole circle (at 1 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 16 /SWDIO))
    (pad 7 thru_hole circle (at 3 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 15 /SWCLK))
    (pad 4 thru_hole circle (at -3 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 18 /I2C_SDA-PB7))
    (pad 3 thru_hole circle (at -5 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 19 /RESET_n))
    (pad 9 thru_hole circle (at 7 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 13 /IO4-PC12))
    (pad 8 thru_hole circle (at 5 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 14 /IO3))
    (pad 1 thru_hole rect (at -9 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 21 /VCC_3V))
    (pad 2 thru_hole circle (at -7 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 20 /IRQ))
    (pad 10 thru_hole circle (at 9 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 1 GND))
  )
  (module Bitcraze:CF2-DECK-SMD-HOLES (layer F.Cu) (tedit 570E483E)
    (at 185.42 88.265 180)
    (attr smd)
    (fp_text reference P2 (at 0 0.1) (layer F.SilkS))
    (fp_text value CF_EXP_RIGHT (at 11.43 0.635 90) (layer F.SilkS))
    (fp_text user 10 (at 9 -1.9) (layer F.SilkS))
    (fp_text user 1 (at -9 2) (layer F.SilkS))
    (pad 10 thru_hole circle (at 9 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 2 /VUSB))
    (pad 2 thru_hole circle (at -7 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 22 /UART2_RX))
    (pad 1 thru_hole rect (at -9 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 23 /UART2_TX))
    (pad 8 thru_hole circle (at 5 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 51 /OW))
    (pad 9 thru_hole circle (at 7 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 24 /VCOM))
    (pad 3 thru_hole circle (at -5 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 25 "/SCK(PA5)"))
    (pad 4 thru_hole circle (at -3 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 26 "/MISO(PA6)"))
    (pad 7 thru_hole circle (at 3 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 27 /WKUP-P0.12))
    (pad 6 thru_hole circle (at 1 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 28 /N_IO_1-P0.11))
    (pad 5 thru_hole circle (at -1 0 180) (size 1.05 1.05) (drill 0.8) (layers *.Cu F.SilkS B.Mask)
      (net 29 "/MOSI(PA7)"))
    (pad 1 smd rect (at -9 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /UART2_TX))
    (pad 2 smd rect (at -7 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /UART2_RX))
    (pad 3 smd rect (at -5 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "/SCK(PA5)"))
    (pad 4 smd rect (at -3 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "/MISO(PA6)"))
    (pad 5 smd rect (at -1 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "/MOSI(PA7)"))
    (pad 6 smd rect (at 1 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /N_IO_1-P0.11))
    (pad 7 smd rect (at 3 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /WKUP-P0.12))
    (pad 8 smd rect (at 5 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /OW))
    (pad 9 smd rect (at 7 -1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /VCOM))
    (pad 10 smd rect (at 9 1.6 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /VUSB))
    (pad 1 smd circle (at -9 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 23 /UART2_TX) (solder_mask_margin -0.05))
    (pad 2 smd circle (at -7 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 22 /UART2_RX) (solder_mask_margin -0.05))
    (pad 3 smd circle (at -5 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 25 "/SCK(PA5)") (solder_mask_margin -0.05))
    (pad 4 smd circle (at -3 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 26 "/MISO(PA6)") (solder_mask_margin -0.05))
    (pad 5 smd circle (at -1 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 29 "/MOSI(PA7)") (solder_mask_margin -0.05))
    (pad 6 smd circle (at 1 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 28 /N_IO_1-P0.11) (solder_mask_margin -0.05))
    (pad 7 smd circle (at 3 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 27 /WKUP-P0.12) (solder_mask_margin -0.05))
    (pad 8 smd circle (at 5 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 51 /OW) (solder_mask_margin -0.05))
    (pad 9 smd circle (at 7 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 24 /VCOM) (solder_mask_margin -0.05))
    (pad 10 smd circle (at 9 0 180) (size 1.05 1.05) (layers F.Cu F.Mask)
      (net 2 /VUSB) (solder_mask_margin -0.05))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.5595 79.375 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.5595 77.47 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.5595 75.565 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.595 73.66 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 177.165 83.185 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -1.3335 -2.54 180) (layer F.SilkS))
    (fp_text value TLV70233_SOT23-5 (at 2.3495 1.27 180) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /VUSB))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /VUSB))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DWM1004C:DWM1004C (layer B.Cu) (tedit 5E5EF418)
    (at 193.167 76.835 90)
    (attr smd)
    (fp_text reference U2 (at 1.2 -0.5 -90) (layer B.SilkS))
    (fp_text value DWM-1004c (at 0.1 -3.4 -90) (layer B.SilkS))
    (fp_text user "PCB EDGE" (at -0.1 4 -90) (layer B.SilkS))
    (pad 1 smd oval (at -8.2 2.7 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -8.2 1.45 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(U2-Pad2)"))
    (pad 3 smd oval (at -8.2 0.16 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 4 smd oval (at -8.2 -1.09 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 5 smd oval (at -8.2 -2.36 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 6 smd oval (at -8.2 -3.64 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U2-Pad6)"))
    (pad 7 smd oval (at -8.2 -4.91 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U2-Pad7)"))
    (pad 8 smd oval (at -8.2 -6.17 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U2-Pad8)"))
    (pad 9 smd oval (at -8.2 -7.45 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 /IRQ))
    (pad 10 smd oval (at -8.2 -8.73 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /TXLED))
    (pad 11 smd oval (at -8.2 -9.98 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /RXLED))
    (pad 12 smd oval (at -8.2 -11.26 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /SFDLED))
    (pad 13 smd oval (at -8.2 -12.53 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /RXOKLED))
    (pad 14 smd oval (at -8.2 -13.8 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd oval (at -5.96 -16.55) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U2-Pad15)"))
    (pad 16 smd oval (at -4.7 -16.54) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 17 smd oval (at -3.43 -16.54) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 /SWDIO))
    (pad 18 smd oval (at -2.15 -16.54) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /SWCLK))
    (pad 19 smd oval (at -0.88 -16.53) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U2-Pad19)"))
    (pad 20 smd oval (at 0.39 -16.53) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U2-Pad20)"))
    (pad 21 smd oval (at 1.65 -16.53) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U2-Pad21)"))
    (pad 22 smd oval (at 2.93 -16.52) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U2-Pad22)"))
    (pad 23 smd oval (at 4.2 -16.52) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U2-Pad23)"))
    (pad 24 smd oval (at 5.47 -16.52) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 25 smd oval (at 7.71 -13.77 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 26 smd oval (at 7.71 -12.5 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 /UART2_RX))
    (pad 37 smd oval (at 7.7 1.44 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U2-Pad37)"))
    (pad 28 smd oval (at 7.7 -9.99 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 /RESET_n))
    (pad 33 smd oval (at 7.7 -3.63 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 /LIS_SDA))
    (pad 31 smd oval (at 7.7 -6.18 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D5-Pad2)"))
    (pad 36 smd oval (at 7.7 0.19 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U2-Pad36)"))
    (pad 32 smd oval (at 7.7 -4.9 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 32 /LIS_INT2))
    (pad 29 smd oval (at 7.7 -8.7 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U2-Pad29)"))
    (pad 27 smd oval (at 7.7 -11.24 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 /UART2_TX))
    (pad 35 smd oval (at 7.7 -1.09 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U2-Pad35)"))
    (pad 34 smd oval (at 7.7 -2.37 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 /LIS_SCL))
    (pad 38 smd oval (at 7.7 2.72 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 30 smd oval (at 7.7 -7.45 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U2-Pad30)"))
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 177.165 71.755)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D5 (at 2.6035 0) (layer F.SilkS))
    (fp_text value STATUS (at 6.223 -0.0635) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.SilkS))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 172.847 79.375 270)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at -0.127 1.9685 180) (layer B.SilkS))
    (fp_text value LIS_SCL (at 1.397 0.0635 180) (layer B.SilkS))
    (fp_text user %R (at 0 1.45 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1 1) (layers B.Cu B.Mask)
      (net 30 /LIS_SCL))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 172.974 75.819 270)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0.127 2.032 180) (layer B.SilkS))
    (fp_text value LIS_SDA (at 1.524 0.254 180) (layer B.SilkS))
    (fp_text user %R (at 0 1.45 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1 1) (layers B.Cu B.Mask)
      (net 31 /LIS_SDA))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 172.9105 72.1995 270)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 1.9685 180) (layer B.SilkS))
    (fp_text value LIS_INT2 (at 1.27 0.0635 180) (layer B.SilkS))
    (fp_text user %R (at 0 1.45 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 270) (size 1 1) (layers B.Cu B.Mask)
      (net 32 /LIS_INT2))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 190.4365 70.2945)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP4 (at 0 1.5875) (layer F.SilkS))
    (fp_text value RESET_n (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 19 /RESET_n))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 195.8975 83.947)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.448) (layer F.SilkS))
    (fp_text value TX2 (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 23 /UART2_TX))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 192.405 83.947)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.448) (layer F.SilkS))
    (fp_text value RX2 (at 0 1.55) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 22 /UART2_RX))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.595 71.755 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.5895 -0.0635) (layer F.SilkS))
    (fp_text value R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OneWireMemory:DS28E05R&plus_T (layer F.Cu) (tedit 0)
    (at 194.691 72.4027)
    (fp_text reference U3 (at -1.651 -1.7907) (layer F.SilkS))
    (fp_text value DS28E05R+T (at -2.667 1.5113) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.950001 1.0287) (size 0.5588 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 51 /OW))
    (pad 2 smd rect (at 0.950001 1.0287) (size 0.5588 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP1-Pad1)"))
    (pad 3 smd rect (at 0 -1.0287) (size 0.5588 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 194.691 76.327 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value VCC_Select (at 0.762 -2.794) (layer F.SilkS))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 50 "Net-(JP1-Pad1)"))
  )
  (module BitcrazeGraphics:Up (layer F.Cu) (tedit 5E73A960)
    (at 198.12 76.962 270)
    (fp_text reference TP7 (at -2.2 -2.4) (layer F.SilkS))
    (fp_text value up_graphic (at -0.1 1.6 90) (layer F.Fab))
    (fp_text user Front (at 0 -6.4 90) (layer F.SilkS))
    (fp_text user Up (at 0 0.4 90) (layer F.SilkS))
  )
  (module Graphics:nyan (layer B.Cu) (tedit 0)
    (at 192.151 88.011)
    (fp_text reference TP8 (at 0 0) (layer B.SilkS) hide)
    (fp_text value nyan (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "Loco Deck rev 0.1" (at 178.054 90.17) (layer B.SilkS))
  (gr_text "Thomas Snyder 2020" (at 188.595 64.135) (layer B.SilkS))
  (gr_line (start 172.085 62.865) (end 198.755 62.865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.545 89.535) (end 169.545 65.405) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.755 91.44) (end 171.45 91.44) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 171.45 89.535) (end 169.545 89.535) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 172.085 65.405) (end 172.085 62.865) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 205.74 85.725) (end 198.755 91.44) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 205.74 68.58) (end 205.74 85.725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 198.755 62.865) (end 205.74 68.58) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 68.58) (xy 205.74 85.725) (xy 198.755 91.44) (xy 196.85 91.44) (xy 196.85 62.865)
        (xy 198.755 62.865)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 91.44) (xy 171.45 91.44) (xy 169.545 89.535) (xy 169.545 65.405) (xy 172.085 62.865)
        (xy 196.85 62.865)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 91.44) (xy 171.45 91.44) (xy 169.545 89.535) (xy 169.545 65.405) (xy 172.085 62.865)
        (xy 196.85 62.865)
      )
    )
  )
)
