<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.888" y2="0" width="0" layer="20"/>
<wire x1="25.888" y1="0" x2="25.888" y2="32.436" width="0" layer="20"/>
<wire x1="25.888" y1="32.436" x2="0" y2="32.436" width="0" layer="20"/>
<wire x1="0" y1="32.436" x2="0" y2="0" width="0" layer="20"/>
<text>Hong's Electronics TPM 2.0</text>
<text>TRUST
IN YOUR
HARDWARE</text>
<text>Hong's Electronics
Hardware (Security) Matters
</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X10_LOCK">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="INF-PG-TSSOP-28-16_M">
<packages>
<package name="INF-PG-TSSOP-28-16_M_1PRIMARY">
<description>Original name &lt;b&gt;INF-PG-TSSOP-28-16_M&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X10_LOCK" value=""/>
<element name="U$1" library="INF-PG-TSSOP-28-16_M" package="INF-PG-TSSOP-28-16_M_1PRIMARY" value="SLB9965"/>
<element name="R1" library="adafruit" package="R0805" value="1k"/>
<element name="C1" library="adafruit" package="C0805K" value="470n"/>
<element name="C2" library="adafruit" package="C0805K" value="470n"/>
<element name="C3" library="adafruit" package="C0805K" value="470n"/>
<element name="C4" library="adafruit" package="C0805K" value="470n"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="21"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="22"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="16"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="17"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="24"/>
<contactref element="U$1" pad="19"/>
<contactref element="J1" pad="10"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="25"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="11"/>
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="11"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="18"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="26"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="20"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="23"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="27"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="13"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
