<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="48.26" x2="0" y2="2.54" width="0.254" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="24.13" y2="0" width="0.254" layer="20"/>
<wire x1="26.67" y1="2.54" x2="26.67" y2="48.26" width="0.254" layer="20"/>
<wire x1="24.13" y1="50.8" x2="2.54" y2="50.8" width="0.254" layer="20"/>
<text>KD0GLS 2017</text>
<wire x1="24.13" y1="0" x2="26.67" y2="2.54" width="0.254" layer="20" curve="90"/>
<wire x1="26.67" y1="48.26" x2="24.13" y2="50.8" width="0.254" layer="20" curve="90"/>
<wire x1="2.54" y1="50.8" x2="0" y2="48.26" width="0.254" layer="20" curve="90"/>
<text>16V8  36/55</text>
<text>18V10 36/5F</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="SOCKET_PLCC20">
</package>
<package name="CONN_BREAKAWAY_1X10_100_SMT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PLCC1" library="kd0gls" package="SOCKET_PLCC20" value="SOCKET_PLCC20"/>
<element name="U$1" library="kd0gls" package="CONN_BREAKAWAY_1X10_100_SMT" value="CONN_BREAKAWAY_1X10_100_SMT"/>
<element name="U$2" library="kd0gls" package="CONN_BREAKAWAY_1X10_100_SMT" value="CONN_BREAKAWAY_1X10_100_SMT"/>
</elements>
<signals>
<signal name="1">
<contactref element="PLCC1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="2">
<contactref element="PLCC1" pad="2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="3">
<contactref element="PLCC1" pad="3"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="4">
<contactref element="PLCC1" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="5">
<contactref element="PLCC1" pad="5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="6">
<contactref element="PLCC1" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="7">
<contactref element="PLCC1" pad="7"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="8">
<contactref element="PLCC1" pad="8"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="9">
<contactref element="PLCC1" pad="9"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="PLCC1" pad="10"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="11">
<contactref element="PLCC1" pad="11"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="12">
<contactref element="PLCC1" pad="12"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="13">
<contactref element="PLCC1" pad="13"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="14">
<contactref element="PLCC1" pad="14"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="15">
<contactref element="PLCC1" pad="15"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="16">
<contactref element="PLCC1" pad="16"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="17">
<contactref element="PLCC1" pad="17"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="18">
<contactref element="PLCC1" pad="18"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="19">
<contactref element="PLCC1" pad="19"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="VCC">
<contactref element="PLCC1" pad="20"/>
<contactref element="U$2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
