<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="79.99" y2="0" width="0" layer="20"/>
<wire x1="79.99" y1="0" x2="79.99" y2="36.246" width="0" layer="20"/>
<wire x1="79.99" y1="36.246" x2="0" y2="36.246" width="0" layer="20"/>
<wire x1="0" y1="36.246" x2="0" y2="0" width="0" layer="20"/>
<text>Board by NI2O 04/2011</text>
<text>Board by NI2O 04/2011 for Splitrock ARA</text>
<text>WWVB Receiver</text>
<text>Original by N0QBH. Modifications by NI2O</text>
<text>Contrast</text>
<text>Shackurate Clock</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="RESONATOR-PTH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="SWITCH-SPDT">
</package>
<package name="1X06">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="microchip">
<packages>
<package name="SO-18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="display-lcd">
<packages>
<package name="TUXGR_16X2_R2">
<description>&lt;b&gt;Tuxgraphics LCD display 16x2 characters&lt;/b&gt; reflective, without background light&lt;p&gt;
Source: tuxgr_12x2_r2.pdf</description>
</package>
</packages>
</library>
<library name="pot">
<packages>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="microchip" package="SO-18W" value="PIC16F628SO">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC16F628-20I/SO"/>
<attribute name="OC_FARNELL" value="9760415"/>
<attribute name="OC_NEWARK" value="23C4986"/>
</element>
<element name="U1" library="SparkFun" package="SSOP28DB" value="FT232RL-BASICSSOP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun" package="RESONATOR-PTH" value="4MHz"/>
<element name="X1" library="SparkFun" package="USB-MINIB" value="USBSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="SWITCH-SPDT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DIS1" library="display-lcd" package="TUXGR_16X2_R2" value="TUXGR_16X2_R2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R2" library="pot" package="CA6V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M1206" value="1K"/>
<element name="PICKIT2" library="SparkFun" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CMMR-6" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="M1206" value="4k7"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="15"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="16"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="Y1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="X1" pad="GND"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="25"/>
<contactref element="DIS1" pad="1"/>
<contactref element="R2" pad="A"/>
<contactref element="DIS1" pad="5"/>
<contactref element="DIS1" pad="15"/>
<contactref element="CMMR-6" pad="1"/>
<contactref element="PICKIT2" pad="3"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="X1" pad="VBUS"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="4"/>
<contactref element="IC1" pad="14"/>
<contactref element="R1" pad="1"/>
<contactref element="DIS1" pad="2"/>
<contactref element="R2" pad="E"/>
<contactref element="R3" pad="1"/>
<contactref element="CMMR-6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="PICKIT2" pad="2"/>
</signal>
<signal name="USBDM">
<contactref element="X1" pad="D-"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="USBDP">
<contactref element="X1" pad="D+"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="DIS1" pad="3"/>
<contactref element="R2" pad="S"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="1"/>
<contactref element="DIS1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="9"/>
<contactref element="DIS1" pad="4"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="5"/>
<contactref element="IC1" pad="7"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="10"/>
<contactref element="DIS1" pad="11"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="11"/>
<contactref element="DIS1" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="12"/>
<contactref element="DIS1" pad="13"/>
<contactref element="PICKIT2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
<contactref element="DIS1" pad="16"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="18"/>
<contactref element="CMMR-6" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="17"/>
<contactref element="CMMR-6" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="4"/>
<contactref element="PICKIT2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="PICKIT2" pad="4"/>
<contactref element="IC1" pad="13"/>
<contactref element="DIS1" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
