(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 19)
    (no_connects 0)
    (area 149.276999 86.792999 167.207001 110.819001)
    (thickness 1.6)
    (drawings 9)
    (tracks 57)
    (zones 0)
    (modules 9)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 5A)
  (net 3 A)
  (net 4 B)
  (net 5 5B)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.15)
    (trace_width 1.27)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.15)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5A)
    (add_net 5B)
    (add_net A)
    (add_net B)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
  )
  (module RJ45:EJ45_RJHSE-5080 (layer F.Cu) (tedit 58771648)
    (at 164.592 91.948 180)
    (fp_text reference J1 (at 6.51002 3.79476 180) (layer F.SilkS))
    (fp_text value RJ45 (at 6.62178 -8.3312 180) (layer F.Fab))
    (fp_text user RJ45 (at 6.35 1.905 180) (layer F.SilkS))
    (pad 8 thru_hole circle (at 2.794 -4.318 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.81 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 5A))
    (pad 6 thru_hole circle (at 4.826 -4.318 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 A))
    (pad 4 thru_hole circle (at 6.858 -4.318 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 B))
    (pad 2 thru_hole circle (at 8.89 -4.318 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 5B))
    (pad 5 thru_hole circle (at 5.842 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 B))
    (pad 3 thru_hole circle (at 7.874 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 A))
    (pad 1 thru_hole circle (at 9.906 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 0 180) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 180) (size 3.4 3.4) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5878A8C8)
    (at 160.02 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference B (at -2.667 -2.032 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 A))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 5A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5878A8C3)
    (at 157.48 104.14)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference A (at 2.54 -2.032 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 5B))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58789B75)
    (at 163.83 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS))
    (fp_text value C (at 0 1.778 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 5A))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58789BEF)
    (at 153.162 107.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.254 0 90) (layer F.SilkS))
    (fp_text value C (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 5B))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58789B5F)
    (at 165.735 107.95 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 1.524 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58789C06)
    (at 150.876 107.95 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RJ45:LED_0805_w_silk (layer F.Cu) (tedit 5878A78F)
    (at 163.83 104.14 180)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D1 (at 0 1.6 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.05 0 180) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 A))
  )
  (module RJ45:LED_0805_w_silk (layer F.Cu) (tedit 5878A78F)
    (at 153.162 104.14)
    (descr "Diode SMD in 0805 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at 0 1.6) (layer F.SilkS) hide)
    (fp_text value LED (at 0 -1.6) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 0.8 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 B))
  )
  (gr_text "RJ45 ->\nAll Signals" (at 158.496 99.822) (layer B.SilkS))
  (gr_text FRC2168 (at 158.242 88.392) (layer B.SilkS))
  (gr_text BLK (at 155.067 109.093 90) (layer F.SilkS))
  (gr_text WHT (at 155.321 103.886 90) (layer F.SilkS))
  (gr_line (start 149.352 86.868) (end 167.132 86.868) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.352 110.744) (end 149.352 86.868) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 110.744) (end 149.352 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.132 110.744) (end 149.86 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.132 86.868) (end 167.132 110.744) (angle 90) (layer Edge.Cuts) (width 0.15))
)
