(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3V3")
  (net 2 "GND")
  (net 3 "/SCL")
  (net 4 "/SDA")
  (net 5 "/RST")
  (net 6 "/IRQ")
  (net 7 "/FOUT")
  (net 8 "Net-(U1-Pad9)")
  (net 9 "Net-(U1-Pad10)")
  (net 10 "Net-(BT1-Pad1)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.795 97.155 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2.4348 0.000905 90) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 92.075 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 101.6 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/IRQ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.509284 92.710559)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(BT1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:10mm Crewmate" (layer "F.Cu")
    (tedit 0)
    (at 139.7 106.172)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.748757 94.245888)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 2.47703 -0.008035) (layer "F.SilkS"))
    (fp_text value ".1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 95.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.4125 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Generic:RX8130CE" (layer "F.Cu")
    (tedit 0)
    (at 132.715 95.885 -90)
    (descr "RX8130CE-2")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "RX8130CE")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/rx8130ce/epson-electronics-america")
    (property "Datasheet_1" "https://www.mouser.in/Search/DownloadDatasheet?url=https%3A%2F%2Fwww.mouser.in%2Fdatasheet%2F2%2F137%2FRX8130CE_en-1825324.pdf")
    (property "Footprint_1" "RX8130CE")
    (property "Height" "1")
    (property "Manufacturer_Name" "Epson Timing")
    (property "Manufacturer_Part_Number" "RX8130CE")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Reference_1" "IC")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "RX8130CE")
    (attr smd)
    (fp_text reference "U1" (at 2.837716 -0.099436 180) (layer "F.SilkS"))
    (fp_text value "RX8130CE" (at 0 0.275 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0.275 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.55 1 270) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VIO") (pintype "passive"))
    (pad "2" smd rect locked (at -0.7 1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/SCL") (pinfunction "SCL") (pintype "passive"))
    (pad "3" smd rect locked (at 0 1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/SDA") (pinfunction "SDA") (pintype "passive"))
    (pad "4" smd rect locked (at 0.7 1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/FOUT") (pinfunction "FOUT") (pintype "passive"))
    (pad "5" smd rect locked (at 1.55 1 270) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/RST") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" smd rect locked (at 1.55 -1 270) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/IRQ") (pinfunction "~{IRQ}") (pintype "passive"))
    (pad "7" smd rect locked (at 0.7 -1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "8" smd rect locked (at 0 -1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3V3") (pinfunction "VDD") (pintype "passive"))
    (pad "9" smd rect locked (at -0.7 -1 270) (size 0.4 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U1-Pad9)") (pinfunction "VOUT") (pintype "passive"))
    (pad "10" smd rect locked (at -1.55 -1 270) (size 0.7 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U1-Pad10)") (pinfunction "VBAT") (pintype "passive"))
    (model "RX8130CE.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 98.425 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.00489 1.49288 90) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/RST") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.89 97.155 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 2.585494 -0.022228 90) (layer "F.SilkS"))
    (fp_text value ".1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.4 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A433)
    (at 121.92 88.265)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Conn_01x07_Male" (at -4.064 7.239 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/RST") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/IRQ") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/FOUT") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Generic:BAT_BAT-HLD-003-SMT" (layer "B.Cu")
    (tedit 6442D358)
    (at 135.255 95.885 -90)
    (property "Sheetfile" "RX8130 Breakout.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "BT1" (at -10.055 12.389 90) (layer "B.SilkS"))
    (fp_text value "CR2032" (at 2.391 -11.389 90) (layer "B.Fab"))
    (pad "1" smd circle locked (at 0 0 270) (size 17.9 17.9) (layers "B.Cu" "B.Mask")
      (net 10 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect locked (at -12.9 0 270) (size 5.7 6.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "2" smd rect locked (at 12.9 0 270) (size 5.7 6.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
  )
  (gr_arc (start 142.875 79.375) (mid 144.671051 80.118949) (end 145.415 81.915) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 121.92 113.03) (mid 120.123949 112.286051) (end 119.38 110.49) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 119.38 81.915) (mid 120.123949 80.118949) (end 121.92 79.375) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 121.92 113.03) (end 142.875 113.03) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 142.875 79.375) (end 121.92 79.375) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 145.415 110.49) (mid 144.671051 112.286051) (end 142.875 113.03) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 145.415 110.49) (end 145.415 81.915) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 119.38 81.915) (end 119.38 110.49) (layer "Edge.Cuts") (width 0.2))
  (gr_text "RX8130 Breakout\nRev 1.0 \nArsenio Menendez" (at 134.62 83.82) (layer "F.Cu"))
  (gr_text "SDA" (at 125.476 96.012) (layer "F.SilkS"))
  (gr_text "RST" (at 125.476 98.552) (layer "F.SilkS"))
  (gr_text "IRQ" (at 125.476 101.092) (layer "F.SilkS"))
  (gr_text "FOUT" (at 125.476 103.632) (layer "F.SilkS"))
  (gr_text "GND" (at 125.476 90.932) (layer "F.SilkS"))
  (gr_text "3V3\n" (at 125.476 88.392) (layer "F.SilkS"))
  (gr_text "SCL" (at 125.476 93.472) (layer "F.SilkS"))
  (gr_text "RX8130 Breakout\nRev 1.0 \nArsenio Menendez" (at 134.62 83.82) (layer "F.Mask"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.05 114.3)
        (xy 118.745 114.3)
        (xy 118.745 78.74)
        (xy 146.05 78.74)
      )
    )
  )
)
