(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 134.950005 66.2834)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/SIG1")
  (net 2 "/GND")
  (footprint "Library:CONN_XF3M1-0515-1B_OMR" (layer "F.Cu")
    (at 135.549994 72.5288 -90)
    (tags "XF3M1-0515-1B ")
    (property "Sheetfile" "CoaxBreakoutSymmetric.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "XF3M(1)-0515-1B")
    (attr smd)
    (fp_text reference "J1" (at -2 3.5 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "XF3M10515-1B" (at -2 1.599989 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at -4.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -3.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG1") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at -2 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "3") (pintype "unspecified"))
    (pad "4" smd rect (at -0.999999 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG1") (pinfunction "4") (pintype "unspecified"))
    (pad "5" smd rect (at 0.000001 0 270) (size 0.6 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "5") (pintype "unspecified"))
    (pad "6" smd rect (at -6.4 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "7" smd rect (at 2.4 3.250001 270) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
  )
  (footprint "Library:CONN1_CONUFL_TEC" (layer "F.Cu")
    (at 141.200005 73.7834 -90)
    (tags "CONUFL001-SMD-T ")
    (property "Sheetfile" "CoaxBreakoutSymmetric.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "CONUFL001-SMD-T")
    (attr smd)
    (fp_text reference "J4" (at 0 1.544599 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "CONUFL001-SMD-T" (at 0 1.544599 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 1.544599 270) (size 1.0414 1.0922) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG1") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -1.475001 0 270) (size 1.0414 2.2606) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 1.475001 0 270) (size 1.0414 2.2606) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "3") (pintype "unspecified"))
  )
  (footprint "Library:CONN1_CONUFL_TEC" (layer "F.Cu")
    (at 141.200005 67.258401 -90)
    (tags "CONUFL001-SMD-T ")
    (property "Sheetfile" "CoaxBreakoutSymmetric.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "CONUFL001-SMD-T")
    (attr smd)
    (fp_text reference "J2" (at 0 1.544599 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "CONUFL001-SMD-T" (at 0 1.544599 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd rect (at 0 1.544599 270) (size 1.0414 1.0922) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/SIG1") (pinfunction "1") (pintype "unspecified"))
    (pad "2" smd rect (at -1.475001 0 270) (size 1.0414 2.2606) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" smd rect (at 1.475001 0 270) (size 1.0414 2.2606) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/GND") (pinfunction "3") (pintype "unspecified"))
  )
  (gr_poly
    (pts
      (xy 129.850005 64.7334)
      (xy 143.850005 64.7334)
      (xy 143.850005 76.4834)
      (xy 129.850005 76.4834)
    )
    (fill none) (layer "Edge.Cuts"))
  (gr_text "XF3M(1)\n0515-1B" (at 132.200005 70.2834 -90) (layer "F.SilkS"))
  (zone (net 2) (net_name "/GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.25))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 129.850005 53.4834)
        (xy 143.850005 53.4834)
        (xy 143.850005 76.4834)
        (xy 129.850005 76.4834)
      )
    )
  )
)
