(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 20)
    (no_connects 0)
    (area 0 0 0 0)
    (thickness 1.6)
    (drawings 25)
    (tracks 102)
    (zones 0)
    (modules 3)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "Net-(J1-Pad13)")
  (net 14 "Net-(J1-Pad14)")
  (net 15 "Net-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "Net-(J1-Pad19)")
  (net 20 "Net-(J1-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module AMPHENOL_UE75-A20-6000T (layer F.Cu) (tedit 5CA813AF)
    (at 149.86 109.22)
    (attr smd)
    (fp_text reference J1 (at -1.90737 -6.99366) (layer F.SilkS))
    (fp_text value UE75-A20-6000T (at -1.27115 6.99135) (layer F.SilkS) hide)
    (pad 1 smd rect (at -3.2 -3.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -3.2 -2.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -3.2 -1.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -3.2 -1) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -3.2 -0.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -3.2 0.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -3.2 1.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -3.2 2.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -3.2 3) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at -3.2 3.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 5 3.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 5 2.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 13 smd rect (at 5 1.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 5 1) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at 5 0.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at 5 -0.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at 5 -1.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 18 smd rect (at 5 -2.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 19 smd rect (at 5 -3) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (pad 20 smd rect (at 5 -3.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad20)"))
    (pad Hole np_thru_hole circle (at 0.9 -4.8) (size 1.55 1.55) (drill 1.55) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at 0.9 4.8) (size 1.55 1.55) (drill 1.55) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5CA813B3)
    (at 129.54 121.92 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 25.19 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 5CA813B6)
    (at 152.4 96.52 270)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x10_Male (at 0 25.19 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 11.43 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad13)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad14)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad15)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad17)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad19)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad20)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 126.365 93.345) (end 164.465 93.345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.365 125.095) (end 126.365 93.345) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.465 125.095) (end 126.365 125.095) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.465 93.345) (end 164.465 125.095) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "SFP CONNECTOR\nBREAKOUT BRD\nK. FINNEGAN" (at 137.16 109.22) (layer F.SilkS))
  (gr_text "11\nR_GND" (at 152.4 98.425 90) (layer F.SilkS))
  (gr_text "12\nRD-" (at 149.86 98.425 90) (layer F.SilkS))
  (gr_text "13\nRD+" (at 147.32 98.425 90) (layer F.SilkS))
  (gr_text "14\nR_GND" (at 144.78 98.425 90) (layer F.SilkS))
  (gr_text "15\nR_VCC" (at 142.24 98.425 90) (layer F.SilkS))
  (gr_text "16\nT_VCC" (at 139.7 98.425 90) (layer F.SilkS))
  (gr_text "17\nT_GND" (at 137.16 98.425 90) (layer F.SilkS))
  (gr_text "18\nTD+" (at 134.62 98.425 90) (layer F.SilkS))
  (gr_text "19\nTD-" (at 132.08 98.425 90) (layer F.SilkS))
  (gr_text "20\nT_GND" (at 129.54 98.425 90) (layer F.SilkS))
  (gr_text "10\nR_GND" (at 152.4 120.015 90) (layer F.SilkS))
  (gr_text "9\nRATE_S1" (at 149.86 120.015 90) (layer F.SilkS))
  (gr_text "8\nR_LOS" (at 147.32 120.015 90) (layer F.SilkS))
  (gr_text "7\nRATE_S0" (at 144.78 120.015 90) (layer F.SilkS))
  (gr_text "6\nMOD_ABS" (at 142.24 120.015 90) (layer F.SilkS))
  (gr_text "5\nMOD_SCL" (at 139.7 120.015 90) (layer F.SilkS))
  (gr_text "4\nMOD_SDA" (at 137.16 120.015 90) (layer F.SilkS))
  (gr_text "3\nT_DISAB" (at 134.62 120.015 90) (layer F.SilkS))
  (gr_text "2\nT_FAULT" (at 132.08 120.015 90) (layer F.SilkS))
  (gr_text "1\nT_GND" (at 129.54 120.015 90) (layer F.SilkS))
)
