(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu14.04.1)
  (general
    (links 137)
    (no_connects 0)
    (area 64.924999 86.200001 365.075001 193.200001)
    (thickness 1.6)
    (drawings 23)
    (tracks 1174)
    (zones 0)
    (modules 48)
    (nets 47)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 12.8 12.8)
    (pad_drill 6.4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "/home/clive/tombsserver/DOCUMENTS/KiCAD shematics/B6526_meter_panel/"))
  )
  (net 0 "")
  (net 1 /P1-11)
  (net 2 /P1-3)
  (net 3 /P1-8)
  (net 4 /P1-7)
  (net 5 /P1-9)
  (net 6 /P1-10)
  (net 7 /P1-1)
  (net 8 /P1-2)
  (net 9 /P1-4)
  (net 10 /P1-5)
  (net 11 /P1-6)
  (net 12 /P1-12)
  (net 13 /P2-1)
  (net 14 /P2-13)
  (net 15 /M3+)
  (net 16 GNDPWR)
  (net 17 /P2-4)
  (net 18 /P2-5)
  (net 19 /P2-6)
  (net 20 /P2-7)
  (net 21 /P2-8)
  (net 22 /M3-)
  (net 23 /P2-11)
  (net 24 /P2-12)
  (net 25 /M2+)
  (net 26 /M2-)
  (net 27 /-12v)
  (net 28 /P2-3)
  (net 29 /P2-10)
  (net 30 /Spare3)
  (net 31 /Spare4)
  (net 32 /Spare5)
  (net 33 /LOCPWR)
  (net 34 /Spare1)
  (net 35 /Spare2)
  (net 36 "Net-(F1-Pad2)")
  (net 37 /MONPWR)
  (net 38 "Net-(PH-1-Pad1)")
  (net 39 "Net-(PH-1-Pad3)")
  (net 40 "Net-(PH-1-Pad7)")
  (net 41 "Net-(PH-1-Pad9)")
  (net 42 "Net-(PH-1-Pad25)")
  (net 43 "Net-(PF-1-Pad25)")
  (net 44 "Net-(PF-1-Pad26)")
  (net 45 "Net-(PF-1-Pad15)")
  (net 46 "Net-(PF-1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Spare1)
    (add_net /Spare2)
    (add_net /Spare3)
    (add_net /Spare4)
    (add_net /Spare5)
    (add_net "Net-(PF-1-Pad15)")
    (add_net "Net-(PF-1-Pad16)")
    (add_net "Net-(PF-1-Pad25)")
    (add_net "Net-(PF-1-Pad26)")
    (add_net "Net-(PH-1-Pad1)")
    (add_net "Net-(PH-1-Pad25)")
    (add_net "Net-(PH-1-Pad3)")
    (add_net "Net-(PH-1-Pad7)")
    (add_net "Net-(PH-1-Pad9)")
  )
  (net_class POWER ""
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.762)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /-12v)
    (add_net /LOCPWR)
    (add_net /MONPWR)
    (add_net /P2-3)
    (add_net GNDPWR)
    (add_net "Net-(F1-Pad2)")
  )
  (net_class SIGNAL ""
    (clearance 0.254)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /M2+)
    (add_net /M2-)
    (add_net /M3+)
    (add_net /M3-)
    (add_net /P1-1)
    (add_net /P1-10)
    (add_net /P1-11)
    (add_net /P1-12)
    (add_net /P1-2)
    (add_net /P1-3)
    (add_net /P1-4)
    (add_net /P1-5)
    (add_net /P1-6)
    (add_net /P1-7)
    (add_net /P1-8)
    (add_net /P1-9)
    (add_net /P2-1)
    (add_net /P2-10)
    (add_net /P2-11)
    (add_net /P2-12)
    (add_net /P2-13)
    (add_net /P2-4)
    (add_net /P2-5)
    (add_net /P2-6)
    (add_net /P2-7)
    (add_net /P2-8)
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-12A1_2x06x4.20mm_Angled (layer F.Cu) (tedit 592EE54F)
    (at 110 110)
    (descr "Molex Mini-Fit JR, PN:5569-12A1, dual row, side entry type, through hole, with screw mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P1 (at 10.5 8.5) (layer F.SilkS))
    (fp_text value CONN_6X2inLine (at 10.5 10) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 7 /P1-1))
    (pad 2 thru_hole circle (at 4.2 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 8 /P1-2))
    (pad 3 thru_hole circle (at 8.4 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 4 thru_hole circle (at 12.6 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 9 /P1-4))
    (pad 5 thru_hole circle (at 16.8 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 10 /P1-5))
    (pad 6 thru_hole circle (at 21 0) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 11 /P1-6))
    (pad 7 thru_hole circle (at 0 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 4 /P1-7))
    (pad 8 thru_hole circle (at 4.2 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /P1-8))
    (pad 9 thru_hole circle (at 8.4 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 5 /P1-9))
    (pad 10 thru_hole circle (at 12.6 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 6 /P1-10))
    (pad 11 thru_hole circle (at 16.8 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 1 /P1-11))
    (pad 12 thru_hole circle (at 21 5.5) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 12 /P1-12))
    (pad "" np_thru_hole circle (at -4.5 -4.2) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 25.5 -4.2) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-12A1_2x06x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_MiniFit-JR-5569-14A1_2x07x4.20mm_Angled (layer F.Cu) (tedit 592EE540)
    (at 80 135 90)
    (descr "Molex Mini-Fit JR, PN:5569-14A1, dual row, side entry type, through hole, with screw mount")
    (tags "connector molex mini-fit 5569")
    (fp_text reference P2 (at 12.6 8.5 90) (layer F.SilkS))
    (fp_text value CONN_7X2In_Line (at 12.6 10 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 13 /P2-1))
    (pad 2 thru_hole circle (at 4.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 16 GNDPWR))
    (pad 3 thru_hole circle (at 8.4 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 28 /P2-3))
    (pad 4 thru_hole circle (at 12.6 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 17 /P2-4))
    (pad 5 thru_hole circle (at 16.8 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 18 /P2-5))
    (pad 6 thru_hole circle (at 21 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 19 /P2-6))
    (pad 7 thru_hole circle (at 25.2 0 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 20 /P2-7))
    (pad 8 thru_hole circle (at 0 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 21 /P2-8))
    (pad 9 thru_hole circle (at 4.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 29 /P2-10))
    (pad 10 thru_hole circle (at 8.4 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 29 /P2-10))
    (pad 11 thru_hole circle (at 12.6 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 23 /P2-11))
    (pad 12 thru_hole circle (at 16.8 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 24 /P2-12))
    (pad 13 thru_hole circle (at 21 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask)
      (net 14 /P2-13))
    (pad 14 thru_hole circle (at 25.2 5.5 90) (size 3 3) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.5 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 29.7 -4.2 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu))
    (model Connectors_Molex.3dshapes/Molex_MiniFit-JR-5569-14A1_2x07x4.20mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Multicomp:Multicomp_MC9A12-3434_2x17x2.54mm_Straight (layer F.Cu) (tedit 56C61E6B)
    (at 195 170)
    (descr http://www.farnell.com/datasheets/1520732.pdf)
    (tags "connector multicomp MC9A MC9A12")
    (fp_text reference SV1 (at -3 -7) (layer F.SilkS))
    (fp_text value ML34 (at 20.32 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P1-1))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /P1-7))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /P1-2))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /P1-8))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /P1-12))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /P1-4))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /P2-1))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /P1-5))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /P1-6))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P2-13))
    (pad 12 thru_hole circle (at 12.7 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /P1-11))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /P2-7))
    (pad 14 thru_hole circle (at 15.24 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /P2-8))
    (pad 15 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /P2-10))
    (pad 16 thru_hole circle (at 17.78 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /P2-10))
    (pad 17 thru_hole circle (at 20.32 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /P2-12))
    (pad 18 thru_hole circle (at 20.32 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /P2-11))
    (pad 19 thru_hole circle (at 22.86 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GNDPWR))
    (pad 20 thru_hole circle (at 22.86 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /MONPWR))
    (pad 21 thru_hole circle (at 25.4 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /P2-4))
    (pad 22 thru_hole circle (at 25.4 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /P2-5))
    (pad 23 thru_hole circle (at 27.94 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /P2-6))
    (pad 24 thru_hole circle (at 27.94 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /M3+))
    (pad 25 thru_hole circle (at 30.48 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /M3-))
    (pad 26 thru_hole circle (at 30.48 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /M2+))
    (pad 27 thru_hole circle (at 33.02 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /M2-))
    (pad 28 thru_hole circle (at 33.02 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1-10))
    (pad 29 thru_hole circle (at 35.56 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P1-9))
    (pad 30 thru_hole circle (at 35.56 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /Spare1))
    (pad 31 thru_hole circle (at 38.1 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /Spare2))
    (pad 32 thru_hole circle (at 38.1 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /Spare3))
    (pad 33 thru_hole circle (at 40.64 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /Spare4))
    (pad 34 thru_hole circle (at 40.64 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /Spare5))
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 54130BC5)
    (at 350 140)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference R1 (at -1.27 -10.16) (layer F.SilkS))
    (fp_text value 3266P-1-502 (at 0 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 "Net-(PH-1-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 38 "Net-(PH-1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 /P2-7))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 54130BC5)
    (at 320 140)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference R2 (at -1.27 -10.16) (layer F.SilkS))
    (fp_text value 3266P-1-502 (at 0 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(PH-1-Pad3)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "Net-(PH-1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 /P2-8))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 54130BC5)
    (at 290 140)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference R3 (at -1.27 -10.16) (layer F.SilkS))
    (fp_text value 3266P-1-502 (at 0 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 "Net-(PH-1-Pad7)"))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 "Net-(PH-1-Pad7)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 /P2-11))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 54130BC5)
    (at 260 140)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference R4 (at -1.27 -10.16) (layer F.SilkS))
    (fp_text value 3266P-1-102 (at 0 5.08) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /P2-12))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /P2-12))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 "Net-(PH-1-Pad9)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 275 155 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 50 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(PH-1-Pad9)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 265 155 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 50 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(PH-1-Pad7)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-W (layer F.Cu) (tedit 592EE523)
    (at 100 165 270)
    (descr "Module CMS SOJ 16 pins tres large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -9.044 -0.33 360) (layer F.SilkS))
    (fp_text value LTC1151CSW (at -7.393 -0.076 360) (layer F.Fab))
    (pad 1 smd rect (at -4.445 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.175 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.905 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 /M2-))
    (pad 4 smd rect (at -0.635 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 /M2-))
    (pad 5 smd rect (at 0.635 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(PF-1-Pad26)"))
    (pad 6 smd rect (at 1.905 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 /-12v))
    (pad 7 smd rect (at 3.175 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.445 5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.445 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 3.175 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 1.905 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(PF-1-Pad25)"))
    (pad 12 smd rect (at 0.635 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 /M2+))
    (pad 13 smd rect (at -0.635 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 25 /M2+))
    (pad 14 smd rect (at -1.905 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 33 /LOCPWR))
    (pad 15 smd rect (at -3.175 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -4.445 -5.08 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SO-16-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-W (layer F.Cu) (tedit 592EE50B)
    (at 330 165 90)
    (descr "Module CMS SOJ 16 pins tres large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 8.917 0.2 180) (layer F.SilkS))
    (fp_text value LTC1151CSW (at 7.139 0.2 180) (layer F.Fab))
    (pad 1 smd rect (at -4.445 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.175 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.905 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 /M3-))
    (pad 4 smd rect (at -0.635 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 /M3-))
    (pad 5 smd rect (at 0.635 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (pad 6 smd rect (at 1.905 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 /-12v))
    (pad 7 smd rect (at 3.175 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.445 5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 4.445 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 3.175 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 1.905 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(PH-1-Pad25)"))
    (pad 12 smd rect (at 0.635 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 /M3+))
    (pad 13 smd rect (at -0.635 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 /M3+))
    (pad 14 smd rect (at -1.905 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 33 /LOCPWR))
    (pad 15 smd rect (at -3.175 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -4.445 -5.08 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SO-16-W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.6 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 275 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 62 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(PH-1-Pad9)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 255 155 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 62 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(PH-1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 220 135 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 62 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(PH-1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 210 135 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 62 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(PH-1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 255 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /P1-11))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /P1-3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 265 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /P1-12))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /P1-3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 155 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /P2-13))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /P1-3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 165 155 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /P1-6))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /P1-3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 165 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /P1-5))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /P1-3))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 155 155 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /P1-7))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /P1-1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 175 155 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /P1-8))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /P1-2))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 175 170 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R18 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /P1-4))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /P2-1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 102.235 162.2425 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 GNDPWR))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 /LOCPWR))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 98.8695 167.8305 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 GNDPWR))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 27 /-12v))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x4.5 (layer F.Cu) (tedit 57FA4558)
    (at 180.6575 123.8885)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x4.5")
    (attr smd)
    (fp_text reference C3 (at 0 4.5593) (layer F.SilkS))
    (fp_text value 10u (at 0 -4.5593) (layer F.Fab))
    (fp_text user + (at -1.7272 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.2799 2.9591) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /LOCPWR))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GNDPWR))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x4.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 177.4825 144.018)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1u (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /-12v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 327.8505 162.306 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 GNDPWR))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 33 /LOCPWR))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 331.7875 167.386 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 27 /-12v))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 GNDPWR))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 592EE5C4)
    (at 270.383 163.957)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P13 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 34 /Spare1))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 592EE5CD)
    (at 281.178 158.877)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P14 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 35 /Spare2))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 592EE5D1)
    (at 292.481 158.877)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P15 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 30 /Spare3))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 592EE5C9)
    (at 281.178 167.767)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P16 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 31 /Spare4))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 592EE5D5)
    (at 292.735 167.767)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P17 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 32 /Spare5))
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201 (layer F.Cu) (tedit 56B65074)
    (at 114.7445 128.905)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F1 (at 11.25 -6) (layer F.SilkS))
    (fp_text value "FUSE 315mA" (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 /P2-3))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 36 "Net-(F1-Pad2)"))
    (pad "" np_thru_hole circle (at 11.25 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_Schurter_0031_8201 (layer F.Cu) (tedit 5A856640)
    (at 114.7445 143.1925)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F2 (at 11.25 -6) (layer F.SilkS))
    (fp_text value "FUSE 1.5A" (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 28 /P2-3))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 /MONPWR))
    (pad "" np_thru_hole circle (at 11.25 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Converters_DCDC_ACDC:DCDC-Conv_Recom_RO-4pin (layer F.Cu) (tedit 5975DBCD)
    (at 177.6095 135.001)
    (descr DCDC-Conv_Recom_RO-4pin)
    (tags "Recom 4pin")
    (fp_text reference PS1 (at -9.7155 -3.81) (layer F.SilkS))
    (fp_text value CONVERTERcdt (at 0 -3.85) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at -7.62 0) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 16 GNDPWR))
    (pad 2 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 33 /LOCPWR))
    (pad 3 thru_hole oval (at -5.08 0) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 27 /-12v))
    (pad 1 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 16 GNDPWR))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 330.708 152.7175)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R19 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 100K (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(PH-1-Pad25)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /P2-10))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 99.949 156.464)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R20 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 100k (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(PF-1-Pad25)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(PF-1-Pad26)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_6.4mm_M6_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 81.28 165.1)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (fp_text reference P3 (at 0 -7.4) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 7.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 12.8 12.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 25 /M2+))
  )
  (module Mounting_Holes:MountingHole_6.4mm_M6_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 119.38 165.1)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (fp_text reference P4 (at 0 -7.4) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 7.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 12.8 12.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 26 /M2-))
  )
  (module Mounting_Holes:MountingHole_6.4mm_M6_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 309.88 165.1)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (fp_text reference P5 (at 0 -7.4) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 7.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 12.8 12.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 15 /M3+))
  )
  (module Mounting_Holes:MountingHole_6.4mm_M6_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 347.98 165.1)
    (descr "Mounting Hole 6.4mm, M6")
    (tags "mounting hole 6.4mm m6")
    (fp_text reference P6 (at 0 -7.4) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 7.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 12.8 12.8) (drill 6.4) (layers *.Cu *.Mask)
      (net 22 /M3-))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 144.78 128.905 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R21 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 /LOCPWR))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(F1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:IDC_Header_Straight_26pins (layer F.Cu) (tedit 0)
    (at 152.4 102.87)
    (descr "26 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference PF-1 (at 15.24 -7.62) (layer F.SilkS))
    (fp_text value HE10-26 (at 15.24 5.223) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /P1-11))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /P1-11))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /P1-8))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /P1-9))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /P1-7))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /P1-10))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(PF-1-Pad15)"))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(PF-1-Pad16)"))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(PF-1-Pad25)"))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(PF-1-Pad26)"))
  )
  (module Connectors:IDC_Header_Straight_26pins (layer F.Cu) (tedit 0)
    (at 228.6 102.87)
    (descr "26 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference PG-1 (at 15.24 -7.62) (layer F.SilkS))
    (fp_text value HE10-26 (at 15.24 5.223) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /P1-1))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /P1-7))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /P1-2))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /P1-8))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /P1-12))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /P1-4))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /P2-1))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /P1-5))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /P1-6))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /P1-3))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /P2-13))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(PF-1-Pad15)"))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(PF-1-Pad16)"))
  )
  (module Connectors:IDC_Header_Straight_26pins (layer F.Cu) (tedit 0)
    (at 304.8 102.87)
    (descr "26 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference PH-1 (at 15.24 -7.62) (layer F.SilkS))
    (fp_text value HE10-26 (at 15.24 5.223) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(PH-1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(PH-1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(PH-1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(PH-1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 22.86 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 22.86 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 25.4 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 25.4 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 27.94 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 30.48 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(PH-1-Pad25)"))
    (pad 26 thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module MountingHole_RevA_04Jul2011:MountingHole_3mm_RevA_Date21Jun2010 (layer F.Cu) (tedit 5A85A17A)
    (at 257.81 111.506)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm_RevA_Date21Jun2010 (at 1.00076 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 2.99974) (layers))
  )
  (dimension 35.56 (width 0.3) (layer Cmts.User)
    (gr_text "1.4000 in" (at 205.74 88.82) (layer Cmts.User))
    (feature1 (pts (xy 223.52 97.79) (xy 223.52 87.47)))
    (feature2 (pts (xy 187.96 97.79) (xy 187.96 87.47)))
    (crossbar (pts (xy 187.96 90.17) (xy 223.52 90.17)))
    (arrow1a (pts (xy 223.52 90.17) (xy 222.393496 90.756421)))
    (arrow1b (pts (xy 223.52 90.17) (xy 222.393496 89.583579)))
    (arrow2a (pts (xy 187.96 90.17) (xy 189.086504 90.756421)))
    (arrow2b (pts (xy 187.96 90.17) (xy 189.086504 89.583579)))
  )
  (dimension 35.56 (width 0.3) (layer Cmts.User)
    (gr_text "1.4000 in" (at 281.94 87.550001) (layer Cmts.User))
    (feature1 (pts (xy 264.16 97.79) (xy 264.16 86.200001)))
    (feature2 (pts (xy 299.72 97.79) (xy 299.72 86.200001)))
    (crossbar (pts (xy 299.72 88.900001) (xy 264.16 88.900001)))
    (arrow1a (pts (xy 264.16 88.900001) (xy 265.286504 88.31358)))
    (arrow1b (pts (xy 264.16 88.900001) (xy 265.286504 89.486422)))
    (arrow2a (pts (xy 299.72 88.900001) (xy 298.593496 88.31358)))
    (arrow2b (pts (xy 299.72 88.900001) (xy 298.593496 89.486422)))
  )
  (gr_text "LOCAL FUSE" (at 126.0475 135.3185) (layer F.SilkS))
  (gr_text "MON SKT FUSE" (at 126.4285 151.1935) (layer F.SilkS))
  (gr_text "Monitor Socket" (at 214.884 178.943) (layer F.SilkS))
  (gr_text "SWITCH \n  SH" (at 345.44 102.87) (layer F.SilkS))
  (gr_text "SWITCH \n  SG" (at 269.24 102.87) (layer F.SilkS))
  (gr_text "SWITCH \n  SF" (at 193.04 104.14) (layer F.SilkS))
  (gr_text "CONNECTIONS\n   TO TX" (at 102.0445 122.682) (layer F.SilkS))
  (gr_text "    CAL\nFEEDER BACKWARDS" (at 251.968 136.0805 270) (layer F.SilkS))
  (gr_text "    CAL\nFEEDER FORWARDS" (at 282.194 134.747 270) (layer F.SilkS))
  (gr_text "    CAL\nGRID FORWARDS" (at 311.785 135.509 270) (layer F.SilkS))
  (gr_text "   CAL\nGRID BACKWARDS" (at 342.138 136.017 270) (layer F.SilkS))
  (gr_text "B6525/6 Metering PCB v2\n       CDT 2017" (at 359.6005 126.0475 270) (layer F.SilkS))
  (dimension 38.1 (width 0.3) (layer Dwgs.User)
    (gr_text "1.5000 in" (at 100.33 176.61) (layer Dwgs.User))
    (feature1 (pts (xy 81.28 165.1) (xy 81.28 177.96)))
    (feature2 (pts (xy 119.38 165.1) (xy 119.38 177.96)))
    (crossbar (pts (xy 119.38 175.26) (xy 81.28 175.26)))
    (arrow1a (pts (xy 81.28 175.26) (xy 82.406504 174.673579)))
    (arrow1b (pts (xy 81.28 175.26) (xy 82.406504 175.846421)))
    (arrow2a (pts (xy 119.38 175.26) (xy 118.253496 174.673579)))
    (arrow2b (pts (xy 119.38 175.26) (xy 118.253496 175.846421)))
  )
  (dimension 38.1 (width 0.3) (layer Dwgs.User)
    (gr_text "1.5000 in" (at 328.93 153.59) (layer Dwgs.User))
    (feature1 (pts (xy 309.88 165.1) (xy 309.88 152.24)))
    (feature2 (pts (xy 347.98 165.1) (xy 347.98 152.24)))
    (crossbar (pts (xy 347.98 154.94) (xy 309.88 154.94)))
    (arrow1a (pts (xy 309.88 154.94) (xy 311.006504 154.353579)))
    (arrow1b (pts (xy 309.88 154.94) (xy 311.006504 155.526421)))
    (arrow2a (pts (xy 347.98 154.94) (xy 346.853496 154.353579)))
    (arrow2b (pts (xy 347.98 154.94) (xy 346.853496 155.526421)))
  )
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8000 in" (at 356.95 175.26 270) (layer Dwgs.User))
    (feature1 (pts (xy 347.98 185.42) (xy 358.3 185.42)))
    (feature2 (pts (xy 347.98 165.1) (xy 358.3 165.1)))
    (crossbar (pts (xy 355.6 165.1) (xy 355.6 185.42)))
    (arrow1a (pts (xy 355.6 185.42) (xy 355.013579 184.293496)))
    (arrow1b (pts (xy 355.6 185.42) (xy 356.186421 184.293496)))
    (arrow2a (pts (xy 355.6 165.1) (xy 355.013579 166.226504)))
    (arrow2b (pts (xy 355.6 165.1) (xy 356.186421 166.226504)))
  )
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8000 in" (at 133.43 175.26 270) (layer Dwgs.User))
    (feature1 (pts (xy 119.38 185.42) (xy 134.78 185.42)))
    (feature2 (pts (xy 119.38 165.1) (xy 134.78 165.1)))
    (crossbar (pts (xy 132.08 165.1) (xy 132.08 185.42)))
    (arrow1a (pts (xy 132.08 185.42) (xy 131.493579 184.293496)))
    (arrow1b (pts (xy 132.08 185.42) (xy 132.666421 184.293496)))
    (arrow2a (pts (xy 132.08 165.1) (xy 131.493579 166.226504)))
    (arrow2b (pts (xy 132.08 165.1) (xy 132.666421 166.226504)))
  )
  (dimension 228.6 (width 0.3) (layer Dwgs.User)
    (gr_text "9.0000 in" (at 233.68 191.85) (layer Dwgs.User))
    (feature1 (pts (xy 347.98 165.1) (xy 347.98 193.2)))
    (feature2 (pts (xy 119.38 165.1) (xy 119.38 193.2)))
    (crossbar (pts (xy 119.38 190.5) (xy 347.98 190.5)))
    (arrow1a (pts (xy 347.98 190.5) (xy 346.853496 191.086421)))
    (arrow1b (pts (xy 347.98 190.5) (xy 346.853496 189.913579)))
    (arrow2a (pts (xy 119.38 190.5) (xy 120.506504 191.086421)))
    (arrow2b (pts (xy 119.38 190.5) (xy 120.506504 189.913579)))
  )
  (gr_line (start 65 185) (end 65 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 365 185) (end 65 185) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 365 95) (end 365 185) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65 95) (end 365 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 364.871 95.123) (xy 364.871 184.912) (xy 65.0875 184.912) (xy 65.0875 95.0595)
      )
    )
  )
  (zone (net 16) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 364.871 95.123) (xy 364.871 184.912) (xy 65.0875 184.912) (xy 65.0875 95.0595)
      )
    )
  )
)
