(kicad_pcb (version 20171130) (host pcbnew 5.1.9)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 18)
    (zones 0)
    (modules 3)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.778)
    (user_trace_width 1.778)
    (user_trace_width 2.925001)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 113.03 83.82)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vna_jig:sma_edge (layer F.Cu) (tedit 606D34E9)
    (at 124.46 87.5 90)
    (fp_text reference J2 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25 90) (layer F.Fab))
    (pad 2 smd rect (at -3.4925 0 90) (size 2.665 5) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4925 0 90) (size 2.665 5) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4925 0 90) (size 2.665 5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.4925 0 90) (size 2.665 5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.78 5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
  )
  (module vna_jig:sma_edge (layer F.Cu) (tedit 606D34E9)
    (at 104.14 87.5 270)
    (fp_text reference J1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -3.25 90) (layer F.Fab))
    (pad 2 smd rect (at -3.4925 0 270) (size 2.665 5) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4925 0 270) (size 2.665 5) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.4925 0 270) (size 2.665 5) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.4925 0 270) (size 2.665 5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.78 5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (gr_text "vna_jig v0.2\nby Kamocat" (at 109.22 87.63 90) (layer B.SilkS))
  (gr_line (start 127 81.28) (end 101.6 81.28) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 127 93.98) (end 127 81.28) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 93.98) (end 127 93.98) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 81.28) (end 101.6 93.98) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127 93.98) (xy 101.6 93.98) (xy 101.6 81.28) (xy 127 81.28)
      )
    )
  )
)
