<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="101.6" width="0" layer="20"/>
<wire x1="38.1" y1="101.6" x2="0" y2="101.6" width="0" layer="20"/>
<wire x1="0" y1="101.6" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="0.635" drill="0.35"/>
<hole x="3.81" y="1.27" drill="0.35"/>
<hole x="3.81" y="1.905" drill="0.35"/>
<hole x="3.81" y="2.54" drill="0.35"/>
<hole x="3.81" y="3.175" drill="0.35"/>
<hole x="3.81" y="3.81" drill="0.35"/>
<hole x="3.81" y="4.445" drill="0.35"/>
<hole x="3.81" y="5.08" drill="0.35"/>
<hole x="3.81" y="5.715" drill="0.35"/>
<hole x="3.81" y="6.35" drill="0.35"/>
<hole x="3.81" y="6.985" drill="0.35"/>
<hole x="3.81" y="7.62" drill="0.35"/>
<hole x="3.81" y="8.255" drill="0.35"/>
<hole x="3.81" y="8.89" drill="0.35"/>
<hole x="3.81" y="9.525" drill="0.35"/>
<hole x="3.81" y="10.16" drill="0.35"/>
<hole x="3.81" y="10.795" drill="0.35"/>
<hole x="3.81" y="11.43" drill="0.35"/>
<hole x="3.81" y="12.065" drill="0.35"/>
<hole x="3.81" y="12.7" drill="0.35"/>
<hole x="3.81" y="13.335" drill="0.35"/>
<hole x="3.81" y="13.97" drill="0.35"/>
<hole x="3.81" y="14.605" drill="0.35"/>
<hole x="3.81" y="15.24" drill="0.35"/>
<hole x="3.81" y="15.875" drill="0.35"/>
<hole x="3.81" y="16.51" drill="0.35"/>
<hole x="3.81" y="17.145" drill="0.35"/>
<hole x="3.81" y="17.78" drill="0.35"/>
<hole x="3.81" y="18.415" drill="0.35"/>
<hole x="3.81" y="19.05" drill="0.35"/>
<hole x="3.81" y="19.685" drill="0.35"/>
<hole x="3.81" y="20.32" drill="0.35"/>
<hole x="4.445" y="20.32" drill="0.35"/>
<hole x="5.08" y="20.32" drill="0.35"/>
<hole x="5.715" y="20.32" drill="0.35"/>
<hole x="6.35" y="20.32" drill="0.35"/>
<hole x="6.985" y="20.32" drill="0.35"/>
<hole x="7.62" y="20.32" drill="0.35"/>
<hole x="8.255" y="20.32" drill="0.35"/>
<hole x="8.89" y="20.32" drill="0.35"/>
<hole x="9.525" y="20.32" drill="0.35"/>
<hole x="10.16" y="20.32" drill="0.35"/>
<hole x="10.795" y="20.32" drill="0.35"/>
<hole x="11.43" y="20.32" drill="0.35"/>
<hole x="11.43" y="0.635" drill="0.35"/>
<hole x="11.43" y="1.27" drill="0.35"/>
<hole x="11.43" y="1.905" drill="0.35"/>
<hole x="11.43" y="2.54" drill="0.35"/>
<hole x="11.43" y="3.175" drill="0.35"/>
<hole x="11.43" y="3.81" drill="0.35"/>
<hole x="11.43" y="4.445" drill="0.35"/>
<hole x="11.43" y="5.08" drill="0.35"/>
<hole x="11.43" y="5.715" drill="0.35"/>
<hole x="11.43" y="6.35" drill="0.35"/>
<hole x="11.43" y="6.985" drill="0.35"/>
<hole x="11.43" y="7.62" drill="0.35"/>
<hole x="11.43" y="8.255" drill="0.35"/>
<hole x="11.43" y="8.89" drill="0.35"/>
<hole x="11.43" y="9.525" drill="0.35"/>
<hole x="11.43" y="10.16" drill="0.35"/>
<hole x="11.43" y="10.795" drill="0.35"/>
<hole x="11.43" y="11.43" drill="0.35"/>
<hole x="11.43" y="12.065" drill="0.35"/>
<hole x="11.43" y="12.7" drill="0.35"/>
<hole x="11.43" y="13.335" drill="0.35"/>
<hole x="11.43" y="13.97" drill="0.35"/>
<hole x="11.43" y="14.605" drill="0.35"/>
<hole x="11.43" y="15.24" drill="0.35"/>
<hole x="11.43" y="15.875" drill="0.35"/>
<hole x="11.43" y="16.51" drill="0.35"/>
<hole x="11.43" y="17.145" drill="0.35"/>
<hole x="11.43" y="17.78" drill="0.35"/>
<hole x="11.43" y="18.415" drill="0.35"/>
<hole x="11.43" y="19.05" drill="0.35"/>
<hole x="11.43" y="19.685" drill="0.35"/>
<hole x="12.065" y="20.32" drill="0.35"/>
<hole x="12.7" y="20.32" drill="0.35"/>
<hole x="13.335" y="20.32" drill="0.35"/>
<hole x="13.97" y="20.32" drill="0.35"/>
<hole x="14.605" y="20.32" drill="0.35"/>
<hole x="15.24" y="20.32" drill="0.35"/>
<hole x="15.875" y="20.32" drill="0.35"/>
<hole x="16.51" y="20.32" drill="0.35"/>
<hole x="17.145" y="20.32" drill="0.35"/>
<hole x="17.78" y="20.32" drill="0.35"/>
<hole x="18.415" y="20.32" drill="0.35"/>
<hole x="19.05" y="20.32" drill="0.35"/>
<hole x="19.05" y="0.635" drill="0.35"/>
<hole x="19.05" y="1.27" drill="0.35"/>
<hole x="19.05" y="1.905" drill="0.35"/>
<hole x="19.05" y="2.54" drill="0.35"/>
<hole x="19.05" y="3.175" drill="0.35"/>
<hole x="19.05" y="3.81" drill="0.35"/>
<hole x="19.05" y="4.445" drill="0.35"/>
<hole x="19.05" y="5.08" drill="0.35"/>
<hole x="19.05" y="5.715" drill="0.35"/>
<hole x="19.05" y="6.35" drill="0.35"/>
<hole x="19.05" y="6.985" drill="0.35"/>
<hole x="19.05" y="7.62" drill="0.35"/>
<hole x="19.05" y="8.255" drill="0.35"/>
<hole x="19.05" y="8.89" drill="0.35"/>
<hole x="19.05" y="9.525" drill="0.35"/>
<hole x="19.05" y="10.16" drill="0.35"/>
<hole x="19.05" y="10.795" drill="0.35"/>
<hole x="19.05" y="11.43" drill="0.35"/>
<hole x="19.05" y="12.065" drill="0.35"/>
<hole x="19.05" y="12.7" drill="0.35"/>
<hole x="19.05" y="13.335" drill="0.35"/>
<hole x="19.05" y="13.97" drill="0.35"/>
<hole x="19.05" y="14.605" drill="0.35"/>
<hole x="19.05" y="15.24" drill="0.35"/>
<hole x="19.05" y="15.875" drill="0.35"/>
<hole x="19.05" y="16.51" drill="0.35"/>
<hole x="19.05" y="17.145" drill="0.35"/>
<hole x="19.05" y="17.78" drill="0.35"/>
<hole x="19.05" y="18.415" drill="0.35"/>
<hole x="19.05" y="19.05" drill="0.35"/>
<hole x="19.05" y="19.685" drill="0.35"/>
<hole x="3.81" y="20.955" drill="0.35"/>
<hole x="3.81" y="21.59" drill="0.35"/>
<hole x="3.81" y="22.225" drill="0.35"/>
<hole x="3.81" y="22.86" drill="0.35"/>
<hole x="3.81" y="23.495" drill="0.35"/>
<hole x="3.81" y="24.13" drill="0.35"/>
<hole x="3.81" y="24.765" drill="0.35"/>
<hole x="3.81" y="25.4" drill="0.35"/>
<hole x="3.81" y="26.035" drill="0.35"/>
<hole x="3.81" y="26.67" drill="0.35"/>
<hole x="3.81" y="27.305" drill="0.35"/>
<hole x="3.81" y="27.94" drill="0.35"/>
<hole x="3.81" y="28.575" drill="0.35"/>
<hole x="3.81" y="29.21" drill="0.35"/>
<hole x="3.81" y="29.845" drill="0.35"/>
<hole x="3.81" y="30.48" drill="0.35"/>
<hole x="3.81" y="31.115" drill="0.35"/>
<hole x="3.81" y="31.75" drill="0.35"/>
<hole x="3.81" y="32.385" drill="0.35"/>
<hole x="3.81" y="33.02" drill="0.35"/>
<hole x="3.81" y="33.655" drill="0.35"/>
<hole x="3.81" y="34.29" drill="0.35"/>
<hole x="3.81" y="34.925" drill="0.35"/>
<hole x="3.81" y="35.56" drill="0.35"/>
<hole x="3.81" y="36.195" drill="0.35"/>
<hole x="3.81" y="36.83" drill="0.35"/>
<hole x="3.81" y="37.465" drill="0.35"/>
<hole x="3.81" y="38.1" drill="0.35"/>
<hole x="3.81" y="38.735" drill="0.35"/>
<hole x="3.81" y="39.37" drill="0.35"/>
<hole x="3.81" y="40.005" drill="0.35"/>
<hole x="3.81" y="40.64" drill="0.35"/>
<hole x="4.445" y="40.64" drill="0.35"/>
<hole x="5.08" y="40.64" drill="0.35"/>
<hole x="5.715" y="40.64" drill="0.35"/>
<hole x="6.35" y="40.64" drill="0.35"/>
<hole x="6.985" y="40.64" drill="0.35"/>
<hole x="7.62" y="40.64" drill="0.35"/>
<hole x="8.255" y="40.64" drill="0.35"/>
<hole x="8.89" y="40.64" drill="0.35"/>
<hole x="9.525" y="40.64" drill="0.35"/>
<hole x="10.16" y="40.64" drill="0.35"/>
<hole x="10.795" y="40.64" drill="0.35"/>
<hole x="11.43" y="40.64" drill="0.35"/>
<hole x="11.43" y="20.955" drill="0.35"/>
<hole x="11.43" y="21.59" drill="0.35"/>
<hole x="11.43" y="22.225" drill="0.35"/>
<hole x="11.43" y="22.86" drill="0.35"/>
<hole x="11.43" y="23.495" drill="0.35"/>
<hole x="11.43" y="24.13" drill="0.35"/>
<hole x="11.43" y="24.765" drill="0.35"/>
<hole x="11.43" y="25.4" drill="0.35"/>
<hole x="11.43" y="26.035" drill="0.35"/>
<hole x="11.43" y="26.67" drill="0.35"/>
<hole x="11.43" y="27.305" drill="0.35"/>
<hole x="11.43" y="27.94" drill="0.35"/>
<hole x="11.43" y="28.575" drill="0.35"/>
<hole x="11.43" y="29.21" drill="0.35"/>
<hole x="11.43" y="29.845" drill="0.35"/>
<hole x="11.43" y="30.48" drill="0.35"/>
<hole x="11.43" y="31.115" drill="0.35"/>
<hole x="11.43" y="31.75" drill="0.35"/>
<hole x="11.43" y="32.385" drill="0.35"/>
<hole x="11.43" y="33.02" drill="0.35"/>
<hole x="11.43" y="33.655" drill="0.35"/>
<hole x="11.43" y="34.29" drill="0.35"/>
<hole x="11.43" y="34.925" drill="0.35"/>
<hole x="11.43" y="35.56" drill="0.35"/>
<hole x="11.43" y="36.195" drill="0.35"/>
<hole x="11.43" y="36.83" drill="0.35"/>
<hole x="11.43" y="37.465" drill="0.35"/>
<hole x="11.43" y="38.1" drill="0.35"/>
<hole x="11.43" y="38.735" drill="0.35"/>
<hole x="11.43" y="39.37" drill="0.35"/>
<hole x="11.43" y="40.005" drill="0.35"/>
<hole x="12.065" y="40.64" drill="0.35"/>
<hole x="12.7" y="40.64" drill="0.35"/>
<hole x="13.335" y="40.64" drill="0.35"/>
<hole x="13.97" y="40.64" drill="0.35"/>
<hole x="14.605" y="40.64" drill="0.35"/>
<hole x="15.24" y="40.64" drill="0.35"/>
<hole x="15.875" y="40.64" drill="0.35"/>
<hole x="16.51" y="40.64" drill="0.35"/>
<hole x="17.145" y="40.64" drill="0.35"/>
<hole x="17.78" y="40.64" drill="0.35"/>
<hole x="18.415" y="40.64" drill="0.35"/>
<hole x="19.05" y="40.64" drill="0.35"/>
<hole x="19.05" y="20.955" drill="0.35"/>
<hole x="19.05" y="21.59" drill="0.35"/>
<hole x="19.05" y="22.225" drill="0.35"/>
<hole x="19.05" y="22.86" drill="0.35"/>
<hole x="19.05" y="23.495" drill="0.35"/>
<hole x="19.05" y="24.13" drill="0.35"/>
<hole x="19.05" y="24.765" drill="0.35"/>
<hole x="19.05" y="25.4" drill="0.35"/>
<hole x="19.05" y="26.035" drill="0.35"/>
<hole x="19.05" y="26.67" drill="0.35"/>
<hole x="19.05" y="27.305" drill="0.35"/>
<hole x="19.05" y="27.94" drill="0.35"/>
<hole x="19.05" y="28.575" drill="0.35"/>
<hole x="19.05" y="29.21" drill="0.35"/>
<hole x="19.05" y="29.845" drill="0.35"/>
<hole x="19.05" y="30.48" drill="0.35"/>
<hole x="19.05" y="31.115" drill="0.35"/>
<hole x="19.05" y="31.75" drill="0.35"/>
<hole x="19.05" y="32.385" drill="0.35"/>
<hole x="19.05" y="33.02" drill="0.35"/>
<hole x="19.05" y="33.655" drill="0.35"/>
<hole x="19.05" y="34.29" drill="0.35"/>
<hole x="19.05" y="34.925" drill="0.35"/>
<hole x="19.05" y="35.56" drill="0.35"/>
<hole x="19.05" y="36.195" drill="0.35"/>
<hole x="19.05" y="36.83" drill="0.35"/>
<hole x="19.05" y="37.465" drill="0.35"/>
<hole x="19.05" y="38.1" drill="0.35"/>
<hole x="19.05" y="38.735" drill="0.35"/>
<hole x="19.05" y="39.37" drill="0.35"/>
<hole x="19.05" y="40.005" drill="0.35"/>
<hole x="3.81" y="41.275" drill="0.35"/>
<hole x="3.81" y="41.91" drill="0.35"/>
<hole x="3.81" y="42.545" drill="0.35"/>
<hole x="3.81" y="43.18" drill="0.35"/>
<hole x="3.81" y="43.815" drill="0.35"/>
<hole x="3.81" y="44.45" drill="0.35"/>
<hole x="3.81" y="45.085" drill="0.35"/>
<hole x="3.81" y="45.72" drill="0.35"/>
<hole x="3.81" y="46.355" drill="0.35"/>
<hole x="3.81" y="46.99" drill="0.35"/>
<hole x="3.81" y="47.625" drill="0.35"/>
<hole x="3.81" y="48.26" drill="0.35"/>
<hole x="3.81" y="48.895" drill="0.35"/>
<hole x="3.81" y="49.53" drill="0.35"/>
<hole x="3.81" y="50.165" drill="0.35"/>
<hole x="3.81" y="50.8" drill="0.35"/>
<hole x="3.81" y="51.435" drill="0.35"/>
<hole x="3.81" y="52.07" drill="0.35"/>
<hole x="3.81" y="52.705" drill="0.35"/>
<hole x="3.81" y="53.34" drill="0.35"/>
<hole x="3.81" y="53.975" drill="0.35"/>
<hole x="3.81" y="54.61" drill="0.35"/>
<hole x="3.81" y="55.245" drill="0.35"/>
<hole x="3.81" y="55.88" drill="0.35"/>
<hole x="3.81" y="56.515" drill="0.35"/>
<hole x="3.81" y="57.15" drill="0.35"/>
<hole x="3.81" y="57.785" drill="0.35"/>
<hole x="3.81" y="58.42" drill="0.35"/>
<hole x="3.81" y="59.055" drill="0.35"/>
<hole x="3.81" y="59.69" drill="0.35"/>
<hole x="3.81" y="60.325" drill="0.35"/>
<hole x="3.81" y="60.96" drill="0.35"/>
<hole x="4.445" y="60.96" drill="0.35"/>
<hole x="5.08" y="60.96" drill="0.35"/>
<hole x="5.715" y="60.96" drill="0.35"/>
<hole x="6.35" y="60.96" drill="0.35"/>
<hole x="6.985" y="60.96" drill="0.35"/>
<hole x="7.62" y="60.96" drill="0.35"/>
<hole x="8.255" y="60.96" drill="0.35"/>
<hole x="8.89" y="60.96" drill="0.35"/>
<hole x="9.525" y="60.96" drill="0.35"/>
<hole x="10.16" y="60.96" drill="0.35"/>
<hole x="10.795" y="60.96" drill="0.35"/>
<hole x="11.43" y="60.96" drill="0.35"/>
<hole x="11.43" y="41.275" drill="0.35"/>
<hole x="11.43" y="41.91" drill="0.35"/>
<hole x="11.43" y="42.545" drill="0.35"/>
<hole x="11.43" y="43.18" drill="0.35"/>
<hole x="11.43" y="43.815" drill="0.35"/>
<hole x="11.43" y="44.45" drill="0.35"/>
<hole x="11.43" y="45.085" drill="0.35"/>
<hole x="11.43" y="45.72" drill="0.35"/>
<hole x="11.43" y="46.355" drill="0.35"/>
<hole x="11.43" y="46.99" drill="0.35"/>
<hole x="11.43" y="47.625" drill="0.35"/>
<hole x="11.43" y="48.26" drill="0.35"/>
<hole x="11.43" y="48.895" drill="0.35"/>
<hole x="11.43" y="49.53" drill="0.35"/>
<hole x="11.43" y="50.165" drill="0.35"/>
<hole x="11.43" y="50.8" drill="0.35"/>
<hole x="11.43" y="51.435" drill="0.35"/>
<hole x="11.43" y="52.07" drill="0.35"/>
<hole x="11.43" y="52.705" drill="0.35"/>
<hole x="11.43" y="53.34" drill="0.35"/>
<hole x="11.43" y="53.975" drill="0.35"/>
<hole x="11.43" y="54.61" drill="0.35"/>
<hole x="11.43" y="55.245" drill="0.35"/>
<hole x="11.43" y="55.88" drill="0.35"/>
<hole x="11.43" y="56.515" drill="0.35"/>
<hole x="11.43" y="57.15" drill="0.35"/>
<hole x="11.43" y="57.785" drill="0.35"/>
<hole x="11.43" y="58.42" drill="0.35"/>
<hole x="11.43" y="59.055" drill="0.35"/>
<hole x="11.43" y="59.69" drill="0.35"/>
<hole x="11.43" y="60.325" drill="0.35"/>
<hole x="12.065" y="60.96" drill="0.35"/>
<hole x="12.7" y="60.96" drill="0.35"/>
<hole x="13.335" y="60.96" drill="0.35"/>
<hole x="13.97" y="60.96" drill="0.35"/>
<hole x="14.605" y="60.96" drill="0.35"/>
<hole x="15.24" y="60.96" drill="0.35"/>
<hole x="15.875" y="60.96" drill="0.35"/>
<hole x="16.51" y="60.96" drill="0.35"/>
<hole x="17.145" y="60.96" drill="0.35"/>
<hole x="17.78" y="60.96" drill="0.35"/>
<hole x="18.415" y="60.96" drill="0.35"/>
<hole x="19.05" y="60.96" drill="0.35"/>
<hole x="19.05" y="41.275" drill="0.35"/>
<hole x="19.05" y="41.91" drill="0.35"/>
<hole x="19.05" y="42.545" drill="0.35"/>
<hole x="19.05" y="43.18" drill="0.35"/>
<hole x="19.05" y="43.815" drill="0.35"/>
<hole x="19.05" y="44.45" drill="0.35"/>
<hole x="19.05" y="45.085" drill="0.35"/>
<hole x="19.05" y="45.72" drill="0.35"/>
<hole x="19.05" y="46.355" drill="0.35"/>
<hole x="19.05" y="46.99" drill="0.35"/>
<hole x="19.05" y="47.625" drill="0.35"/>
<hole x="19.05" y="48.26" drill="0.35"/>
<hole x="19.05" y="48.895" drill="0.35"/>
<hole x="19.05" y="49.53" drill="0.35"/>
<hole x="19.05" y="50.165" drill="0.35"/>
<hole x="19.05" y="50.8" drill="0.35"/>
<hole x="19.05" y="51.435" drill="0.35"/>
<hole x="19.05" y="52.07" drill="0.35"/>
<hole x="19.05" y="52.705" drill="0.35"/>
<hole x="19.05" y="53.34" drill="0.35"/>
<hole x="19.05" y="53.975" drill="0.35"/>
<hole x="19.05" y="54.61" drill="0.35"/>
<hole x="19.05" y="55.245" drill="0.35"/>
<hole x="19.05" y="55.88" drill="0.35"/>
<hole x="19.05" y="56.515" drill="0.35"/>
<hole x="19.05" y="57.15" drill="0.35"/>
<hole x="19.05" y="57.785" drill="0.35"/>
<hole x="19.05" y="58.42" drill="0.35"/>
<hole x="19.05" y="59.055" drill="0.35"/>
<hole x="19.05" y="59.69" drill="0.35"/>
<hole x="19.05" y="60.325" drill="0.35"/>
<hole x="3.81" y="61.595" drill="0.35"/>
<hole x="3.81" y="62.23" drill="0.35"/>
<hole x="3.81" y="62.865" drill="0.35"/>
<hole x="3.81" y="63.5" drill="0.35"/>
<hole x="3.81" y="64.135" drill="0.35"/>
<hole x="3.81" y="64.77" drill="0.35"/>
<hole x="3.81" y="65.405" drill="0.35"/>
<hole x="3.81" y="66.04" drill="0.35"/>
<hole x="3.81" y="66.675" drill="0.35"/>
<hole x="3.81" y="67.31" drill="0.35"/>
<hole x="3.81" y="67.945" drill="0.35"/>
<hole x="3.81" y="68.58" drill="0.35"/>
<hole x="3.81" y="69.215" drill="0.35"/>
<hole x="3.81" y="69.85" drill="0.35"/>
<hole x="3.81" y="70.485" drill="0.35"/>
<hole x="3.81" y="71.12" drill="0.35"/>
<hole x="3.81" y="71.755" drill="0.35"/>
<hole x="3.81" y="72.39" drill="0.35"/>
<hole x="3.81" y="73.025" drill="0.35"/>
<hole x="3.81" y="73.66" drill="0.35"/>
<hole x="3.81" y="74.295" drill="0.35"/>
<hole x="3.81" y="74.93" drill="0.35"/>
<hole x="3.81" y="75.565" drill="0.35"/>
<hole x="3.81" y="76.2" drill="0.35"/>
<hole x="3.81" y="76.835" drill="0.35"/>
<hole x="3.81" y="77.47" drill="0.35"/>
<hole x="3.81" y="78.105" drill="0.35"/>
<hole x="3.81" y="78.74" drill="0.35"/>
<hole x="3.81" y="79.375" drill="0.35"/>
<hole x="3.81" y="80.01" drill="0.35"/>
<hole x="3.81" y="80.645" drill="0.35"/>
<hole x="3.81" y="81.28" drill="0.35"/>
<hole x="4.445" y="81.28" drill="0.35"/>
<hole x="5.08" y="81.28" drill="0.35"/>
<hole x="5.715" y="81.28" drill="0.35"/>
<hole x="6.35" y="81.28" drill="0.35"/>
<hole x="6.985" y="81.28" drill="0.35"/>
<hole x="7.62" y="81.28" drill="0.35"/>
<hole x="8.255" y="81.28" drill="0.35"/>
<hole x="8.89" y="81.28" drill="0.35"/>
<hole x="9.525" y="81.28" drill="0.35"/>
<hole x="10.16" y="81.28" drill="0.35"/>
<hole x="10.795" y="81.28" drill="0.35"/>
<hole x="11.43" y="81.28" drill="0.35"/>
<hole x="11.43" y="61.595" drill="0.35"/>
<hole x="11.43" y="62.23" drill="0.35"/>
<hole x="11.43" y="62.865" drill="0.35"/>
<hole x="11.43" y="63.5" drill="0.35"/>
<hole x="11.43" y="64.135" drill="0.35"/>
<hole x="11.43" y="64.77" drill="0.35"/>
<hole x="11.43" y="65.405" drill="0.35"/>
<hole x="11.43" y="66.04" drill="0.35"/>
<hole x="11.43" y="66.675" drill="0.35"/>
<hole x="11.43" y="67.31" drill="0.35"/>
<hole x="11.43" y="67.945" drill="0.35"/>
<hole x="11.43" y="68.58" drill="0.35"/>
<hole x="11.43" y="69.215" drill="0.35"/>
<hole x="11.43" y="69.85" drill="0.35"/>
<hole x="11.43" y="70.485" drill="0.35"/>
<hole x="11.43" y="71.12" drill="0.35"/>
<hole x="11.43" y="71.755" drill="0.35"/>
<hole x="11.43" y="72.39" drill="0.35"/>
<hole x="11.43" y="73.025" drill="0.35"/>
<hole x="11.43" y="73.66" drill="0.35"/>
<hole x="11.43" y="74.295" drill="0.35"/>
<hole x="11.43" y="74.93" drill="0.35"/>
<hole x="11.43" y="75.565" drill="0.35"/>
<hole x="11.43" y="76.2" drill="0.35"/>
<hole x="11.43" y="76.835" drill="0.35"/>
<hole x="11.43" y="77.47" drill="0.35"/>
<hole x="11.43" y="78.105" drill="0.35"/>
<hole x="11.43" y="78.74" drill="0.35"/>
<hole x="11.43" y="79.375" drill="0.35"/>
<hole x="11.43" y="80.01" drill="0.35"/>
<hole x="11.43" y="80.645" drill="0.35"/>
<hole x="12.065" y="81.28" drill="0.35"/>
<hole x="12.7" y="81.28" drill="0.35"/>
<hole x="13.335" y="81.28" drill="0.35"/>
<hole x="13.97" y="81.28" drill="0.35"/>
<hole x="14.605" y="81.28" drill="0.35"/>
<hole x="15.24" y="81.28" drill="0.35"/>
<hole x="15.875" y="81.28" drill="0.35"/>
<hole x="16.51" y="81.28" drill="0.35"/>
<hole x="17.145" y="81.28" drill="0.35"/>
<hole x="17.78" y="81.28" drill="0.35"/>
<hole x="18.415" y="81.28" drill="0.35"/>
<hole x="19.05" y="81.28" drill="0.35"/>
<hole x="19.05" y="61.595" drill="0.35"/>
<hole x="19.05" y="62.23" drill="0.35"/>
<hole x="19.05" y="62.865" drill="0.35"/>
<hole x="19.05" y="63.5" drill="0.35"/>
<hole x="19.05" y="64.135" drill="0.35"/>
<hole x="19.05" y="64.77" drill="0.35"/>
<hole x="19.05" y="65.405" drill="0.35"/>
<hole x="19.05" y="66.04" drill="0.35"/>
<hole x="19.05" y="66.675" drill="0.35"/>
<hole x="19.05" y="67.31" drill="0.35"/>
<hole x="19.05" y="67.945" drill="0.35"/>
<hole x="19.05" y="68.58" drill="0.35"/>
<hole x="19.05" y="69.215" drill="0.35"/>
<hole x="19.05" y="69.85" drill="0.35"/>
<hole x="19.05" y="70.485" drill="0.35"/>
<hole x="19.05" y="71.12" drill="0.35"/>
<hole x="19.05" y="71.755" drill="0.35"/>
<hole x="19.05" y="72.39" drill="0.35"/>
<hole x="19.05" y="73.025" drill="0.35"/>
<hole x="19.05" y="73.66" drill="0.35"/>
<hole x="19.05" y="74.295" drill="0.35"/>
<hole x="19.05" y="74.93" drill="0.35"/>
<hole x="19.05" y="75.565" drill="0.35"/>
<hole x="19.05" y="76.2" drill="0.35"/>
<hole x="19.05" y="76.835" drill="0.35"/>
<hole x="19.05" y="77.47" drill="0.35"/>
<hole x="19.05" y="78.105" drill="0.35"/>
<hole x="19.05" y="78.74" drill="0.35"/>
<hole x="19.05" y="79.375" drill="0.35"/>
<hole x="19.05" y="80.01" drill="0.35"/>
<hole x="19.05" y="80.645" drill="0.35"/>
<hole x="19.685" y="20.32" drill="0.35"/>
<hole x="20.32" y="20.32" drill="0.35"/>
<hole x="20.955" y="20.32" drill="0.35"/>
<hole x="21.59" y="20.32" drill="0.35"/>
<hole x="22.225" y="20.32" drill="0.35"/>
<hole x="22.86" y="20.32" drill="0.35"/>
<hole x="23.495" y="20.32" drill="0.35"/>
<hole x="24.13" y="20.32" drill="0.35"/>
<hole x="24.765" y="20.32" drill="0.35"/>
<hole x="25.4" y="20.32" drill="0.35"/>
<hole x="26.035" y="20.32" drill="0.35"/>
<hole x="26.67" y="20.32" drill="0.35"/>
<hole x="26.67" y="0.635" drill="0.35"/>
<hole x="26.67" y="1.27" drill="0.35"/>
<hole x="26.67" y="1.905" drill="0.35"/>
<hole x="26.67" y="2.54" drill="0.35"/>
<hole x="26.67" y="3.175" drill="0.35"/>
<hole x="26.67" y="3.81" drill="0.35"/>
<hole x="26.67" y="4.445" drill="0.35"/>
<hole x="26.67" y="5.08" drill="0.35"/>
<hole x="26.67" y="5.715" drill="0.35"/>
<hole x="26.67" y="6.35" drill="0.35"/>
<hole x="26.67" y="6.985" drill="0.35"/>
<hole x="26.67" y="7.62" drill="0.35"/>
<hole x="26.67" y="8.255" drill="0.35"/>
<hole x="26.67" y="8.89" drill="0.35"/>
<hole x="26.67" y="9.525" drill="0.35"/>
<hole x="26.67" y="10.16" drill="0.35"/>
<hole x="26.67" y="10.795" drill="0.35"/>
<hole x="26.67" y="11.43" drill="0.35"/>
<hole x="26.67" y="12.065" drill="0.35"/>
<hole x="26.67" y="12.7" drill="0.35"/>
<hole x="26.67" y="13.335" drill="0.35"/>
<hole x="26.67" y="13.97" drill="0.35"/>
<hole x="26.67" y="14.605" drill="0.35"/>
<hole x="26.67" y="15.24" drill="0.35"/>
<hole x="26.67" y="15.875" drill="0.35"/>
<hole x="26.67" y="16.51" drill="0.35"/>
<hole x="26.67" y="17.145" drill="0.35"/>
<hole x="26.67" y="17.78" drill="0.35"/>
<hole x="26.67" y="18.415" drill="0.35"/>
<hole x="26.67" y="19.05" drill="0.35"/>
<hole x="26.67" y="19.685" drill="0.35"/>
<hole x="27.305" y="20.32" drill="0.35"/>
<hole x="27.94" y="20.32" drill="0.35"/>
<hole x="28.575" y="20.32" drill="0.35"/>
<hole x="29.21" y="20.32" drill="0.35"/>
<hole x="29.845" y="20.32" drill="0.35"/>
<hole x="30.48" y="20.32" drill="0.35"/>
<hole x="31.115" y="20.32" drill="0.35"/>
<hole x="31.75" y="20.32" drill="0.35"/>
<hole x="32.385" y="20.32" drill="0.35"/>
<hole x="33.02" y="20.32" drill="0.35"/>
<hole x="33.655" y="20.32" drill="0.35"/>
<hole x="34.29" y="20.32" drill="0.35"/>
<hole x="34.29" y="0.635" drill="0.35"/>
<hole x="34.29" y="1.27" drill="0.35"/>
<hole x="34.29" y="1.905" drill="0.35"/>
<hole x="34.29" y="2.54" drill="0.35"/>
<hole x="34.29" y="3.175" drill="0.35"/>
<hole x="34.29" y="3.81" drill="0.35"/>
<hole x="34.29" y="4.445" drill="0.35"/>
<hole x="34.29" y="5.08" drill="0.35"/>
<hole x="34.29" y="5.715" drill="0.35"/>
<hole x="34.29" y="6.35" drill="0.35"/>
<hole x="34.29" y="6.985" drill="0.35"/>
<hole x="34.29" y="7.62" drill="0.35"/>
<hole x="34.29" y="8.255" drill="0.35"/>
<hole x="34.29" y="8.89" drill="0.35"/>
<hole x="34.29" y="9.525" drill="0.35"/>
<hole x="34.29" y="10.16" drill="0.35"/>
<hole x="34.29" y="10.795" drill="0.35"/>
<hole x="34.29" y="11.43" drill="0.35"/>
<hole x="34.29" y="12.065" drill="0.35"/>
<hole x="34.29" y="12.7" drill="0.35"/>
<hole x="34.29" y="13.335" drill="0.35"/>
<hole x="34.29" y="13.97" drill="0.35"/>
<hole x="34.29" y="14.605" drill="0.35"/>
<hole x="34.29" y="15.24" drill="0.35"/>
<hole x="34.29" y="15.875" drill="0.35"/>
<hole x="34.29" y="16.51" drill="0.35"/>
<hole x="34.29" y="17.145" drill="0.35"/>
<hole x="34.29" y="17.78" drill="0.35"/>
<hole x="34.29" y="18.415" drill="0.35"/>
<hole x="34.29" y="19.05" drill="0.35"/>
<hole x="34.29" y="19.685" drill="0.35"/>
<hole x="19.685" y="40.64" drill="0.35"/>
<hole x="20.32" y="40.64" drill="0.35"/>
<hole x="20.955" y="40.64" drill="0.35"/>
<hole x="21.59" y="40.64" drill="0.35"/>
<hole x="22.225" y="40.64" drill="0.35"/>
<hole x="22.86" y="40.64" drill="0.35"/>
<hole x="23.495" y="40.64" drill="0.35"/>
<hole x="24.13" y="40.64" drill="0.35"/>
<hole x="24.765" y="40.64" drill="0.35"/>
<hole x="25.4" y="40.64" drill="0.35"/>
<hole x="26.035" y="40.64" drill="0.35"/>
<hole x="26.67" y="40.64" drill="0.35"/>
<hole x="26.67" y="20.955" drill="0.35"/>
<hole x="26.67" y="21.59" drill="0.35"/>
<hole x="26.67" y="22.225" drill="0.35"/>
<hole x="26.67" y="22.86" drill="0.35"/>
<hole x="26.67" y="23.495" drill="0.35"/>
<hole x="26.67" y="24.13" drill="0.35"/>
<hole x="26.67" y="24.765" drill="0.35"/>
<hole x="26.67" y="25.4" drill="0.35"/>
<hole x="26.67" y="26.035" drill="0.35"/>
<hole x="26.67" y="26.67" drill="0.35"/>
<hole x="26.67" y="27.305" drill="0.35"/>
<hole x="26.67" y="27.94" drill="0.35"/>
<hole x="26.67" y="28.575" drill="0.35"/>
<hole x="26.67" y="29.21" drill="0.35"/>
<hole x="26.67" y="29.845" drill="0.35"/>
<hole x="26.67" y="30.48" drill="0.35"/>
<hole x="26.67" y="31.115" drill="0.35"/>
<hole x="26.67" y="31.75" drill="0.35"/>
<hole x="26.67" y="32.385" drill="0.35"/>
<hole x="26.67" y="33.02" drill="0.35"/>
<hole x="26.67" y="33.655" drill="0.35"/>
<hole x="26.67" y="34.29" drill="0.35"/>
<hole x="26.67" y="34.925" drill="0.35"/>
<hole x="26.67" y="35.56" drill="0.35"/>
<hole x="26.67" y="36.195" drill="0.35"/>
<hole x="26.67" y="36.83" drill="0.35"/>
<hole x="26.67" y="37.465" drill="0.35"/>
<hole x="26.67" y="38.1" drill="0.35"/>
<hole x="26.67" y="38.735" drill="0.35"/>
<hole x="26.67" y="39.37" drill="0.35"/>
<hole x="26.67" y="40.005" drill="0.35"/>
<hole x="27.305" y="40.64" drill="0.35"/>
<hole x="27.94" y="40.64" drill="0.35"/>
<hole x="28.575" y="40.64" drill="0.35"/>
<hole x="29.21" y="40.64" drill="0.35"/>
<hole x="29.845" y="40.64" drill="0.35"/>
<hole x="30.48" y="40.64" drill="0.35"/>
<hole x="31.115" y="40.64" drill="0.35"/>
<hole x="31.75" y="40.64" drill="0.35"/>
<hole x="32.385" y="40.64" drill="0.35"/>
<hole x="33.02" y="40.64" drill="0.35"/>
<hole x="33.655" y="40.64" drill="0.35"/>
<hole x="34.29" y="40.64" drill="0.35"/>
<hole x="34.29" y="20.955" drill="0.35"/>
<hole x="34.29" y="21.59" drill="0.35"/>
<hole x="34.29" y="22.225" drill="0.35"/>
<hole x="34.29" y="22.86" drill="0.35"/>
<hole x="34.29" y="23.495" drill="0.35"/>
<hole x="34.29" y="24.13" drill="0.35"/>
<hole x="34.29" y="24.765" drill="0.35"/>
<hole x="34.29" y="25.4" drill="0.35"/>
<hole x="34.29" y="26.035" drill="0.35"/>
<hole x="34.29" y="26.67" drill="0.35"/>
<hole x="34.29" y="27.305" drill="0.35"/>
<hole x="34.29" y="27.94" drill="0.35"/>
<hole x="34.29" y="28.575" drill="0.35"/>
<hole x="34.29" y="29.21" drill="0.35"/>
<hole x="34.29" y="29.845" drill="0.35"/>
<hole x="34.29" y="30.48" drill="0.35"/>
<hole x="34.29" y="31.115" drill="0.35"/>
<hole x="34.29" y="31.75" drill="0.35"/>
<hole x="34.29" y="32.385" drill="0.35"/>
<hole x="34.29" y="33.02" drill="0.35"/>
<hole x="34.29" y="33.655" drill="0.35"/>
<hole x="34.29" y="34.29" drill="0.35"/>
<hole x="34.29" y="34.925" drill="0.35"/>
<hole x="34.29" y="35.56" drill="0.35"/>
<hole x="34.29" y="36.195" drill="0.35"/>
<hole x="34.29" y="36.83" drill="0.35"/>
<hole x="34.29" y="37.465" drill="0.35"/>
<hole x="34.29" y="38.1" drill="0.35"/>
<hole x="34.29" y="38.735" drill="0.35"/>
<hole x="34.29" y="39.37" drill="0.35"/>
<hole x="34.29" y="40.005" drill="0.35"/>
<hole x="19.685" y="60.96" drill="0.35"/>
<hole x="20.32" y="60.96" drill="0.35"/>
<hole x="20.955" y="60.96" drill="0.35"/>
<hole x="21.59" y="60.96" drill="0.35"/>
<hole x="22.225" y="60.96" drill="0.35"/>
<hole x="22.86" y="60.96" drill="0.35"/>
<hole x="23.495" y="60.96" drill="0.35"/>
<hole x="24.13" y="60.96" drill="0.35"/>
<hole x="24.765" y="60.96" drill="0.35"/>
<hole x="25.4" y="60.96" drill="0.35"/>
<hole x="26.035" y="60.96" drill="0.35"/>
<hole x="26.67" y="60.96" drill="0.35"/>
<hole x="26.67" y="41.275" drill="0.35"/>
<hole x="26.67" y="41.91" drill="0.35"/>
<hole x="26.67" y="42.545" drill="0.35"/>
<hole x="26.67" y="43.18" drill="0.35"/>
<hole x="26.67" y="43.815" drill="0.35"/>
<hole x="26.67" y="44.45" drill="0.35"/>
<hole x="26.67" y="45.085" drill="0.35"/>
<hole x="26.67" y="45.72" drill="0.35"/>
<hole x="26.67" y="46.355" drill="0.35"/>
<hole x="26.67" y="46.99" drill="0.35"/>
<hole x="26.67" y="47.625" drill="0.35"/>
<hole x="26.67" y="48.26" drill="0.35"/>
<hole x="26.67" y="48.895" drill="0.35"/>
<hole x="26.67" y="49.53" drill="0.35"/>
<hole x="26.67" y="50.165" drill="0.35"/>
<hole x="26.67" y="50.8" drill="0.35"/>
<hole x="26.67" y="51.435" drill="0.35"/>
<hole x="26.67" y="52.07" drill="0.35"/>
<hole x="26.67" y="52.705" drill="0.35"/>
<hole x="26.67" y="53.34" drill="0.35"/>
<hole x="26.67" y="53.975" drill="0.35"/>
<hole x="26.67" y="54.61" drill="0.35"/>
<hole x="26.67" y="55.245" drill="0.35"/>
<hole x="26.67" y="55.88" drill="0.35"/>
<hole x="26.67" y="56.515" drill="0.35"/>
<hole x="26.67" y="57.15" drill="0.35"/>
<hole x="26.67" y="57.785" drill="0.35"/>
<hole x="26.67" y="58.42" drill="0.35"/>
<hole x="26.67" y="59.055" drill="0.35"/>
<hole x="26.67" y="59.69" drill="0.35"/>
<hole x="26.67" y="60.325" drill="0.35"/>
<hole x="27.305" y="60.96" drill="0.35"/>
<hole x="27.94" y="60.96" drill="0.35"/>
<hole x="28.575" y="60.96" drill="0.35"/>
<hole x="29.21" y="60.96" drill="0.35"/>
<hole x="29.845" y="60.96" drill="0.35"/>
<hole x="30.48" y="60.96" drill="0.35"/>
<hole x="31.115" y="60.96" drill="0.35"/>
<hole x="31.75" y="60.96" drill="0.35"/>
<hole x="32.385" y="60.96" drill="0.35"/>
<hole x="33.02" y="60.96" drill="0.35"/>
<hole x="33.655" y="60.96" drill="0.35"/>
<hole x="34.29" y="60.96" drill="0.35"/>
<hole x="34.29" y="41.275" drill="0.35"/>
<hole x="34.29" y="41.91" drill="0.35"/>
<hole x="34.29" y="42.545" drill="0.35"/>
<hole x="34.29" y="43.18" drill="0.35"/>
<hole x="34.29" y="43.815" drill="0.35"/>
<hole x="34.29" y="44.45" drill="0.35"/>
<hole x="34.29" y="45.085" drill="0.35"/>
<hole x="34.29" y="45.72" drill="0.35"/>
<hole x="34.29" y="46.355" drill="0.35"/>
<hole x="34.29" y="46.99" drill="0.35"/>
<hole x="34.29" y="47.625" drill="0.35"/>
<hole x="34.29" y="48.26" drill="0.35"/>
<hole x="34.29" y="48.895" drill="0.35"/>
<hole x="34.29" y="49.53" drill="0.35"/>
<hole x="34.29" y="50.165" drill="0.35"/>
<hole x="34.29" y="50.8" drill="0.35"/>
<hole x="34.29" y="51.435" drill="0.35"/>
<hole x="34.29" y="52.07" drill="0.35"/>
<hole x="34.29" y="52.705" drill="0.35"/>
<hole x="34.29" y="53.34" drill="0.35"/>
<hole x="34.29" y="53.975" drill="0.35"/>
<hole x="34.29" y="54.61" drill="0.35"/>
<hole x="34.29" y="55.245" drill="0.35"/>
<hole x="34.29" y="55.88" drill="0.35"/>
<hole x="34.29" y="56.515" drill="0.35"/>
<hole x="34.29" y="57.15" drill="0.35"/>
<hole x="34.29" y="57.785" drill="0.35"/>
<hole x="34.29" y="58.42" drill="0.35"/>
<hole x="34.29" y="59.055" drill="0.35"/>
<hole x="34.29" y="59.69" drill="0.35"/>
<hole x="34.29" y="60.325" drill="0.35"/>
<hole x="19.685" y="81.28" drill="0.35"/>
<hole x="20.32" y="81.28" drill="0.35"/>
<hole x="20.955" y="81.28" drill="0.35"/>
<hole x="21.59" y="81.28" drill="0.35"/>
<hole x="22.225" y="81.28" drill="0.35"/>
<hole x="22.86" y="81.28" drill="0.35"/>
<hole x="23.495" y="81.28" drill="0.35"/>
<hole x="24.13" y="81.28" drill="0.35"/>
<hole x="24.765" y="81.28" drill="0.35"/>
<hole x="25.4" y="81.28" drill="0.35"/>
<hole x="26.035" y="81.28" drill="0.35"/>
<hole x="26.67" y="81.28" drill="0.35"/>
<hole x="26.67" y="61.595" drill="0.35"/>
<hole x="26.67" y="62.23" drill="0.35"/>
<hole x="26.67" y="62.865" drill="0.35"/>
<hole x="26.67" y="63.5" drill="0.35"/>
<hole x="26.67" y="64.135" drill="0.35"/>
<hole x="26.67" y="64.77" drill="0.35"/>
<hole x="26.67" y="65.405" drill="0.35"/>
<hole x="26.67" y="66.04" drill="0.35"/>
<hole x="26.67" y="66.675" drill="0.35"/>
<hole x="26.67" y="67.31" drill="0.35"/>
<hole x="26.67" y="67.945" drill="0.35"/>
<hole x="26.67" y="68.58" drill="0.35"/>
<hole x="26.67" y="69.215" drill="0.35"/>
<hole x="26.67" y="69.85" drill="0.35"/>
<hole x="26.67" y="70.485" drill="0.35"/>
<hole x="26.67" y="71.12" drill="0.35"/>
<hole x="26.67" y="71.755" drill="0.35"/>
<hole x="26.67" y="72.39" drill="0.35"/>
<hole x="26.67" y="73.025" drill="0.35"/>
<hole x="26.67" y="73.66" drill="0.35"/>
<hole x="26.67" y="74.295" drill="0.35"/>
<hole x="26.67" y="74.93" drill="0.35"/>
<hole x="26.67" y="75.565" drill="0.35"/>
<hole x="26.67" y="76.2" drill="0.35"/>
<hole x="26.67" y="76.835" drill="0.35"/>
<hole x="26.67" y="77.47" drill="0.35"/>
<hole x="26.67" y="78.105" drill="0.35"/>
<hole x="26.67" y="78.74" drill="0.35"/>
<hole x="26.67" y="79.375" drill="0.35"/>
<hole x="26.67" y="80.01" drill="0.35"/>
<hole x="26.67" y="80.645" drill="0.35"/>
<hole x="27.305" y="81.28" drill="0.35"/>
<hole x="27.94" y="81.28" drill="0.35"/>
<hole x="28.575" y="81.28" drill="0.35"/>
<hole x="29.21" y="81.28" drill="0.35"/>
<hole x="29.845" y="81.28" drill="0.35"/>
<hole x="30.48" y="81.28" drill="0.35"/>
<hole x="31.115" y="81.28" drill="0.35"/>
<hole x="31.75" y="81.28" drill="0.35"/>
<hole x="32.385" y="81.28" drill="0.35"/>
<hole x="33.02" y="81.28" drill="0.35"/>
<hole x="33.655" y="81.28" drill="0.35"/>
<hole x="34.29" y="81.28" drill="0.35"/>
<hole x="34.29" y="61.595" drill="0.35"/>
<hole x="34.29" y="62.23" drill="0.35"/>
<hole x="34.29" y="62.865" drill="0.35"/>
<hole x="34.29" y="63.5" drill="0.35"/>
<hole x="34.29" y="64.135" drill="0.35"/>
<hole x="34.29" y="64.77" drill="0.35"/>
<hole x="34.29" y="65.405" drill="0.35"/>
<hole x="34.29" y="66.04" drill="0.35"/>
<hole x="34.29" y="66.675" drill="0.35"/>
<hole x="34.29" y="67.31" drill="0.35"/>
<hole x="34.29" y="67.945" drill="0.35"/>
<hole x="34.29" y="68.58" drill="0.35"/>
<hole x="34.29" y="69.215" drill="0.35"/>
<hole x="34.29" y="69.85" drill="0.35"/>
<hole x="34.29" y="70.485" drill="0.35"/>
<hole x="34.29" y="71.12" drill="0.35"/>
<hole x="34.29" y="71.755" drill="0.35"/>
<hole x="34.29" y="72.39" drill="0.35"/>
<hole x="34.29" y="73.025" drill="0.35"/>
<hole x="34.29" y="73.66" drill="0.35"/>
<hole x="34.29" y="74.295" drill="0.35"/>
<hole x="34.29" y="74.93" drill="0.35"/>
<hole x="34.29" y="75.565" drill="0.35"/>
<hole x="34.29" y="76.2" drill="0.35"/>
<hole x="34.29" y="76.835" drill="0.35"/>
<hole x="34.29" y="77.47" drill="0.35"/>
<hole x="34.29" y="78.105" drill="0.35"/>
<hole x="34.29" y="78.74" drill="0.35"/>
<hole x="34.29" y="79.375" drill="0.35"/>
<hole x="34.29" y="80.01" drill="0.35"/>
<hole x="34.29" y="80.645" drill="0.35"/>
<hole x="3.81" y="81.915" drill="0.35"/>
<hole x="3.81" y="82.55" drill="0.35"/>
<hole x="3.81" y="83.185" drill="0.35"/>
<hole x="3.81" y="83.82" drill="0.35"/>
<hole x="3.81" y="84.455" drill="0.35"/>
<hole x="3.81" y="85.09" drill="0.35"/>
<hole x="3.81" y="85.725" drill="0.35"/>
<hole x="3.81" y="86.36" drill="0.35"/>
<hole x="3.81" y="86.995" drill="0.35"/>
<hole x="3.81" y="87.63" drill="0.35"/>
<hole x="3.81" y="88.265" drill="0.35"/>
<hole x="3.81" y="88.9" drill="0.35"/>
<hole x="3.81" y="89.535" drill="0.35"/>
<hole x="3.81" y="90.17" drill="0.35"/>
<hole x="3.81" y="90.805" drill="0.35"/>
<hole x="3.81" y="91.44" drill="0.35"/>
<hole x="3.81" y="92.075" drill="0.35"/>
<hole x="3.81" y="92.71" drill="0.35"/>
<hole x="3.81" y="93.345" drill="0.35"/>
<hole x="3.81" y="93.98" drill="0.35"/>
<hole x="3.81" y="94.615" drill="0.35"/>
<hole x="3.81" y="95.25" drill="0.35"/>
<hole x="3.81" y="95.885" drill="0.35"/>
<hole x="3.81" y="96.52" drill="0.35"/>
<hole x="3.81" y="97.155" drill="0.35"/>
<hole x="3.81" y="97.79" drill="0.35"/>
<hole x="3.81" y="98.425" drill="0.35"/>
<hole x="3.81" y="99.06" drill="0.35"/>
<hole x="3.81" y="99.695" drill="0.35"/>
<hole x="3.81" y="100.33" drill="0.35"/>
<hole x="3.81" y="100.965" drill="0.35"/>
<hole x="11.43" y="81.915" drill="0.35"/>
<hole x="11.43" y="82.55" drill="0.35"/>
<hole x="11.43" y="83.185" drill="0.35"/>
<hole x="11.43" y="83.82" drill="0.35"/>
<hole x="11.43" y="84.455" drill="0.35"/>
<hole x="11.43" y="85.09" drill="0.35"/>
<hole x="11.43" y="85.725" drill="0.35"/>
<hole x="11.43" y="86.36" drill="0.35"/>
<hole x="11.43" y="86.995" drill="0.35"/>
<hole x="11.43" y="87.63" drill="0.35"/>
<hole x="11.43" y="88.265" drill="0.35"/>
<hole x="11.43" y="88.9" drill="0.35"/>
<hole x="11.43" y="89.535" drill="0.35"/>
<hole x="11.43" y="90.17" drill="0.35"/>
<hole x="11.43" y="90.805" drill="0.35"/>
<hole x="11.43" y="91.44" drill="0.35"/>
<hole x="11.43" y="92.075" drill="0.35"/>
<hole x="11.43" y="92.71" drill="0.35"/>
<hole x="11.43" y="93.345" drill="0.35"/>
<hole x="11.43" y="93.98" drill="0.35"/>
<hole x="11.43" y="94.615" drill="0.35"/>
<hole x="11.43" y="95.25" drill="0.35"/>
<hole x="11.43" y="95.885" drill="0.35"/>
<hole x="11.43" y="96.52" drill="0.35"/>
<hole x="11.43" y="97.155" drill="0.35"/>
<hole x="11.43" y="97.79" drill="0.35"/>
<hole x="11.43" y="98.425" drill="0.35"/>
<hole x="11.43" y="99.06" drill="0.35"/>
<hole x="11.43" y="99.695" drill="0.35"/>
<hole x="11.43" y="100.33" drill="0.35"/>
<hole x="11.43" y="100.965" drill="0.35"/>
<hole x="19.05" y="81.915" drill="0.35"/>
<hole x="19.05" y="82.55" drill="0.35"/>
<hole x="19.05" y="83.185" drill="0.35"/>
<hole x="19.05" y="83.82" drill="0.35"/>
<hole x="19.05" y="84.455" drill="0.35"/>
<hole x="19.05" y="85.09" drill="0.35"/>
<hole x="19.05" y="85.725" drill="0.35"/>
<hole x="19.05" y="86.36" drill="0.35"/>
<hole x="19.05" y="86.995" drill="0.35"/>
<hole x="19.05" y="87.63" drill="0.35"/>
<hole x="19.05" y="88.265" drill="0.35"/>
<hole x="19.05" y="88.9" drill="0.35"/>
<hole x="19.05" y="89.535" drill="0.35"/>
<hole x="19.05" y="90.17" drill="0.35"/>
<hole x="19.05" y="90.805" drill="0.35"/>
<hole x="19.05" y="91.44" drill="0.35"/>
<hole x="19.05" y="92.075" drill="0.35"/>
<hole x="19.05" y="92.71" drill="0.35"/>
<hole x="19.05" y="93.345" drill="0.35"/>
<hole x="19.05" y="93.98" drill="0.35"/>
<hole x="19.05" y="94.615" drill="0.35"/>
<hole x="19.05" y="95.25" drill="0.35"/>
<hole x="19.05" y="95.885" drill="0.35"/>
<hole x="19.05" y="96.52" drill="0.35"/>
<hole x="19.05" y="97.155" drill="0.35"/>
<hole x="19.05" y="97.79" drill="0.35"/>
<hole x="19.05" y="98.425" drill="0.35"/>
<hole x="19.05" y="99.06" drill="0.35"/>
<hole x="19.05" y="99.695" drill="0.35"/>
<hole x="19.05" y="100.33" drill="0.35"/>
<hole x="19.05" y="100.965" drill="0.35"/>
<hole x="26.67" y="81.915" drill="0.35"/>
<hole x="26.67" y="82.55" drill="0.35"/>
<hole x="26.67" y="83.185" drill="0.35"/>
<hole x="26.67" y="83.82" drill="0.35"/>
<hole x="26.67" y="84.455" drill="0.35"/>
<hole x="26.67" y="85.09" drill="0.35"/>
<hole x="26.67" y="85.725" drill="0.35"/>
<hole x="26.67" y="86.36" drill="0.35"/>
<hole x="26.67" y="86.995" drill="0.35"/>
<hole x="26.67" y="87.63" drill="0.35"/>
<hole x="26.67" y="88.265" drill="0.35"/>
<hole x="26.67" y="88.9" drill="0.35"/>
<hole x="26.67" y="89.535" drill="0.35"/>
<hole x="26.67" y="90.17" drill="0.35"/>
<hole x="26.67" y="90.805" drill="0.35"/>
<hole x="26.67" y="91.44" drill="0.35"/>
<hole x="26.67" y="92.075" drill="0.35"/>
<hole x="26.67" y="92.71" drill="0.35"/>
<hole x="26.67" y="93.345" drill="0.35"/>
<hole x="26.67" y="93.98" drill="0.35"/>
<hole x="26.67" y="94.615" drill="0.35"/>
<hole x="26.67" y="95.25" drill="0.35"/>
<hole x="26.67" y="95.885" drill="0.35"/>
<hole x="26.67" y="96.52" drill="0.35"/>
<hole x="26.67" y="97.155" drill="0.35"/>
<hole x="26.67" y="97.79" drill="0.35"/>
<hole x="26.67" y="98.425" drill="0.35"/>
<hole x="26.67" y="99.06" drill="0.35"/>
<hole x="26.67" y="99.695" drill="0.35"/>
<hole x="26.67" y="100.33" drill="0.35"/>
<hole x="26.67" y="100.965" drill="0.35"/>
<hole x="34.29" y="81.915" drill="0.35"/>
<hole x="34.29" y="82.55" drill="0.35"/>
<hole x="34.29" y="83.185" drill="0.35"/>
<hole x="34.29" y="83.82" drill="0.35"/>
<hole x="34.29" y="84.455" drill="0.35"/>
<hole x="34.29" y="85.09" drill="0.35"/>
<hole x="34.29" y="85.725" drill="0.35"/>
<hole x="34.29" y="86.36" drill="0.35"/>
<hole x="34.29" y="86.995" drill="0.35"/>
<hole x="34.29" y="87.63" drill="0.35"/>
<hole x="34.29" y="88.265" drill="0.35"/>
<hole x="34.29" y="88.9" drill="0.35"/>
<hole x="34.29" y="89.535" drill="0.35"/>
<hole x="34.29" y="90.17" drill="0.35"/>
<hole x="34.29" y="90.805" drill="0.35"/>
<hole x="34.29" y="91.44" drill="0.35"/>
<hole x="34.29" y="92.075" drill="0.35"/>
<hole x="34.29" y="92.71" drill="0.35"/>
<hole x="34.29" y="93.345" drill="0.35"/>
<hole x="34.29" y="93.98" drill="0.35"/>
<hole x="34.29" y="94.615" drill="0.35"/>
<hole x="34.29" y="95.25" drill="0.35"/>
<hole x="34.29" y="95.885" drill="0.35"/>
<hole x="34.29" y="96.52" drill="0.35"/>
<hole x="34.29" y="97.155" drill="0.35"/>
<hole x="34.29" y="97.79" drill="0.35"/>
<hole x="34.29" y="98.425" drill="0.35"/>
<hole x="34.29" y="99.06" drill="0.35"/>
<hole x="34.29" y="99.695" drill="0.35"/>
<hole x="34.29" y="100.33" drill="0.35"/>
<hole x="34.29" y="100.965" drill="0.35"/>
<hole x="0.508" y="10.16" drill="0.35"/>
<hole x="1.143" y="10.16" drill="0.35"/>
<hole x="1.778" y="10.16" drill="0.35"/>
<hole x="2.413" y="10.16" drill="0.35"/>
<hole x="3.175" y="10.16" drill="0.35"/>
<hole x="0.508" y="20.32" drill="0.35"/>
<hole x="1.143" y="20.32" drill="0.35"/>
<hole x="1.778" y="20.32" drill="0.35"/>
<hole x="2.413" y="20.32" drill="0.35"/>
<hole x="3.175" y="20.32" drill="0.35"/>
<hole x="0.508" y="30.48" drill="0.35"/>
<hole x="1.143" y="30.48" drill="0.35"/>
<hole x="1.778" y="30.48" drill="0.35"/>
<hole x="2.413" y="30.48" drill="0.35"/>
<hole x="3.175" y="30.48" drill="0.35"/>
<hole x="0.508" y="40.64" drill="0.35"/>
<hole x="1.143" y="40.64" drill="0.35"/>
<hole x="1.778" y="40.64" drill="0.35"/>
<hole x="2.413" y="40.64" drill="0.35"/>
<hole x="3.175" y="40.64" drill="0.35"/>
<hole x="0.508" y="50.8" drill="0.35"/>
<hole x="1.143" y="50.8" drill="0.35"/>
<hole x="1.778" y="50.8" drill="0.35"/>
<hole x="2.413" y="50.8" drill="0.35"/>
<hole x="3.175" y="50.8" drill="0.35"/>
<hole x="0.508" y="60.96" drill="0.35"/>
<hole x="1.143" y="60.96" drill="0.35"/>
<hole x="1.778" y="60.96" drill="0.35"/>
<hole x="2.413" y="60.96" drill="0.35"/>
<hole x="3.175" y="60.96" drill="0.35"/>
<hole x="0.508" y="71.12" drill="0.35"/>
<hole x="1.143" y="71.12" drill="0.35"/>
<hole x="1.778" y="71.12" drill="0.35"/>
<hole x="2.413" y="71.12" drill="0.35"/>
<hole x="3.175" y="71.12" drill="0.35"/>
<hole x="0.508" y="81.28" drill="0.35"/>
<hole x="1.143" y="81.28" drill="0.35"/>
<hole x="1.778" y="81.28" drill="0.35"/>
<hole x="2.413" y="81.28" drill="0.35"/>
<hole x="3.175" y="81.28" drill="0.35"/>
<hole x="0.508" y="91.44" drill="0.35"/>
<hole x="1.143" y="91.44" drill="0.35"/>
<hole x="1.778" y="91.44" drill="0.35"/>
<hole x="2.413" y="91.44" drill="0.35"/>
<hole x="3.175" y="91.44" drill="0.35"/>
<hole x="35.052" y="91.44" drill="0.35"/>
<hole x="35.687" y="91.44" drill="0.35"/>
<hole x="36.322" y="91.44" drill="0.35"/>
<hole x="36.957" y="91.44" drill="0.35"/>
<hole x="37.719" y="91.44" drill="0.35"/>
<hole x="35.052" y="81.28" drill="0.35"/>
<hole x="35.687" y="81.28" drill="0.35"/>
<hole x="36.322" y="81.28" drill="0.35"/>
<hole x="36.957" y="81.28" drill="0.35"/>
<hole x="37.719" y="81.28" drill="0.35"/>
<hole x="35.052" y="71.12" drill="0.35"/>
<hole x="35.687" y="71.12" drill="0.35"/>
<hole x="36.322" y="71.12" drill="0.35"/>
<hole x="36.957" y="71.12" drill="0.35"/>
<hole x="37.719" y="71.12" drill="0.35"/>
<hole x="35.052" y="60.96" drill="0.35"/>
<hole x="35.687" y="60.96" drill="0.35"/>
<hole x="36.322" y="60.96" drill="0.35"/>
<hole x="36.957" y="60.96" drill="0.35"/>
<hole x="37.719" y="60.96" drill="0.35"/>
<hole x="35.052" y="50.8" drill="0.35"/>
<hole x="35.687" y="50.8" drill="0.35"/>
<hole x="36.322" y="50.8" drill="0.35"/>
<hole x="36.957" y="50.8" drill="0.35"/>
<hole x="37.719" y="50.8" drill="0.35"/>
<hole x="35.052" y="40.64" drill="0.35"/>
<hole x="35.687" y="40.64" drill="0.35"/>
<hole x="36.322" y="40.64" drill="0.35"/>
<hole x="36.957" y="40.64" drill="0.35"/>
<hole x="37.719" y="40.64" drill="0.35"/>
<hole x="35.052" y="30.48" drill="0.35"/>
<hole x="35.687" y="30.48" drill="0.35"/>
<hole x="36.322" y="30.48" drill="0.35"/>
<hole x="36.957" y="30.48" drill="0.35"/>
<hole x="37.719" y="30.48" drill="0.35"/>
<hole x="35.052" y="20.32" drill="0.35"/>
<hole x="35.687" y="20.32" drill="0.35"/>
<hole x="36.322" y="20.32" drill="0.35"/>
<hole x="36.957" y="20.32" drill="0.35"/>
<hole x="37.719" y="20.32" drill="0.35"/>
<hole x="35.052" y="10.16" drill="0.35"/>
<hole x="35.687" y="10.16" drill="0.35"/>
<hole x="36.322" y="10.16" drill="0.35"/>
<hole x="36.957" y="10.16" drill="0.35"/>
<hole x="37.719" y="10.16" drill="0.35"/>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>MUSSEL
HEATER</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>NTC</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>LP MILLER
2020</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
<text>RevA</text>
</plain>
<libraries>
<library name="miller">
<packages>
<package name="1X01_SMALL_0.7">
<description>Very small 1-pin terminal&lt;br&gt;
0.7mm (0.0279") drill diameter&lt;br&gt;
1.0566mm (0. 0416") terminal diameter</description>
</package>
<package name="1X01_SMALL">
<description>0.035" (0.89 mm) diameter drill, 0.055" (1.397mm) copper diameter&lt;br&gt;
This hole should be barely large enough for standard 0.1" pitch header pins.</description>
</package>
<package name="R0603_THERMISTOR">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GND_HEAT1" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT1" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM1" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM1" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME1" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL">
<attribute name="VALUE"/>
</element>
<element name="GND_NICHROME1" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL">
<attribute name="VALUE"/>
</element>
<element name="THERM1" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT2" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT2" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM2" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM2" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME2" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME2" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM2" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT3" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT3" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM3" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM3" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME3" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME3" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM3" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT4" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT4" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM4" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM4" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME4" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME4" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM4" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT5" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT5" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM5" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM5" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME5" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME5" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM5" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT6" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT6" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM6" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM6" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME6" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME6" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM6" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT7" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT7" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM7" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM7" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME7" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME7" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM7" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT8" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT8" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM8" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM8" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME8" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME8" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM8" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT9" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT9" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM9" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM9" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME9" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME9" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM9" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT10" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT10" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM10" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM10" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME10" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME10" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM10" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT11" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT11" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM11" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM11" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME11" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME11" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM11" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT12" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT12" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM12" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM12" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME12" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME12" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM12" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT13" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT13" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM13" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM13" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME13" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME13" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM13" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT14" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT14" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM14" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM14" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME14" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME14" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM14" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT15" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT15" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="U$30" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM15" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME15" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME15" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM15" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT16" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT16" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM16" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM16" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME16" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME16" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM16" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT17" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT17" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM17" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM17" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME17" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME17" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM17" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT18" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT18" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM18" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM18" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME18" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME18" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM18" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT19" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT19" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM19" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM19" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME19" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME19" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM19" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
<element name="GND_HEAT20" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_HEAT20" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="GND_THERM20" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VCC_THERM20" library="miller" package="1X01_SMALL" value="PINHD-1X1SMALL">
<attribute name="VALUE"/>
</element>
<element name="VRAW_NICHROME20" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="GND_NICHROME20" library="miller" package="1X01_SMALL_0.7" value="PINHD-1X10.7MM_DRILL"/>
<element name="THERM20" library="miller" package="R0603_THERMISTOR" value="10K_NTC">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC_THERM1">
<contactref element="VCC_THERM1" pad="1"/>
<contactref element="THERM1" pad="2"/>
</signal>
<signal name="GND_THERM1">
<contactref element="GND_THERM1" pad="1"/>
<contactref element="THERM1" pad="1"/>
</signal>
<signal name="GND_THERM2">
<contactref element="GND_THERM2" pad="1"/>
<contactref element="THERM2" pad="1"/>
</signal>
<signal name="VCC_THERM2">
<contactref element="VCC_THERM2" pad="1"/>
<contactref element="THERM2" pad="2"/>
</signal>
<signal name="GND_HEAT3">
<contactref element="GND_NICHROME3" pad="P$1"/>
<contactref element="GND_HEAT3" pad="1"/>
</signal>
<signal name="VRAW_HEAT3">
<contactref element="VRAW_NICHROME3" pad="P$1"/>
<contactref element="VRAW_HEAT3" pad="1"/>
</signal>
<signal name="GND_THERM3">
<contactref element="GND_THERM3" pad="1"/>
<contactref element="THERM3" pad="1"/>
</signal>
<signal name="VCC_THERM3">
<contactref element="VCC_THERM3" pad="1"/>
<contactref element="THERM3" pad="2"/>
</signal>
<signal name="GND_HEAT2">
<contactref element="GND_NICHROME2" pad="P$1"/>
<contactref element="GND_HEAT2" pad="1"/>
</signal>
<signal name="VRAW_HEAT2">
<contactref element="VRAW_NICHROME2" pad="P$1"/>
<contactref element="VRAW_HEAT2" pad="1"/>
</signal>
<signal name="GND_HEAT1">
<contactref element="GND_NICHROME1" pad="P$1"/>
<contactref element="GND_HEAT1" pad="1"/>
</signal>
<signal name="VRAW_HEAT1">
<contactref element="VRAW_NICHROME1" pad="P$1"/>
<contactref element="VRAW_HEAT1" pad="1"/>
</signal>
<signal name="VRAW_HEAT4">
<contactref element="VRAW_HEAT4" pad="1"/>
<contactref element="VRAW_NICHROME4" pad="P$1"/>
</signal>
<signal name="GND_HEAT4">
<contactref element="GND_HEAT4" pad="1"/>
<contactref element="GND_NICHROME4" pad="P$1"/>
</signal>
<signal name="GND_THERM4">
<contactref element="GND_THERM4" pad="1"/>
<contactref element="THERM4" pad="1"/>
</signal>
<signal name="VCC_THERM4">
<contactref element="VCC_THERM4" pad="1"/>
<contactref element="THERM4" pad="2"/>
</signal>
<signal name="VRAW_HEAT5">
<contactref element="VRAW_HEAT5" pad="1"/>
<contactref element="VRAW_NICHROME5" pad="P$1"/>
</signal>
<signal name="GND_HEAT5">
<contactref element="GND_HEAT5" pad="1"/>
<contactref element="GND_NICHROME5" pad="P$1"/>
</signal>
<signal name="GND_THERM5">
<contactref element="GND_THERM5" pad="1"/>
<contactref element="THERM5" pad="1"/>
</signal>
<signal name="VCC_THERM5">
<contactref element="VCC_THERM5" pad="1"/>
<contactref element="THERM5" pad="2"/>
</signal>
<signal name="VRAW_HEAT6">
<contactref element="VRAW_HEAT6" pad="1"/>
<contactref element="VRAW_NICHROME6" pad="P$1"/>
</signal>
<signal name="GND_HEAT6">
<contactref element="GND_HEAT6" pad="1"/>
<contactref element="GND_NICHROME6" pad="P$1"/>
</signal>
<signal name="VRAW_HEAT7">
<contactref element="VRAW_HEAT7" pad="1"/>
<contactref element="VRAW_NICHROME7" pad="P$1"/>
</signal>
<signal name="GND_HEAT7">
<contactref element="GND_HEAT7" pad="1"/>
<contactref element="GND_NICHROME7" pad="P$1"/>
</signal>
<signal name="GND_THERM7">
<contactref element="GND_THERM7" pad="1"/>
<contactref element="THERM7" pad="1"/>
</signal>
<signal name="VCC_THERM7">
<contactref element="VCC_THERM7" pad="1"/>
<contactref element="THERM7" pad="2"/>
</signal>
<signal name="VRAW_HEAT8">
<contactref element="VRAW_HEAT8" pad="1"/>
<contactref element="VRAW_NICHROME8" pad="P$1"/>
</signal>
<signal name="GND_HEAT8">
<contactref element="GND_HEAT8" pad="1"/>
<contactref element="GND_NICHROME8" pad="P$1"/>
</signal>
<signal name="GND_THERM8">
<contactref element="GND_THERM8" pad="1"/>
<contactref element="THERM8" pad="1"/>
</signal>
<signal name="VCC_THERM8">
<contactref element="VCC_THERM8" pad="1"/>
<contactref element="THERM8" pad="2"/>
</signal>
<signal name="VCC_THERM6">
<contactref element="VCC_THERM6" pad="1"/>
<contactref element="THERM6" pad="2"/>
</signal>
<signal name="GND_THERM6">
<contactref element="GND_THERM6" pad="1"/>
<contactref element="THERM6" pad="1"/>
</signal>
<signal name="GND_THERM12">
<contactref element="GND_THERM12" pad="1"/>
<contactref element="THERM12" pad="1"/>
</signal>
<signal name="VCC_THERM12">
<contactref element="VCC_THERM12" pad="1"/>
<contactref element="THERM12" pad="2"/>
</signal>
<signal name="GND_HEAT12">
<contactref element="GND_NICHROME12" pad="P$1"/>
<contactref element="GND_HEAT12" pad="1"/>
</signal>
<signal name="VRAW_HEAT12">
<contactref element="VRAW_NICHROME12" pad="P$1"/>
<contactref element="VRAW_HEAT12" pad="1"/>
</signal>
<signal name="GND_THERM11">
<contactref element="GND_THERM11" pad="1"/>
<contactref element="THERM11" pad="1"/>
</signal>
<signal name="VCC_THERM11">
<contactref element="VCC_THERM11" pad="1"/>
<contactref element="THERM11" pad="2"/>
</signal>
<signal name="GND_HEAT11">
<contactref element="GND_NICHROME11" pad="P$1"/>
<contactref element="GND_HEAT11" pad="1"/>
</signal>
<signal name="VRAW_HEAT11">
<contactref element="VRAW_NICHROME11" pad="P$1"/>
<contactref element="VRAW_HEAT11" pad="1"/>
</signal>
<signal name="GND_THERM10">
<contactref element="GND_THERM10" pad="1"/>
<contactref element="THERM10" pad="1"/>
</signal>
<signal name="VCC_THERM10">
<contactref element="VCC_THERM10" pad="1"/>
<contactref element="THERM10" pad="2"/>
</signal>
<signal name="GND_HEAT10">
<contactref element="GND_NICHROME10" pad="P$1"/>
<contactref element="GND_HEAT10" pad="1"/>
</signal>
<signal name="VRAW_HEAT10">
<contactref element="VRAW_NICHROME10" pad="P$1"/>
<contactref element="VRAW_HEAT10" pad="1"/>
</signal>
<signal name="GND_THERM9">
<contactref element="GND_THERM9" pad="1"/>
<contactref element="THERM9" pad="1"/>
</signal>
<signal name="VCC_THERM9">
<contactref element="VCC_THERM9" pad="1"/>
<contactref element="THERM9" pad="2"/>
</signal>
<signal name="GND_HEAT9">
<contactref element="GND_NICHROME9" pad="P$1"/>
<contactref element="GND_HEAT9" pad="1"/>
</signal>
<signal name="VRAW_HEAT9">
<contactref element="VRAW_NICHROME9" pad="P$1"/>
<contactref element="VRAW_HEAT9" pad="1"/>
</signal>
<signal name="VRAW_HEAT13">
<contactref element="VRAW_HEAT13" pad="1"/>
<contactref element="VRAW_NICHROME13" pad="P$1"/>
</signal>
<signal name="GND_HEAT13">
<contactref element="GND_HEAT13" pad="1"/>
<contactref element="GND_NICHROME13" pad="P$1"/>
</signal>
<signal name="GND_THERM13">
<contactref element="GND_THERM13" pad="1"/>
<contactref element="THERM13" pad="1"/>
</signal>
<signal name="VCC_THERM13">
<contactref element="VCC_THERM13" pad="1"/>
<contactref element="THERM13" pad="2"/>
</signal>
<signal name="VRAW_HEAT14">
<contactref element="VRAW_HEAT14" pad="1"/>
<contactref element="VRAW_NICHROME14" pad="P$1"/>
</signal>
<signal name="GND_HEAT14">
<contactref element="GND_HEAT14" pad="1"/>
<contactref element="GND_NICHROME14" pad="P$1"/>
</signal>
<signal name="GND_THERM14">
<contactref element="GND_THERM14" pad="1"/>
<contactref element="THERM14" pad="1"/>
</signal>
<signal name="VCC_THERM14">
<contactref element="VCC_THERM14" pad="1"/>
<contactref element="THERM14" pad="2"/>
</signal>
<signal name="VRAW_HEAT15">
<contactref element="VRAW_HEAT15" pad="1"/>
<contactref element="VRAW_NICHROME15" pad="P$1"/>
</signal>
<signal name="GND_HEAT15">
<contactref element="GND_HEAT15" pad="1"/>
<contactref element="GND_NICHROME15" pad="P$1"/>
</signal>
<signal name="VRAW_HEAT16">
<contactref element="VRAW_HEAT16" pad="1"/>
<contactref element="VRAW_NICHROME16" pad="P$1"/>
</signal>
<signal name="GND_HEAT16">
<contactref element="GND_HEAT16" pad="1"/>
<contactref element="GND_NICHROME16" pad="P$1"/>
</signal>
<signal name="GND_THERM16">
<contactref element="GND_THERM16" pad="1"/>
<contactref element="THERM16" pad="1"/>
</signal>
<signal name="VCC_THERM16">
<contactref element="VCC_THERM16" pad="1"/>
<contactref element="THERM16" pad="2"/>
</signal>
<signal name="VCC_THERM15">
<contactref element="VCC_THERM15" pad="1"/>
<contactref element="THERM15" pad="2"/>
</signal>
<signal name="GND_THERM15">
<contactref element="U$30" pad="1"/>
<contactref element="THERM15" pad="1"/>
</signal>
<signal name="VRAW_HEAT17">
<contactref element="VRAW_HEAT17" pad="1"/>
<contactref element="VRAW_NICHROME17" pad="P$1"/>
</signal>
<signal name="GND_HEAT17">
<contactref element="GND_HEAT17" pad="1"/>
<contactref element="GND_NICHROME17" pad="P$1"/>
</signal>
<signal name="GND_THERM17">
<contactref element="GND_THERM17" pad="1"/>
<contactref element="THERM17" pad="1"/>
</signal>
<signal name="VCC_THERM17">
<contactref element="VCC_THERM17" pad="1"/>
<contactref element="THERM17" pad="2"/>
</signal>
<signal name="VRAW_HEAT18">
<contactref element="VRAW_HEAT18" pad="1"/>
<contactref element="VRAW_NICHROME18" pad="P$1"/>
</signal>
<signal name="GND_HEAT18">
<contactref element="GND_HEAT18" pad="1"/>
<contactref element="GND_NICHROME18" pad="P$1"/>
</signal>
<signal name="GND_HEAT19">
<contactref element="GND_HEAT19" pad="1"/>
<contactref element="GND_NICHROME19" pad="P$1"/>
</signal>
<signal name="VRAW_HEAT19">
<contactref element="VRAW_HEAT19" pad="1"/>
<contactref element="VRAW_NICHROME19" pad="P$1"/>
</signal>
<signal name="GND_THERM18">
<contactref element="GND_THERM18" pad="1"/>
<contactref element="THERM18" pad="1"/>
</signal>
<signal name="VCC_THERM18">
<contactref element="VCC_THERM18" pad="1"/>
<contactref element="THERM18" pad="2"/>
</signal>
<signal name="GND_THERM19">
<contactref element="GND_THERM19" pad="1"/>
<contactref element="THERM19" pad="1"/>
</signal>
<signal name="VCC_THERM19">
<contactref element="VCC_THERM19" pad="1"/>
<contactref element="THERM19" pad="2"/>
</signal>
<signal name="VRAW_HEAT20">
<contactref element="VRAW_HEAT20" pad="1"/>
<contactref element="VRAW_NICHROME20" pad="P$1"/>
</signal>
<signal name="GND_HEAT20">
<contactref element="GND_HEAT20" pad="1"/>
<contactref element="GND_NICHROME20" pad="P$1"/>
</signal>
<signal name="GND_THERM20">
<contactref element="GND_THERM20" pad="1"/>
<contactref element="THERM20" pad="1"/>
</signal>
<signal name="VCC_THERM20">
<contactref element="VCC_THERM20" pad="1"/>
<contactref element="THERM20" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
