(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 64)
    (no_connects 0)
    (area 114.949999 126.9226 176.9274 152.9274)
    (thickness 1.6)
    (drawings 7)
    (tracks 367)
    (zones 0)
    (modules 46)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 10)
    (pad_drill 1.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 "Net-(C5-Pad1)")
  (net 2 "Net-(C5-Pad2)")
  (net 3 "Net-(P2-Pad2)")
  (net 4 "Net-(P2-Pad3)")
  (net 5 "Net-(P3-Pad1)")
  (net 6 "Net-(P3-Pad2)")
  (net 7 "Net-(R5-Pad2)")
  (net 8 "Net-(SW2-Pad2)")
  (net 9 "Net-(U1-Pad2)")
  (net 10 "Net-(U3-Pad2)")
  (net 11 +BATT)
  (net 12 GND)
  (net 13 +3V3)
  (net 14 +5V)
  (net 15 /MODECOM)
  (net 16 "Net-(GS2-Pad1)")
  (net 17 /RST)
  (net 18 /GPIO2)
  (net 19 /CH_PD)
  (net 20 /GPIO15)
  (net 21 "Net-(D1-Pad1)")
  (net 22 /GPIO0)
  (net 23 /GPIO4)
  (net 24 /GPIO5)
  (net 25 "Net-(U3-Pad9)")
  (net 26 "Net-(U3-Pad10)")
  (net 27 "Net-(U3-Pad11)")
  (net 28 "Net-(U3-Pad12)")
  (net 29 "Net-(U3-Pad13)")
  (net 30 "Net-(U3-Pad14)")
  (net 31 "Net-(U3-Pad6)")
  (net 32 "Net-(GS3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net /CH_PD)
    (add_net /GPIO0)
    (add_net /GPIO15)
    (add_net /GPIO2)
    (add_net /GPIO4)
    (add_net /GPIO5)
    (add_net /MODECOM)
    (add_net /RST)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(GS2-Pad1)")
    (add_net "Net-(GS3-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(SW2-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 579DC687)
    (at 166 147.5 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference "+ Batt" (at 4.5 1 270) (layer F.SilkS))
    (fp_text value "+ Batt" (at 4.5 1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Switch_SP3T (layer F.Cu) (tedit 579DC9FC)
    (at 154.5 148)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference "prog    run" (at 0 -3) (layer F.SilkS))
    (fp_text value "prog    run" (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at -3 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -1.5 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW2-Pad2)"))
    (pad 3 smd rect (at 1.5 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /GPIO0))
    (pad 4 smd rect (at 3 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R5-Pad2)"))
    (pad "" smd rect (at -5.15 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 5.15 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 5.15 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -5.15 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module custom_footprints:ESP-12E (layer F.Cu) (tedit 579B4571)
    (at 116.25 148 90)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U3 (at 8.5 4 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1 90) (layer F.SilkS))
    (pad 9 smd oval (at 2.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad9)"))
    (pad 10 smd oval (at 4.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad10)"))
    (pad 11 smd oval (at 6.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad11)"))
    (pad 12 smd oval (at 8.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U3-Pad12)"))
    (pad 13 smd oval (at 10.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad13)"))
    (pad 14 smd oval (at 12.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U3-Pad14)"))
    (pad 1 smd rect (at 0 0 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 /RST))
    (pad 2 smd oval (at 0 2 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U3-Pad2)"))
    (pad 3 smd oval (at 0 4 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 /CH_PD))
    (pad 4 smd oval (at 0 6 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(GS2-Pad1)"))
    (pad 5 smd oval (at 0 8 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P3-Pad1)"))
    (pad 6 smd oval (at 0 10 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U3-Pad6)"))
    (pad 7 smd oval (at 0 12 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad2)"))
    (pad 8 smd oval (at 0 14 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 15 smd oval (at 16 14 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 16 smd oval (at 16 12 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 20 /GPIO15))
    (pad 17 smd oval (at 16 10 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO2))
    (pad 18 smd oval (at 16 8 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 22 /GPIO0))
    (pad 19 smd oval (at 16 6 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 /GPIO4))
    (pad 20 smd oval (at 16 4 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 /GPIO5))
    (pad 21 smd oval (at 16 2 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P2-Pad2)"))
    (pad 22 smd oval (at 16 0 90) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P2-Pad3)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579DC69C)
    (at 164.5 144.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.5 0) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 +BATT))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579DCC5F)
    (at 147 135.5 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.5 -1.5 90) (layer F.SilkS))
    (fp_text value 2.2uF (at -1.5 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579DCC6D)
    (at 150.5 135.5 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 1.5 1.5 90) (layer F.SilkS))
    (fp_text value 1uF (at -1 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579DCC9A)
    (at 164.5 135.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at -4.5 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 579DCC89)
    (at 164.5 142 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 579DC6FD)
    (at 148.5 140 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 2 1.5 180) (layer F.SilkS))
    (fp_text value Red (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GS3 (layer F.Cu) (tedit 579DC668)
    (at 171 147.5 90)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference Mode (at -1.5 0 180) (layer F.SilkS))
    (fp_text value Mode (at -1.5 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -1.27 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 0 0 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 15 /MODECOM))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
  )
  (module GS2 (layer F.Cu) (tedit 579DC6D5)
    (at 134 148 90)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference wake (at 1.5 0 180) (layer F.SilkS))
    (fp_text value wake (at 1.524 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(GS2-Pad1)"))
    (pad 2 smd rect (at 0 0.635 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 17 /RST))
  )
  (module GS2 (layer F.Cu) (tedit 579DC660)
    (at 172.5 132)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference com (at -1.5 0 90) (layer F.SilkS))
    (fp_text value com (at -1.5 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 24 /GPIO5))
    (pad 2 smd rect (at 0 0.635) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(GS3-Pad2)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 579DC7DA)
    (at 168 132.5 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference "Serial T R G" (at 11.5 0.5 180) (layer F.SilkS))
    (fp_text value "Serial T R G" (at 11.5 0.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P2-Pad3)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module custom_footprints:10pins_0.5mm_PITCH_connector_FPC (layer F.Cu) (tedit 579DC655)
    (at 172.5 140 180)
    (tags 10_FPC_0.5)
    (attr smd)
    (fp_text reference LCD (at 3.5 1.5 270) (layer F.SilkS))
    (fp_text value Sharp_Memory_LCD (at -3.5 -0.5 270) (layer F.Fab))
    (pad "" smd rect (at -1.5 4 180) (size 1.5 1.5) (drill (offset 0.25 0.25)) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1.75 -2 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 1.75 -1.5 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad2)"))
    (pad 3 smd rect (at 1.75 -1 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 /GPIO4))
    (pad 4 smd rect (at 1.75 -0.5 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(GS3-Pad2)"))
    (pad 5 smd rect (at 1.75 0 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 6 smd rect (at 1.75 0.5 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 7 smd rect (at 1.75 1 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 8 smd rect (at 1.75 1.5 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /MODECOM))
    (pad 9 smd rect (at 1.75 2 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 10 smd rect (at 1.75 2.5 180) (size 1.5 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad "" smd rect (at -1.5 -4 180) (size 1.5 1.5) (drill (offset 0.25 0.25)) (layers F.Cu F.Paste F.Mask))
    (model Housings_SSOP.3dshapes/TSSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 579DCC46)
    (at 139 137 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.5 -1.5 90) (layer F.SilkS))
    (fp_text value 10K (at -1 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 579DCC50)
    (at 139 143.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1 -1.5 90) (layer F.SilkS))
    (fp_text value 10K (at 1.5 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 579DCC4B)
    (at 136 143.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1 -1.5 90) (layer F.SilkS))
    (fp_text value 10K (at 1.5 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /CH_PD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 579DCC40)
    (at 136 137 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.5 -1.5 90) (layer F.SilkS))
    (fp_text value 10K (at -1 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /GPIO15))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 579DCC67)
    (at 148 143.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.5 -1.5) (layer F.SilkS))
    (fp_text value 1K (at 1 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 579DC76A)
    (at 143 140 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference reset (at 0.01011 -2.60022 90) (layer F.SilkS))
    (fp_text value Reset (at 0.01011 -0.00022 90) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 90) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /RST))
    (pad 2 smd rect (at 4.60243 0.00232 90) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module custom_footprints:SOT-223-5 (layer F.Cu) (tedit 579B4104)
    (at 156 138)
    (descr "module CMS SOT223 5 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value LP38692 (at 0 0.5) (layer F.Fab))
    (pad 4 smd rect (at 2.25 3) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 11 +BATT))
    (pad 5 smd rect (at 0 -4) (size 3.3 2) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -0.75 3) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at 0.75 3) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at -2.25 3) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 11 +BATT))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 579DCC82)
    (at 164.5 138.5 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at 0 2.5 270) (layer F.SilkS))
    (fp_text value REG710 (at 0 -0.5 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 +5V))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C5-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAE4)
    (at 119.888 144.272)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 16 (at 0 2) (layer B.SilkS))
    (fp_text value G16 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 16 "Net-(GS2-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAA1)
    (at 129.032 135.636)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 15 (at -0.032 -1.636) (layer B.SilkS))
    (fp_text value G15 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 /GPIO15))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAAD)
    (at 125.984 138.43)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 10 (at 2.016 0.07) (layer B.SilkS))
    (fp_text value G10 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 28 "Net-(U3-Pad12)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCABE)
    (at 125.984 141.478)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 9 (at 1.516 0.022) (layer B.SilkS))
    (fp_text value G9 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 27 "Net-(U3-Pad11)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCA9A)
    (at 125.984 135.636)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 2 (at 0.016 -1.636) (layer B.SilkS))
    (fp_text value G2 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 18 /GPIO2))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCA93)
    (at 122.936 135.636)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 0 (at 0.064 -1.636) (layer B.SilkS))
    (fp_text value G0 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 /GPIO0))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCA8D)
    (at 119.888 135.636)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 4 (at 0.112 -1.636) (layer B.SilkS))
    (fp_text value G4 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 /GPIO4))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCB02)
    (at 129.032 144.272)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 13 (at 0 2) (layer B.SilkS))
    (fp_text value G13 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 6 "Net-(P3-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAF0)
    (at 122.936 144.272)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 14 (at 0 2) (layer B.SilkS))
    (fp_text value G14 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 5 "Net-(P3-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCA86)
    (at 116.84 135.636)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 5 (at 0.16 -1.636) (layer B.SilkS))
    (fp_text value G5 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 24 /GPIO5))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAC6)
    (at 118 140)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference rst (at 2 0) (layer B.SilkS))
    (fp_text value RST (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 17 /RST))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAD3)
    (at 116.84 144.272)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference adc (at 0 2) (layer B.SilkS))
    (fp_text value ADC (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 10 "Net-(U3-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 579DCAF7)
    (at 125.984 144.272)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference 12 (at 0 2) (layer B.SilkS))
    (fp_text value G12 (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 31 "Net-(U3-Pad6)"))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 138 131)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 140 131)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 142 131)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 144 131)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 146 131)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 146 149)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 144 149)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 142 149)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 140 149)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:BoardSolderSquare (layer F.Cu) (tedit 579DC233)
    (at 138 149)
    (descr "2.8mm x 2.8mm, Drill 1.5mm,")
    (attr virtual)
    (fp_text reference "" (at 0 -3) (layer F.SilkS))
    (fp_text value "" (at 0 3) (layer F.Fab) hide)
    (pad "" thru_hole rect (at 0 0) (size 1.8 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module custom_footprints:LOGO (layer B.Cu) (tedit 579DF455)
    (at 161 140)
    (fp_text reference "" (at -7.5 1) (layer B.SilkS) hide)
    (fp_text value LOGO (at -10.5 5) (layer B.SilkS) hide)
  )
  (gr_text pierremuth.wordpress.com (at 147.5 135) (layer B.SilkS))
  (gr_text "ESP Memory LCD" (at 145.5 140) (layer B.SilkS))
  (gr_line (start 175 150) (end 115 150) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175 130) (end 115 130) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175 150) (end 175 130) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115 130) (end 115 150) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 174.5 130.5) (xy 115.5 130.5) (xy 115.5 149.5) (xy 174.5 149.5)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.254))
    (polygon
      (pts
        (xy 174.5 130.5) (xy 115.5 130.5) (xy 115.5 149.5) (xy 174.5 149.5)
      )
    )
  )
)
