<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="13.97" y1="0" x2="13.97" y2="5.9944" width="0.1524" layer="20"/>
<wire x1="13.97" y1="5.9944" x2="17.145" y2="5.9944" width="0.1524" layer="20"/>
<wire x1="17.145" y1="5.9944" x2="17.145" y2="20.32" width="0.1524" layer="20"/>
<text>12V</text>
<text>RV-Project.Com  LED Light Switch-T2</text>
<text>B</text>
<text>12V</text>
<text>12V</text>
<text>A</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<wire x1="13.97" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="44.45" x2="13.97" y2="44.45" width="0.1524" layer="20"/>
<text>To Light</text>
<text>Supply</text>
<wire x1="14.0208" y1="20.32" x2="14.0716" y2="25.4" width="0.1524" layer="20" curve="-180"/>
<wire x1="13.97" y1="20.32" x2="14.0208" y2="20.32" width="0.1524" layer="20"/>
<wire x1="14.0208" y1="20.32" x2="17.145" y2="20.32" width="0.1524" layer="20"/>
<wire x1="13.97" y1="25.4" x2="14.0716" y2="25.4" width="0.1524" layer="20"/>
<wire x1="14.0716" y1="25.4" x2="17.145" y2="25.4" width="0.1524" layer="20"/>
<wire x1="13.97" y1="44.45" x2="13.97" y2="39.37" width="0.1524" layer="20"/>
<wire x1="13.97" y1="39.37" x2="17.145" y2="39.37" width="0.1524" layer="20"/>
<wire x1="17.145" y1="39.37" x2="17.145" y2="25.4" width="0.1524" layer="20"/>
<text>V1.0    1/30/2019</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="MO1-18AWG">
</package>
<package name="A659">
</package>
<package name="WAFER2PINVERTICAL">
</package>
<package name="KEYSTONE_TAB_TOP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP3" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP4" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="JP1" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
<element name="SW1" library="a-lib" package="A659" value=""/>
<element name="J1" library="a-lib" package="WAFER2PINVERTICAL" value="WAFER2PVERTICAL"/>
<element name="TAB1" library="a-lib" package="KEYSTONE_TAB_TOP" value="">
<attribute name="HOLE" value="0.13 Dia"/>
<attribute name="ORIENTATION" value="SIDE"/>
<attribute name="PARTNUM" value="612"/>
<attribute name="THREAD" value="None"/>
</element>
<element name="TAB2" library="a-lib" package="KEYSTONE_TAB_TOP" value="">
<attribute name="HOLE" value="0.13 Dia"/>
<attribute name="ORIENTATION" value="SIDE"/>
<attribute name="PARTNUM" value="612"/>
<attribute name="THREAD" value="None"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP4" pad="P$1"/>
<contactref element="JP2" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="JP3" pad="P$1"/>
<contactref element="SW1" pad="3"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="P$1"/>
<contactref element="SW1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
