<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<text>SONIC 2470 Prototype</text>
<text>5 DEC 2018</text>
<text>v 1</text>
<text>BENDER</text>
<text>20mm Open Bat v1</text>
</plain>
<libraries>
<library name="Keystone">
<packages>
<package name="1052">
<description>2450 SMT Battery Holder&lt;br&gt;
KeyStone part 1052</description>
</package>
<package name="PLATED_HOLE_1.02MM">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="1206_A">
</package>
<package name="0805_B">
</package>
</packages>
</library>
<library name="microchip">
<packages>
<package name="SOIC-14-N">
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0805">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN02">
</package>
</packages>
</library>
<library name="TAG-CONNECT">
<packages>
<package name="PLUG-OF-NAILS">
</package>
</packages>
</library>
<library name="VISHAY">
<packages>
<package name="TEPT5060">
</package>
</packages>
</library>
<library name="DIALIGHT">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="HEX_22_RADIUS">
<description>Hexagonal base for SONIC project</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="KEMET" package="0805_B" value="0.1u"/>
<element name="PIC16LF1704" library="microchip" package="SOIC-14-N" value="PICF1615">
<attribute name="NAME"/>
</element>
<element name="R1" library="Stackpole" package="0805" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="OST" package="OSTVN02" value="M02"/>
<element name="U$3" library="TAG-CONNECT" package="PLUG-OF-NAILS" value="PIC_ICPH"/>
<element name="R2" library="Stackpole" package="0805" value="10K"/>
<element name="R3" library="Stackpole" package="1206" value="39K"/>
<element name="C2" library="KEMET" package="1206_A" value="22u"/>
<element name="RED" library="DIALIGHT" package="0805" value="LED0805">
<attribute name="NAME"/>
</element>
<element name="B2" library="Keystone" package="1052" value="BATTERY20MM_OPEN"/>
<element name="U$1" library="VISHAY" package="TEPT5060" value="TEMT5060">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="ERIC" package="HEX_22_RADIUS" value=""/>
<element name="VDD" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE"/>
<element name="GND" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE"/>
<element name="VPH" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE"/>
<element name="PWM" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE"/>
<element name="CC" library="Keystone" package="PLATED_HOLE_1.02MM" value="TEST_POINTMINIATURE"/>
</elements>
<signals>
<signal name="GND">
<contactref element="PIC16LF1704" pad="14"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="B2" pad="K"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="LED">
<contactref element="PIC16LF1704" pad="6"/>
<contactref element="RED" pad="A"/>
</signal>
<signal name="CC">
<contactref element="PIC16LF1704" pad="7"/>
<contactref element="U$1" pad="C"/>
<contactref element="CC" pad="1"/>
</signal>
<signal name="PWM">
<contactref element="PIC16LF1704" pad="11"/>
<contactref element="U$2" pad="1"/>
<contactref element="PWM" pad="1"/>
</signal>
<signal name="C1IN1-">
<contactref element="PIC16LF1704" pad="9"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$1" pad="E"/>
<contactref element="VPH" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="RED" pad="K"/>
</signal>
<signal name="ICSPDAT">
<contactref element="U$3" pad="4"/>
<contactref element="PIC16LF1704" pad="13"/>
</signal>
<signal name="MCLR">
<contactref element="PIC16LF1704" pad="4"/>
<contactref element="U$3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="ICSPCLK">
<contactref element="PIC16LF1704" pad="12"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="VDD">
<contactref element="U$3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="B2" pad="A"/>
<contactref element="PIC16LF1704" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="VDD" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="PIC16LF1704" pad="2"/>
<contactref element="PIC16LF1704" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
