(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 0)
    (zones 0)
    (modules 0)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (gr_text "York Modular 2020" (at 116.2812 102.3239 90) (layer B.SilkS))
  (gr_text "BAD TRIP VCO+VCF" (at 135.3439 27.3812) (layer F.Mask))
  (gr_text "BAD TRIP VCO+VCF" (at 135.3439 27.3812) (layer F.Cu))
  (gr_text OUT (at 139.8524 137.2616) (layer F.Mask))
  (gr_text Filter (at 129.5781 140.4493 90) (layer F.Mask))
  (gr_text Form (at 120.5611 140.0048 90) (layer F.Mask))
  (gr_text FBK (at 128.5748 89.1286 90) (layer F.Mask))
  (gr_text LVL (at 122.5423 66.5099) (layer F.Mask))
  (gr_text LVL (at 137.8839 66.4972) (layer F.Mask))
  (gr_text CV (at 139.0396 57.9247) (layer F.Mask))
  (gr_text CV (at 121.5009 57.9247) (layer F.Mask))
  (gr_text "VCF\n" (at 139.2809 40.1828) (layer F.Mask))
  (gr_text VCO (at 121.5898 40.1828) (layer F.Mask))
  (gr_text OUT (at 139.8651 137.2616) (layer F.Cu))
  (gr_text Filter (at 129.5781 140.4493 90) (layer F.Cu))
  (gr_text Form (at 120.5611 140.0048 90) (layer F.Cu))
  (gr_text FBK (at 128.5748 89.1286 90) (layer F.Cu))
  (gr_text LVL (at 137.8839 66.5099) (layer F.Cu))
  (gr_text LVL (at 122.5423 66.5099) (layer F.Cu))
  (gr_text CV (at 139.0396 57.9247) (layer F.Cu))
  (gr_text CV (at 121.5009 57.9247) (layer F.Cu))
  (gr_text "VCF\n" (at 139.2809 40.1828) (layer F.Cu))
  (gr_text VCO (at 121.5898 40.1828) (layer F.Cu))
  (gr_line (start 145.27732 24.53562) (end 145.27732 152.93562) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.13732 24.53562) (end 145.27732 24.53562) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145.27732 152.93562) (end 115.13732 152.93562) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 115.13732 152.93562) (end 115.13732 24.53562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 137.83732 89.20562) (end 141.58732 89.20562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 137.83732 75.23562) (end 141.58732 75.23562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 122.59732 75.23562) (end 126.34732 75.23562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 139.10732 48.56562) (end 142.35732 48.56562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 121.32732 48.56562) (end 124.57732 48.56562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 122.63732 149.93562) (end 124.13732 149.93562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 122.63732 27.43562) (end 124.13732 27.43562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 139.73732 128.57562) (end 142.98732 128.57562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 129.57732 129.84562) (end 132.327319 129.84562) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 120.68732 129.84562) (end 123.43732 129.84562) (layer Edge.Cuts) (width 0.2))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.955 170.4975) (xy 105.2195 163.6522) (xy 110.6932 21.2471) (xy 150.0886 18.8087)
      )
    )
  )
)
