(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 60)
    (no_connects 0)
    (area 129.342143 78.185 158.81262 111.215)
    (thickness 1.6)
    (drawings 18)
    (tracks 184)
    (zones 0)
    (modules 37)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.19)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFCFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "Net-(C5-Pad2)")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C7-Pad2)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(J1-Pad1)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad4)")
  (net 13 "Net-(R1-Pad1)")
  (net 14 "Net-(R2-Pad1)")
  (net 15 "Net-(R5-Pad2)")
  (net 16 "Net-(R6-Pad2)")
  (net 17 "Net-(R7-Pad2)")
  (net 18 "Net-(R8-Pad2)")
  (net 19 "Net-(U1-Pad2)")
  (net 20 "Net-(U1-Pad4)")
  (net 21 "Net-(U2-Pad5)")
  (net 22 "Net-(U2-Pad6)")
  (net 23 "Net-(U2-Pad11)")
  (net 24 "Net-(U2-Pad13)")
  (net 25 "Net-(U2-Pad14)")
  (net 26 "Net-(U2-Pad15)")
  (net 27 "Net-(U2-Pad16)")
  (net 28 "Net-(U2-Pad21)")
  (net 29 "Net-(U2-Pad22)")
  (net 30 "Net-(U2-Pad23)")
  (net 31 VDD)
  (net_class Default "This is the default net class."
    (clearance 0.19)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net VDD)
  )
  (module Headphone:Screw (layer F.Cu) (tedit 581FEC5B)
    (at 154.75 82)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Headphone:Screw (layer F.Cu) (tedit 581FEC53)
    (at 154.75 107)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Headphone:Screw (layer F.Cu) (tedit 581FEC55)
    (at 133.5 107)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Headphone:C_0402 (layer B.Cu) (tedit 581FE741)
    (at 141.5 103.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer B.Cu) (tedit 581FE743)
    (at 144 103.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6BE)
    (at 144.75 96.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6BB)
    (at 144.75 98 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer B.Cu) (tedit 581FE747)
    (at 146.5 103.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 1.7 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6B7)
    (at 145.25 101.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6B4)
    (at 146.5 101.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6C9)
    (at 149.75 90.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:SMD-1206_Pol (layer F.Cu) (tedit 57D0A947)
    (at 151 104.5 270)
    (attr smd)
    (fp_text reference C9 (at -0.05 -2.55 270) (layer F.SilkS) hide)
    (fp_text value CP (at -0.05 3.85 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6AA)
    (at 149 101.75 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.7 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6C6)
    (at 154.25 95.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:C_0402 (layer F.Cu) (tedit 581FE6C4)
    (at 154.25 97.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -1.7 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE73F)
    (at 142.5 99.5)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE73C)
    (at 142.5 101)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE6A7)
    (at 144 102.25 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE6B0)
    (at 147.75 102.25 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer B.Cu) (tedit 581FE6D6)
    (at 147.5 89.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 1.8 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE6AC)
    (at 145.25 103.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer B.Cu) (tedit 581FE6D3)
    (at 149 89.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 1.8 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.8 270) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:R_0402 (layer F.Cu) (tedit 581FE6AE)
    (at 146.5 103.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 -1.8 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 581FE752)
    (at 145.25 100)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.5) (layer B.SilkS) hide)
    (fp_text value PIC12F1822 (at 0 -3.5) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 VDD))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C5-Pad2)"))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Headphone:QFN-28-LM49270 (layer F.Cu) (tedit 581FDF23)
    (at 149.25 96.5)
    (attr smd)
    (fp_text reference U2 (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value LM49270 (at 0 4.1) (layer F.Fab))
    (pad 1 smd rect (at -2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 5 smd rect (at -2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 8 smd rect (at -1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 9 smd rect (at -1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 10 smd rect (at -0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 0 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 13 smd rect (at 1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad15)"))
    (pad 16 smd rect (at 2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 18 smd rect (at 2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 20 smd rect (at 2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad23)"))
    (pad 24 smd rect (at 0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 VDD))
    (pad 25 smd rect (at 0 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R7-Pad2)"))
    (pad 26 smd rect (at -0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
    (pad 27 smd rect (at -1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad 28 smd rect (at -1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FEC47)
    (at 132.75 97.75)
    (fp_text reference W1 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R1-Pad1)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FEC49)
    (at 132.75 101)
    (fp_text reference W2 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R2-Pad1)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FEE7C)
    (at 144.25 107.75)
    (fp_text reference W3 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R6-Pad2)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FEE7E)
    (at 147.5 107.75)
    (fp_text reference W4 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R8-Pad2)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FE722)
    (at 155.5 90.5)
    (fp_text reference W5 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad23)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FE69F)
    (at 155.5 102.5)
    (fp_text reference W6 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad13)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FE721)
    (at 155.5 93.5)
    (fp_text reference W7 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad22)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 581FE6A2)
    (at 155.5 99.5)
    (fp_text reference W8 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad14)"))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 5820FDB5)
    (at 140.75 107.75)
    (fp_text reference W9 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Headphone:Pad (layer F.Cu) (tedit 5820FDAF)
    (at 137.5 107.75)
    (fp_text reference W10 (at 0 2.5) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 31 VDD))
  )
  (module Headphone:SJ-3524-SMT-TR (layer F.Cu) (tedit 581FE6CF)
    (at 135.4 89.5)
    (fp_text reference J1 (at 0 -7.65) (layer F.SilkS) hide)
    (fp_text value JACK_TRS_4PINS (at 0 7.35) (layer F.Fab))
    (pad 3 smd rect (at 0 -3.7) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -2 3.7) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 7.4 3.7) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at 11.3 -0.75) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad4)"))
    (pad "" np_thru_hole circle (at 6.1 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -0.9 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Headphone:Screw (layer F.Cu) (tedit 581FEC59)
    (at 133.5 82)
    (fp_text reference Screw (at 0 2.4) (layer F.SilkS) hide)
    (fp_text value Screw (at 0 -2.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text GND (at 140.75 105.5) (layer F.SilkS))
  (gr_text 5v (at 137.5 105.5) (layer F.SilkS))
  (gr_text DOWN (at 136.4 101) (layer F.SilkS))
  (gr_text UP (at 135.3 97.75) (layer F.SilkS))
  (gr_line (start 131 109.5) (end 157.25 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 79.5) (end 157.25 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.25 109.5) (end 157.25 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131 79.5) (end 131 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text RIN (at 147.5 105.5) (layer F.SilkS))
  (gr_text LIN (at 144.25 105.5) (layer F.SilkS))
  (gr_text L- (at 153.25 93.5 90) (layer F.SilkS))
  (gr_text L+ (at 153.25 90.5 90) (layer F.SilkS))
  (gr_text R+ (at 153.25 102.25 90) (layer F.SilkS))
  (gr_text R- (at 153.25 99.5 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 157.25 109.5) (xy 131 109.5) (xy 131 79.5) (xy 157.25 79.5) (xy 157.25 109.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 157.25 109.5) (xy 131 109.5) (xy 131 79.5) (xy 157.25 79.5) (xy 157.25 109.5)
      )
    )
  )
)
