(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 88)
    (zones 0)
    (modules 11)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (trace_clearance 0.1778)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.0254)
    (segment_width 0.1778)
    (pcb_text_width 0.2032)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.127)
    (mod_text_size 0.7112 0.7112)
    (mod_text_width 0.1016)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 96.52)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 /En)
  (net 9 +3V3)
  (net 10 /DTR_TTL)
  (net 11 /DSR_TTL)
  (net 12 /TX_TTL)
  (net 13 /RX_TTL)
  (net 14 /DTR_232)
  (net 15 /DCD_232)
  (net 16 /DSR_232)
  (net 17 /CTS_232)
  (net 18 /RTS_232)
  (net 19 /RX_232)
  (net 20 /TX_232)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.1778)
    (add_net +3V3)
    (add_net /CTS_232)
    (add_net /DCD_232)
    (add_net /DSR_232)
    (add_net /DSR_TTL)
    (add_net /DTR_232)
    (add_net /DTR_TTL)
    (add_net /En)
    (add_net /RTS_232)
    (add_net /RX_232)
    (add_net /RX_TTL)
    (add_net /TX_232)
    (add_net /TX_TTL)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
  )
  (module 0_LOCAL:Adafruit_Feather_stagger_6mil (layer F.Cu) (tedit 60436A52)
    (at 147.32 96.52 180)
    (fp_text reference J1 (at -5.842 0) (layer F.SilkS) hide)
    (fp_text value Adafruit_Feather (at 0 -2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 22.86 -8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 22.86 8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.86 8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -22.86 -8.89 180) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 19.05 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 16.51 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 /TX_TTL))
    (pad 14 thru_hole circle (at 13.97 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 /RX_TTL))
    (pad 13 thru_hole circle (at 11.43 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 8.89 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 6.35 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 3.81 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 1.27 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -1.27 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -3.81 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -6.35 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -8.89 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -11.43 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -13.97 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -16.51 10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 +3V3))
    (pad 1 thru_hole circle (at -19.05 10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 19.05 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 16.51 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 13.97 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 /DTR_TTL))
    (pad 20 thru_hole circle (at 11.43 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 /DSR_TTL))
    (pad 21 thru_hole circle (at 8.89 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 6.35 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 3.81 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 1.27 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -1.27 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at -3.81 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -6.35 -10.2362 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 /En))
    (pad 28 thru_hole circle (at -8.89 -10.0838 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
  )
  (module 0_LOCAL:CSS-121xC (layer F.Cu) (tedit 5F727EB8)
    (at 168.91 96.52 90)
    (fp_text reference S1 (at 0 1.3 90) (layer F.SilkS))
    (fp_text value DS04-254-1L-01BK (at 0 -2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -1 0 90) (size 1.0922 1.0922) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 /En))
    (pad 1 thru_hole circle (at -3 0 90) (size 1.0922 1.0922) (drill 0.6) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1 0 90) (size 1.0922 1.0922) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/CSS-1210MC.wrl
      (offset (xyz 0 -2.2 0.9399999999999999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
  )
  (module 0_LOCAL:PinHeader_1x02_P2.54mm_Horizontal (layer B.Cu) (tedit 5F491FD8)
    (at 127.508 91.694)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 4.385 2.27) (layer B.SilkS) hide)
    (fp_text value Jumper_2_Bridged (at 4.385 -4.81) (layer B.Fab))
    (fp_text user %R (at 2.77 -1.27 -90) (layer B.Fab))
    (pad 2 thru_hole custom (at 0 -2.54) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 /RTS_232) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 17 /CTS_232))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:DSUB-25_Male_Vertical_P2.77x2.84mm (layer B.Cu) (tedit 5F491F41)
    (at 163.957 97.79 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at 1.4605 -1.2827 180) (layer B.SilkS) hide)
    (fp_text value DB25_Male (at 16.62 -8.73 180) (layer B.Fab))
    (fp_text user %R (at 16.62 -1.42 180) (layer B.Fab))
    (pad 25 thru_hole circle (at 31.855 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 29.085 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 26.315 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 23.545 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 20.775 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 18.005 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 14 /DTR_232))
    (pad 19 thru_hole circle (at 15.235 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 12.465 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 33.24 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 30.47 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 27.7 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 24.93 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 22.16 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 19.39 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 15 /DCD_232))
    (pad 7 thru_hole circle (at 16.62 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 13.85 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 16 /DSR_232))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 17 /CTS_232))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 18 /RTS_232))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 19 /RX_232))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 20 /TX_232))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_25_PP_Z_cut.step
      (offset (xyz 16.625 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 154.305 94.9706 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.0254 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +3V3))
    (pad 2 smd roundrect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 154.305 91.0844 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.0254 -0.0254) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 151.13 88.646 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -0.0254 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 147.32 88.646 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.0254 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 143.51 88.646 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.0508 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:NetTie-2_SMD_10 (layer F.Cu) (tedit 5F3D08F8)
    (at 147.3454 99.187 180)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value Net-Tie_2 (at 0 1.2) (layer F.Fab))
    (pad 2 smd circle (at 0.254 0 180) (size 0.254 0.254) (layers F.Cu)
      (net 15 /DCD_232))
    (pad 1 smd circle (at -0.254 0 180) (size 0.254 0.254) (layers F.Cu)
      (net 16 /DSR_232))
  )
  (module 0_LOCAL:SOIC-16_W3.90mm (layer F.Cu) (tedit 5F3A577D)
    (at 147.32 93.2688 180)
    (attr smd)
    (fp_text reference U1 (at 0 -0.762) (layer F.SilkS) hide)
    (fp_text value MAX3232 (at 0 0) (layer F.SilkS))
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 16 smd roundrect (at -4.445 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 +3V3))
    (pad 15 smd roundrect (at -3.175 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 14 smd roundrect (at -1.905 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /RX_232))
    (pad 13 smd roundrect (at -0.635 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /TX_232))
    (pad 12 smd roundrect (at 0.635 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /RX_TTL))
    (pad 11 smd roundrect (at 1.905 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /TX_TTL))
    (pad 10 smd roundrect (at 3.175 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /DTR_TTL))
    (pad 9 smd roundrect (at 4.445 -2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /DSR_TTL))
    (pad 8 smd roundrect (at 4.445 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /DTR_232))
    (pad 7 smd roundrect (at 3.175 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /DSR_232))
    (pad 6 smd roundrect (at 1.905 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)"))
    (pad 5 smd roundrect (at 0.635 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)"))
    (pad 4 smd roundrect (at -0.635 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 smd roundrect (at -1.905 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at -3.175 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -4.445 2.7 180) (size 0.6 1.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text ON (at 171.958 99.822 90) (layer F.SilkS))
  (gr_text OFF (at 171.958 92.837 90) (layer F.SilkS))
  (gr_text OFF (at 171.958 92.71 90) (layer B.SilkS))
  (gr_text Feather (at 134.62 88.9) (layer F.SilkS))
  (gr_text MounT (at 134.62 90.805) (layer F.SilkS))
  (gr_text CTS (at 125.095 91.694) (layer B.SilkS))
  (gr_text RTS (at 125.095 89.789) (layer B.SilkS))
  (gr_text "DB25M this side" (at 147.32 99.2886) (layer B.SilkS))
  (gr_text "Adafruit Feather this side" (at 147.32 99.2632) (layer F.SilkS))
  (gr_text ON (at 171.958 99.822 90) (layer B.SilkS))
  (gr_text "Feather MounT" (at 147.32 88.646) (layer B.SilkS))
  (gr_text github.com/bkw777/MounT (at 147.32 105.029) (layer B.SilkS))
  (gr_text "C* 0.1uf" (at 155.6258 88.5952) (layer F.SilkS))
  (gr_line (start 121.92 87.63) (end 121.92 105.41) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 170.18 85.09) (end 124.46 85.09) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 172.72 105.41) (end 172.72 87.63) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 124.46 107.95) (end 170.18 107.95) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 124.46 105.41) (end 121.92 105.41) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 124.46 87.63) (end 124.46 85.09) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 170.18 87.63) (end 172.72 87.63) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 170.18 105.41) (end 170.18 107.95) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 121.92 85.09) (xy 172.72 85.09) (xy 172.72 107.95) (xy 121.92 107.95)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 121.92 85.09) (xy 172.72 85.09) (xy 172.72 107.95) (xy 121.92 107.95)
      )
    )
  )
)
