(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 76)
    (zones 0)
    (modules 13)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.75)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.75 0.4)
    (user_via 1 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4 1.4)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 147.574 91.44)
    (grid_origin 115.316 108.204)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LaserCathode)
  (net 2 /LaserAnode)
  (net 3 GND)
  (net 4 /TEC-)
  (net 5 /TEC+)
  (net 6 /Therm2)
  (net 7 /Therm1)
  (net 8 /Therm4)
  (net 9 /Therm3)
  (net 10 /TEC2+)
  (net 11 /TEC2-)
  (net 12 /LED1)
  (net 13 /LED2)
  (net 14 "Net-(Amphenolt3638404-Pad6)")
  (net 15 "Net-(Amphenolt3638404-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 1)
    (via_dia 0.75)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LaserAnode)
    (add_net /LaserCathode)
    (add_net /TEC+)
    (add_net /TEC-)
    (add_net /TEC2+)
    (add_net /TEC2-)
    (add_net /Therm1)
    (add_net /Therm2)
    (add_net /Therm3)
    (add_net /Therm4)
    (add_net GND)
    (add_net "Net-(Amphenolt3638404-Pad5)")
    (add_net "Net-(Amphenolt3638404-Pad6)")
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5D6F9523)
    (at 138.176 106.172)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 1.27 -1.92) (layer F.SilkS))
    (fp_text value R (at 1.27 1.92) (layer F.Fab))
    (fp_text user %R (at 1.27 -1.92) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 GND) (zone_connect 1) (thermal_width 0.3) (thermal_gap 0.2))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(Amphenolt3638404-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_CommonMode_Wuerth_WE-SL2 (layer F.Cu) (tedit 5D6F9182)
    (at 146.812 103.966)
    (descr http://katalog.we-online.de/en/pbs/WE-SL2?sid=5fbec16187#vs_t1:c1_ct:1)
    (tags "Wuerth WE-SL2")
    (attr smd)
    (fp_text reference L1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value L_Coupled (at 0.4 4.2) (layer F.Fab))
    (fp_text user %R (at -0.02 0) (layer F.Fab))
    (pad 4 smd rect (at 3.75 -1.27) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /LaserCathode))
    (pad 3 smd rect (at 3.75 1.27) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /LaserAnode))
    (pad 2 smd rect (at -3.75 1.27) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Amphenolt3638404-Pad6)"))
    (pad 1 smd rect (at -3.75 -1.27) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Amphenolt3638404-Pad5)") (zone_connect 0))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_CommonMode_Wuerth_WE-SL2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMB (layer F.Cu) (tedit 58645DF3)
    (at 141.478 96.774 90)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (attr smd)
    (fp_text reference D1 (at 0 -3 90) (layer F.SilkS))
    (fp_text value B220 (at 0 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /LaserCathode))
    (pad 1 smd rect (at -2.15 0 90) (size 2.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /LaserAnode))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:QLMLogo (layer B.Cu) (tedit 0)
    (at 125.222 104.648 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module MyFootprints:QLMLogo (layer B.Cu) (tedit 5D518C75)
    (at 120.396 77.216 180)
    (fp_text reference G*** (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer F.SilkS) hide)
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 148.844 89.408 270)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm2 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /Therm4))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 9 /Therm3))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 119.126 92.71 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC2 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /TEC2+))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 11 /TEC2-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyFootprints:Binder09-0332-90-12 (layer F.Cu) (tedit 5D6F91A0)
    (at 131.412052 98.03)
    (fp_text reference Amphenolt3638404 (at -1.872052 -9.892) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at 0 -6.35) (layer F.Fab))
    (pad 12 thru_hole circle (at -2 1.51) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /LED1))
    (pad 11 thru_hole circle (at 2 -1.51) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /TEC2-) (zone_connect 0))
    (pad 10 thru_hole circle (at -2.71 -3.59) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /TEC+))
    (pad 9 thru_hole circle (at -3.2 -1.34) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /TEC-))
    (pad 8 thru_hole circle (at -4.1 1.21) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /Therm2))
    (pad 7 thru_hole circle (at -2.29 3.61) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /Therm1))
    (pad 6 thru_hole circle (at 0.41 3.45) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Amphenolt3638404-Pad6)"))
    (pad 5 thru_hole circle (at 2.71 3.59) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(Amphenolt3638404-Pad5)") (zone_connect 1) (thermal_width 0.3) (thermal_gap 0.2))
    (pad 4 thru_hole circle (at 3.2 1.34) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /Therm4))
    (pad 3 thru_hole circle (at 4.1 -1.21) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /Therm3))
    (pad 2 thru_hole circle (at 2.29 -3.61) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /TEC2+))
    (pad 1 thru_hole circle (at -0.44 -3.45) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /TEC2-))
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 148.844 95.758 270)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference LD1 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /LaserAnode))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 1 /LaserCathode))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer B.Cu) (tedit 5D4D35B0)
    (at 141.986 88.9 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED1 (at 1.27 2.667 90) (layer B.SilkS))
    (fp_text value SFH4356P (at 1.27 -2.96 270) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(Amphenolt3638404-Pad6)") (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /LED2))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.668 90.1335 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0.254 -2.54) (layer F.SilkS))
    (fp_text value 51 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 /LED2))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 /LED1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 119.126 99.06 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference TEC1 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /TEC+))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 4 /TEC-))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 119.126 105.41 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference Therm1 (at 1.27 3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /Therm2))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 7 /Therm1))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 152.654 108.204) (end 148.336 108.204) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.654 87.376) (end 152.654 108.204) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.336 87.376) (end 152.654 87.376) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.336 108.204) (end 115.316 108.204) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.316 87.376) (end 148.336 87.376) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.316 108.204) (end 115.316 87.376) (layer Edge.Cuts) (width 0.1))
  (gr_text + (at 124.206 90.17) (layer F.SilkS))
  (gr_text - (at 124.206 92.71) (layer F.SilkS))
  (gr_text + (at 124.206 96.52) (layer F.SilkS))
  (gr_text - (at 124.206 99.06) (layer F.SilkS))
  (gr_text A+ (at 144.78 98.806) (layer F.SilkS))
  (gr_text M (at 131.064 99.314) (layer F.SilkS))
  (gr_text L (at 132.08 97.282) (layer F.SilkS))
  (gr_text K (at 127.508 93.472) (layer F.SilkS))
  (gr_text J (at 126.746 96.52) (layer F.SilkS))
  (gr_text H (at 125.984 100.838) (layer F.SilkS))
  (gr_text G (at 128.524 103.886) (layer F.SilkS))
  (gr_text F (at 131.826 103.886) (layer F.SilkS))
  (gr_text E (at 135.636 102.362) (layer F.SilkS))
  (gr_text D (at 136.398 99.822) (layer F.SilkS))
  (gr_text C (at 136.906 96.266) (layer F.SilkS))
  (gr_text B (at 134.874 93.218) (layer F.SilkS))
  (gr_text A (at 130.81 93.218) (layer F.SilkS))
  (gr_text C- (at 144.78 95.25) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.654 87.376) (xy 115.316 87.376) (xy 115.316 108.204) (xy 152.654 108.204)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.654 87.376) (xy 115.316 87.376) (xy 115.316 108.204) (xy 152.654 108.204)
      )
    )
  )
)
