(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 32)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (title_block
    (title "LC12S Breakout")
    (date 2021-09-27)
    (rev v01)
    (comment 3 "License: MIT")
    (comment 4 "Author: Mike Causer")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad6)")
  (net 2 "Net-(J1-Pad5)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
  )
  (module lc12s_breakout:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 6151B40F)
    (at 133.35 127 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J1 (at 3.81 -1.27 180) (layer F.Fab))
    (fp_text value Conn_01x06_Male (at 3.81 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lc12s_breakout:LC12S_module (layer F.Cu) (tedit 6151852D)
    (at 122.00001 119.888)
    (fp_text reference U1 (at -1 -3.81) (layer F.Fab))
    (fp_text value LC12S (at -1 -6.35) (layer F.Fab))
    (pad 6 smd rect (at 10 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 5 smd rect (at 8 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at 6 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at 4 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 2 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at 0 0) (size 1.27 3.81) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad6)"))
  )
  (gr_text v1.0 (at 127 112.268) (layer B.SilkS))
  (gr_text "LC12S\nBreakout" (at 127 108.839) (layer B.SilkS))
  (gr_text GND (at 133.35 125.476 90) (layer B.SilkS))
  (gr_text CS (at 130.81 125.476 90) (layer B.SilkS))
  (gr_text SET (at 128.27 125.476 90) (layer B.SilkS))
  (gr_text TXD (at 125.73 125.476 90) (layer B.SilkS))
  (gr_text RXD (at 123.19 125.476 90) (layer B.SilkS))
  (gr_text VCC (at 120.65 125.476 90) (layer B.SilkS))
  (gr_line (start 134.62 118.11) (end 133.85165 117.33911) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 118.11) (end 120.15089 117.33911) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.15089 103.88854) (end 133.85165 103.88854) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.85165 103.88854) (end 133.85165 117.33911) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.15089 103.88854) (end 120.15089 117.33911) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 128.27) (end 134.62 128.27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 128.27) (end 119.38 118.11) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 128.27) (end 134.62 118.11) (layer Edge.Cuts) (width 0.05))
  (gr_text GND (at 133.35 125.476 90) (layer F.SilkS))
  (gr_text CS (at 130.81 125.476 90) (layer F.SilkS))
  (gr_text SET (at 128.27 125.476 90) (layer F.SilkS))
  (gr_text TXD (at 125.73 125.476 90) (layer F.SilkS))
  (gr_text RXD (at 123.19 125.476 90) (layer F.SilkS))
  (gr_text VCC (at 120.65 125.476 90) (layer F.SilkS))
  (zone (net 6) (net_name "Net-(J1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.874 128.524) (xy 119.126 128.524) (xy 119.126 102.743) (xy 134.874 102.743)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.874 128.524) (xy 119.126 128.524) (xy 119.126 102.743) (xy 134.874 102.743)
      )
    )
  )
)
