(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 60)
    (no_connects 3)
    (area 21.514999 112.319999 54.685001 175.970001)
    (thickness 1.6)
    (drawings 25)
    (tracks 126)
    (zones 0)
    (modules 24)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.3302)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 /RST)
  (net 4 /R7S)
  (net 5 /MISO)
  (net 6 +5V)
  (net 7 /SCK)
  (net 8 /MOSI)
  (net 9 /RX)
  (net 10 /TX)
  (net 11 TIME)
  (net 12 COLOR)
  (net 13 /SDA)
  (net 14 WS2812)
  (net 15 /SCL)
  (net 16 "Net-(IC2-Pad1)")
  (net 17 "Net-(IC2-Pad2)")
  (net 18 "Net-(IC2-Pad7)")
  (net 19 "Net-(J3-Pad2)")
  (net 20 "Net-(D1-Pad1)")
  (net 21 "Net-(C5-Pad1)")
  (net 22 "Net-(IC1-Pad15)")
  (net 23 "Net-(IC1-Pad16)")
  (net 24 "Net-(IC1-Pad9)")
  (net 25 "Net-(IC1-Pad23)")
  (net 26 "Net-(IC1-Pad10)")
  (net 27 "Net-(IC1-Pad24)")
  (net 28 "Net-(IC1-Pad11)")
  (net 29 "Net-(IC1-Pad25)")
  (net 30 "Net-(IC1-Pad12)")
  (net 31 "Net-(IC1-Pad26)")
  (net 32 "Net-(IC1-Pad13)")
  (net 33 "Net-(IC1-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /R7S)
    (add_net /RST)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net COLOR)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(IC2-Pad1)")
    (add_net "Net-(IC2-Pad2)")
    (add_net "Net-(IC2-Pad7)")
    (add_net "Net-(J3-Pad2)")
    (add_net TIME)
    (add_net WS2812)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 26.035 130.81 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /RST))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_1058_1x2032-CoinCell (layer B.Cu) (tedit 589EE147)
    (at 38.1 120.65 180)
    (descr http://www.keyelco.com/product-pdf.cfm?p=14028)
    (tags "Keystone type 1058 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 -7.62 180) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 9.398 180) (layer B.Fab))
    (pad 1 smd rect (at -14.68 0 180) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 14.68 0 180) (size 2.54 3.51) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Crystals:Crystal_C18-LF_d3.0mm_l8.0mm_Horizontal (layer F.Cu) (tedit 58CD2FDC)
    (at 52.07 128.27 180)
    (descr "Crystal THT C18-LF 8.0mm length 3.0mm diameter")
    (tags ['C18-LF'])
    (fp_text reference Y2 (at 3.81 3.175 180) (layer F.SilkS))
    (fp_text value 32.7680kHz (at 3.97 2.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 6.5 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 16 "Net-(IC2-Pad1)"))
    (pad 2 thru_hole circle (at 1.9 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 17 "Net-(IC2-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_C18-LF_d3.0mm_l8.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 31.115 147.36 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.27 -1.905 270) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.11 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 26.035 128.27 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.25 1.905 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /RST))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /R7S))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:IDC_Header_Straight_6pins (layer F.Cu) (tedit 584BD5A1)
    (at 47.625 153.67 270)
    (descr "6 pins through hole IDC header")
    (tags "IDC header socket VASCH AVR ISP")
    (fp_text reference CON1 (at 2.54 -5.08 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 3 5 270) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /RST))
    (pad 6 thru_hole oval (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 23.495 138.43 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -1.905 -1.905 180) (layer F.SilkS))
    (fp_text value UAR7 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /TX))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RX))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /R7S))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5A1BF610)
    (at 44.8 171.45 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J2 (at -8.45 5.75 360) (layer F.SilkS))
    (fp_text value Jack-DC (at -6.2 -5.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at -6 0 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 3 thru_hole rect (at -3 4.7 180) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 6 +5V))
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB133_03x5mm_Straight (layer F.Cu) (tedit 59661312)
    (at 27.305 163.91 270)
    (descr "3-way 5.0mm pitch terminal block, http://www.philmore-datak.com/mc/Page%20197.pdf")
    (tags "screw terminal block")
    (fp_text reference J3 (at 5.635 -5.715 270) (layer F.SilkS))
    (fp_text value "Neo Pixel" (at 5 6.9 270) (layer F.Fab))
    (fp_text user %R (at 5 0.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 10 0 270) (size 2.4 2.4) (drill 1.47) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Connectors_Terminal_Blocks.3dshapes/TerminalBlock_Philmore_TB133_03x5mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 28.575 130.81 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 TIME))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 52.705 140.97 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 3.81 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 23.495 147.955 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 1.905 90) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 TIME))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 TIME))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 23.495 157.48 90)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 3.175 1.905 90) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 COLOR))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 COLOR))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 58CC8E33)
    (at 52.705 130.81 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference IC2 (at -2.54 7.62 360) (layer F.SilkS))
    (fp_text value DS1307+ (at 3.81 10.01 270) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(IC2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(IC2-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(IC2-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 40.005 173.99 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at -1.27 3.175 180) (layer F.SilkS))
    (fp_text value 470uF (at 1.25 4.46 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 23.495 160.02)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 330R (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 WS2812))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 52.705 143.51 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 4.7k (at 3.81 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 /SCL))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 52.665 146.05 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C4 (at 1.23 -1.905 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 47.585 146.05 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C5 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Resonator-3pin_w7.0mm_h2.5mm (layer F.Cu) (tedit 58CD2E9D)
    (at 31.115 157.44 90)
    (descr "Ceramic Resomator/Filter 7.0x2.5mm^2, length*width=7.0x2.5mm^2 package, package length=7.0mm, package width=2.5mm, 3 pins")
    (tags "THT ceramic resonator filter")
    (fp_text reference Y1 (at -1.31 -1.27 180) (layer F.SilkS))
    (fp_text value 16MHz (at 2.5 2.45 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad10)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad9)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Resonator-3pin_w7.0mm_h2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 34.29 171.45 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 3.81 -1.905 360) (layer F.SilkS))
    (fp_text value Green (at 1.27 2.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 58CC8E2F)
    (at 34.29 132.08)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference IC1 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value ATMEGA168PA-PU (at 3.81 35.41) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /RST))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(IC1-Pad15)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /RX))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(IC1-Pad16)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /TX))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 TIME))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 COLOR))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 WS2812))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C5-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad9)"))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(IC1-Pad23)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad10)"))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(IC1-Pad24)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(IC1-Pad11)"))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(IC1-Pad25)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(IC1-Pad12)"))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(IC1-Pad26)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(IC1-Pad13)"))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /SDA))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(IC1-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /SCL))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm_Socket_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 31.115 130.81 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 3.81 -1.86 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 COLOR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 34.29 168.275)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10k (at 3.81 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5V/DC (at 36.83 125.73) (layer F.SilkS))
  (gr_text "WORD CLOCK" (at 36.83 115.57) (layer F.SilkS))
  (gr_text "Battery:\nCR2032" (at 36.83 119.38) (layer F.SilkS))
  (gr_text COLOR (at 31.75 125.095) (layer F.SilkS))
  (gr_text TIME (at 31.75 116.84) (layer F.SilkS))
  (gr_text "RTS\nRX\nTX\nGND" (at 22.225 120.65) (layer F.SilkS))
  (gr_line (start 49.53 175.895) (end 26.67 175.895) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 26.67 170.815) (end 26.67 175.895) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 49.53 170.815) (end 54.61 170.815) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 117.475) (end 54.61 170.815) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 49.53 117.475) (end 49.53 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 26.67 117.475) (end 21.59 117.475) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 26.67 112.395) (end 49.53 112.395) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 21.59 170.815) (end 21.59 117.475) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3302))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21.59 112.395) (xy 53.975 112.395) (xy 54.61 175.895) (xy 20.955 175.895)
      )
    )
  )
)
