(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 12)
    (no_connects 0)
    (area 141.478 79.121 160.655 107.061)
    (thickness 1.6)
    (drawings 14)
    (tracks 106)
    (zones 0)
    (modules 6)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.2794)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 186.11 112.58)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P5-Pad1)")
  (net 2 "Net-(P5-Pad3)")
  (net 3 "Net-(P1-Pad1)")
  (net 4 "Net-(P1-Pad2)")
  (net 5 /VCC)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /VCC)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58C2088E)
    (at 147.6544 84.2336 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58C20896)
    (at 147.6544 102.0136 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P5-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 58C20A6E)
    (at 146.613 93.149 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.127 1.905 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(P5-Pad3)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 58C20A7C)
    (at 150.296 93.149 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -0.127 1.778 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 58C20A8C)
    (at 153.852 93.149 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -0.127 1.905 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /VCC))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sparkfun:SF-ROTARY-ENCODER (layer F.Cu) (tedit 58C20886)
    (at 150.26302 93.07274 90)
    (fp_text reference ROT1 (at 0 9.5 90) (layer F.SilkS) hide)
    (fp_text value ROTARY-ENCODER (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.5 -7 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad2)"))
    (pad 2 thru_hole circle (at -2.5 7.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P5-Pad1)"))
    (pad 3 thru_hole circle (at 0 7.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad1)"))
    (pad 4 thru_hole circle (at 2.5 7.5 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P5-Pad3)"))
    (pad 5 thru_hole circle (at 2.5 -7 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad1)"))
    (pad "" thru_hole circle (at 5.6 0 90) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -5.6 0 90) (size 3 3) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "2017-03-09\n" (at 155.0204 93.022 90) (layer F.SilkS))
  (gr_text "SW1\n" (at 151.4644 84.2844 90) (layer F.SilkS))
  (gr_text "VCC\n\n" (at 155.2744 84.1828 90) (layer F.SilkS))
  (gr_text "GND\n" (at 145.5716 84.2336 90) (layer F.SilkS))
  (gr_line (start 141.914 103.3852) (end 141.914 82.8112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.0844 103.3852) (end 141.914 103.3852) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.0844 82.8112) (end 159.0844 103.3852) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.0156 82.8112) (end 159.0844 82.8112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "2017-03-09\n" (at 155.1855 99.88) (layer B.SilkS))
  (gr_text "github.com/pdp7\n" (at 144.708 93.3268 90) (layer F.SilkS))
  (gr_text GND (at 151.439 101.912 90) (layer F.SilkS))
  (gr_text B (at 154.614 101.912) (layer F.SilkS))
  (gr_text "A\n" (at 145.6605 101.912) (layer F.SilkS))
  (gr_text rotary-encoder-breakout (at 146.1304 93.1236 90) (layer F.SilkS))
)
