(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 97)
    (zones 0)
    (modules 22)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.12)
    (segment_width 0.12)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad5)")
  (net 2 "Net-(J2-Pad6)")
  (net 3 "Net-(BT1-Pad1)")
  (net 4 "Net-(LED1-Pad2)")
  (net 5 "Net-(LED2-Pad2)")
  (net 6 "Net-(LED3-Pad2)")
  (net 7 "Net-(LED4-Pad2)")
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-Pad2)")
  (net 13 /GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(LED4-Pad2)")
  )
  (module footprints:bob-small (layer B.Cu) (tedit 0)
    (at 188.087 98.171 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 181.61 92.71)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 12 "Net-(D4-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 181.5 96.52)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 11 "Net-(D3-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 181.61 100.33)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 10 "Net-(D2-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 181.61 104.14)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 8 "Net-(D1-Pad2)"))
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 103.759)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 5,1 (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(LED4-Pad2)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 99.949)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 5,1 (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(LED3-Pad2)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 96.139)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 5,1 (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(LED2-Pad2)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 92.329)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 5,1 (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(LED1-Pad2)"))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 103.759)
    (descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED4 (at 0 -1.05) (layer F.SilkS))
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(LED4-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 13 /GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 99.949)
    (descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED3 (at 0 -1.05) (layer F.SilkS))
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(LED3-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 13 /GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 96.139)
    (descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED2 (at 0 -1.05) (layer F.SilkS))
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(LED2-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 13 /GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 92.329)
    (descr "Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED1 (at 0 -1.05) (layer F.SilkS))
    (fp_text value LED (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(LED1-Pad2)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 13 /GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 177.8 93.599)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1n4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 177.8 97.409)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1n4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 177.8 101.219)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1n4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 177.8 105.029)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1n4148 (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:USB_A_Stewart_SS-52100-001_Horizontal-SMD (layer F.Cu) (tedit 5E5E1E7B)
    (at 187.706 102.068 90)
    (descr "USB A connector https://belfuse.com/resources/drawings/stewartconnector/dr-stw-ss-52100-001.pdf")
    (tags "USB_A Female Connector receptacle")
    (fp_text reference J1 (at 3.5 -2.26 90) (layer F.SilkS))
    (fp_text value USB_A (at 3.5 14.49 90) (layer F.Fab))
    (fp_text user %R (at 3.5 5.99 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 10.07 2.71 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at -3.07 2.71 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at 0 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 2 smd circle (at 2.5 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 3 smd circle (at 4.5 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 4 smd circle (at 7 0 90) (size 1.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_Stewart_SS-52100-001_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:207E-BA00-RA1 (layer F.Cu) (tedit 5E5D9896)
    (at 153.924 99.06 90)
    (fp_text reference J2 (at 0 -2 90) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.7 90) (layer F.Fab))
    (pad 6 smd rect (at 2.1 3 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at -2.2 3 180) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at -5.5 0.5 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at 5.5 0.5 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at 5.5 -3.8 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 6 smd rect (at -5.5 -3.8 90) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad6)"))
    (pad 5 smd rect (at 1.35 0.8 90) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at 0 0.8 90) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 4 smd rect (at 0.7 0.8 90) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.7 0.8 90) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -1.35 0.8 90) (size 0.4 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (model /Users/simon/electornics/usb-cable-test/board/footprints.pretty/207E-BA00-RA1_C_1.IGS
      (offset (xyz -3.5 0.5 1))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 162.56 92.202)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at -3.048 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at -3.048 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
  )
  (module Button_Switch_SMD:SW_SPST_TL3342 (layer F.Cu) (tedit 5A02FC95)
    (at 161.798 101.346 270)
    (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
    (tags "SPST Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -3.75 90) (layer F.SilkS) hide)
    (fp_text value "BAT Test" (at -0.3175 -4.0005 90) (layer F.SilkS))
    (fp_text user %R (at 0 -3.75 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.15 1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -3.15 1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at 3.15 -1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -3.15 -1.9 270) (size 1.7 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery:BatteryHolder_Keystone_1060_1x2032 (layer B.Cu) (tedit 5B98EF5E)
    (at 171.958 98.806)
    (descr http://www.keyelco.com/product-pdf.cfm?p=726)
    (tags "CR2032 BR2032 BatteryHolder Battery")
    (attr smd)
    (fp_text reference CR2030 (at -14.732 5.3) (layer B.SilkS))
    (fp_text value Battery_Cell (at 10.541 10.414) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -14.65 0 180) (size 2.6 3.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 14.65 0 180) (size 2.6 3.6) (layers B.Cu B.Paste B.Mask)
      (net 13 /GND))
    (model ${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_1060_1x2032.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Rev 1" (at 191.135 108.9025) (layer F.SilkS))
  (gr_text github.com/echox/usb-cable-test (at 169.291 108.7755) (layer B.SilkS))
  (gr_line (start 195.5165 87.376) (end 148.59 87.376) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 148.59 94.996) (end 148.59 87.376) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 153.924 94.996) (end 148.59 94.996) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 153.924 103.124) (end 153.924 94.996) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 148.336 103.124) (end 153.924 103.124) (layer Edge.Cuts) (width 0.12))
  (gr_text "USB Cable Tester" (at 162.052 108.458) (layer F.Mask))
  (gr_text "Remove Battery before using Testpads" (at 166.624 88.9) (layer F.SilkS))
  (gr_line (start 195.5165 110.49) (end 195.5165 87.376) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 148.336 110.49) (end 195.5165 110.49) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 148.336 103.124) (end 148.336 110.49) (layer Edge.Cuts) (width 0.12))
)
