<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<wire x1="34.29" y1="17.78" x2="66.98" y2="17.78" width="0" layer="20"/>
<wire x1="66.98" y1="17.78" x2="66.98" y2="49.52" width="0" layer="20"/>
<wire x1="66.98" y1="49.52" x2="34.29" y2="49.52" width="0" layer="20"/>
<wire x1="34.29" y1="49.52" x2="34.29" y2="17.78" width="0" layer="20"/>
<text>TCOM</text>
<text>T1</text>
<text>T2</text>
<text>T3</text>
<text>T4</text>
<text>LCOM-</text>
<text>L1+</text>
<text>L2+</text>
<text>L3+</text>
<text>L4+</text>
<text>T1</text>
<text>L1</text>
<text>L3</text>
<text>T2</text>
<text>LC</text>
<text>TC</text>
<text>L4</text>
<text>L2</text>
<text>T3</text>
<text>T4</text>
<text>Feller 
3914-1-FMI-L-P61 
Breakout Board</text>
<text>Michael Kroll 
Nov. 26th, 2017</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X05" value="Taster">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05" value="LEDs">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X5" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="TCOM">
<contactref element="J1" pad="1"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="T1">
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="T2">
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="T3">
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="T4">
<contactref element="J1" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="LCOM">
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="L1">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="L2">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="L3">
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="L4">
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
