(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 109)
    (zones 0)
    (modules 27)
    (nets 23)
  )
  (page USLetter)
  (title_block
    (title "Single Supply Audio Band-Pass Filter")
    (date 5.10.20)
    (company "Maxim M.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 VDD)
  (net 10 "Net-(C6-Pad2)")
  (net 11 "Net-(C7-Pad1)")
  (net 12 "Net-(C7-Pad2)")
  (net 13 "Net-(C8-Pad2)")
  (net 14 "Net-(C9-Pad2)")
  (net 15 VCC)
  (net 16 GND)
  (net 17 "Net-(C12-Pad1)")
  (net 18 "Net-(R3-Pad1)")
  (net 19 "Net-(U2-Pad5)")
  (net 20 "Net-(U2-Pad6)")
  (net 21 "Net-(U2-Pad7)")
  (net 22 "Net-(U2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net VDD)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 149.86 89.154 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C10 (at 1.27 4.064) (layer F.SilkS))
    (fp_text value 220uF (at 1.27 -4.191) (layer F.SilkS))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_Power_Jack_Circular_Pads (layer F.Cu) (tedit 54E972BC)
    (at 161.29 85.09 180)
    (descr "Connector, Power Jack")
    (tags "CONN POWER JACK")
    (fp_text reference J1 (at 4.445 -5.715) (layer F.SilkS))
    (fp_text value Power (at 0 -5.715) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 1 thru_hole circle (at 6.20014 0 180) (size 4.5 4.5) (drill 3.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC))
    (pad 3 thru_hole circle (at 2.99974 4.8006 180) (size 4 4) (drill 2.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (model connectors/POWER_21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_RCA_Right (layer F.Cu) (tedit 5C181439)
    (at 162.56 119.38 180)
    (descr "Connector, RCA, Right Angle")
    (tags "CONN POWER JACK")
    (fp_text reference J2 (at 5.715 8.255) (layer F.SilkS))
    (fp_text value Input (at 1.905 8.255) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 0 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole circle (at 5.08 5.08 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 2.9718 2.9718) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad2)"))
    (model connectors/POWER_21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Conn_RCA_Right (layer F.Cu) (tedit 5C181439)
    (at 162.56 101.6 180)
    (descr "Connector, RCA, Right Angle")
    (tags "CONN POWER JACK")
    (fp_text reference J3 (at 5.715 8.255) (layer F.SilkS))
    (fp_text value Output (at 1.27 8.255) (layer F.SilkS))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 2.9718 2.9718) (drill 1.5748) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C9-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 5.08 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole circle (at 0 0 180) (size 4.064 4.064) (drill 2.667) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (model connectors/POWER_21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 133.35 99.06)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value OPA4134 (at 3.81 17.57) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VCC))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C8-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 133.35 80.01)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value TLE2426xP (at 3.81 9.95) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 VDD))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad6)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 VCC))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad7)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 80.01)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 123.19 123.19)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 116.84)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 109.22)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 10nF (at -0.08 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 125.73 116.84 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C3 (at -5.08 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 125.73 114.3 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C4 (at -5.08 0) (layer F.SilkS))
    (fp_text value 10nF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 125.73 99.06 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C5 (at -5.08 0) (layer F.SilkS))
    (fp_text value 1.2nF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 125.73 101.6)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C6 (at 5.08 0) (layer F.SilkS))
    (fp_text value 1nF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 99.06)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C7 (at 5.08 0) (layer F.SilkS))
    (fp_text value 3.3nF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad1)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 104.14 180)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C8 (at -5.08 0) (layer F.SilkS))
    (fp_text value 470pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C8-Pad2)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 101.6)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C9 (at 5.08 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C9-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad1)"))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 137.16 93.345)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C11 (at -6.35 -1.27) (layer F.SilkS))
    (fp_text value 100nF (at -6.35 0.635) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Cap_Cer_508 (layer F.Cu) (tedit 52978A41)
    (at 148.59 80.01)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C12 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1uF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 148.59 114.3)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 5.715 0) (layer F.SilkS))
    (fp_text value 68k (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 148.59 111.76 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R2 (at -5.715 0) (layer F.SilkS))
    (fp_text value 75k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 125.73 111.76 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R3 (at -5.715 0) (layer F.SilkS))
    (fp_text value 27k (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 125.73 109.22 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R4 (at -5.715 0) (layer F.SilkS))
    (fp_text value 180k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 125.73 106.68 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R5 (at -5.715 0) (layer F.SilkS))
    (fp_text value 43k (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R3-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 125.73 104.14)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 5.715 0) (layer F.SilkS))
    (fp_text value 33k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 148.59 96.52)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 5.715 0) (layer F.SilkS))
    (fp_text value 39k (at 0 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Components:Res_762 (layer F.Cu) (tedit 5298DB2F)
    (at 148.59 106.68 180)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R8 (at -5.715 0) (layer F.SilkS))
    (fp_text value 27k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C8-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Single Supply\nAudio Band-Pass Filter\n(C) 2020 Maxim Malinov" (at 140.97 122.555) (layer F.SilkS))
  (gr_arc (start 120.65 77.47) (end 120.65 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 163.83 77.47) (end 165.1 77.47) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 163.83 125.73) (end 163.83 127) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 120.65 125.73) (end 119.38 125.73) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 125.73) (end 119.38 77.47) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.83 127) (end 120.65 127) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 165.1 77.47) (end 165.1 125.73) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 76.2) (end 163.83 76.2) (layer Edge.Cuts) (width 0.05))
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 127) (xy 119.38 127) (xy 119.38 76.2) (xy 165.1 76.2)
      )
    )
  )
)
