<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.1524" y1="12.7304" x2="0.1524" y2="0.994246875" width="0.127" layer="20"/>
<wire x1="0.1524" y1="0.994246875" x2="1.221846875" y2="-0.0752" width="0.127" layer="20"/>
<wire x1="1.221846875" y1="-0.0752" x2="11.122303125" y2="-0.0752" width="0.127" layer="20"/>
<wire x1="11.122303125" y1="-0.0752" x2="12.1524" y2="0.954896875" width="0.127" layer="20"/>
<wire x1="12.1524" y1="0.954896875" x2="12.1524" y2="12.7304" width="0.127" layer="20"/>
<wire x1="12.1524" y1="12.7304" x2="0.1524" y2="12.7304" width="0.127" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-PCB">
<description>Card-edge USB A connector.

For boards designed to be plugged directly into a USB slot. If possible, ensure that your PCB is about 2.4mm thick to fit snugly.</description>
</package>
<package name="1X04">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="USB-A-PCB" value="USBPCB"/>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="5V"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="2"/>
<contactref element="JP1" pad="USB_M"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="USB_P"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="4"/>
<contactref element="JP1" pad="GND"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
