<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="15.24" x2="41.58" y2="15.24" width="0" layer="20"/>
<wire x1="41.58" y1="15.24" x2="41.58" y2="80" width="0" layer="20"/>
<wire x1="41.58" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="15.24" width="0" layer="20"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="SMA90_DIP">
<description>SMA DIP Connector 90° 50 Ohm</description>
</package>
<package name="AVRISP">
</package>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
<package name="PUSHBUTTON_SMD_SJ">
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_LOCK_NO_SILK">
</package>
<package name="1X04-1MM-RA">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X09/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT" library="adafruit" package="SMA90_DIP" value="sma"/>
<element name="C1" library="SparkFun" package="1206" value="22pf"/>
<element name="C2" library="SparkFun" package="1206" value="22pf"/>
<element name="IR1" library="SparkFun-Connectors" package="1X03_LOCK_NO_SILK" value="IR"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="LED1" library="led" package="CHIPLED_1206" value="red"/>
<element name="LED2" library="led" package="CHIPLED_1206" value="red"/>
<element name="OLED" library="pinhead" package="1X04" value="oled"/>
<element name="Q1" library="adafruit" package="CTS406" value="16mhz">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="330"/>
<element name="R4" library="SparkFun-Passives" package="1206" value="330"/>
<element name="RS232" library="SparkFun-Connectors" package="1X04-1MM-RA" value="BT OUT/IN"/>
<element name="RX5880" library="pinhead" package="1X09/90" value="rx5880"/>
<element name="U$1" library="atmel" package="TQFP32-08" value="ATMEGA328P"/>
<element name="JP1" library="pinhead" package="1X02" value=""/>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="C3" library="SparkFun" package="1206" value="22pf"/>
<element name="C4" library="SparkFun" package="1206" value="22pf"/>
<element name="C5" library="SparkFun" package="1206" value="22pf"/>
<element name="SW1" library="adafruit" package="PUSHBUTTON_SMD_SJ" value=""/>
<element name="SW2" library="adafruit" package="PUSHBUTTON_SMD_SJ" value=""/>
<element name="SW3" library="adafruit" package="PUSHBUTTON_SMD_SJ" value=""/>
<element name="JP2" library="adafruit" package="1X01" value=""/>
</elements>
<signals>
<signal name="GND1">
<contactref element="ANT" pad="GND1"/>
</signal>
<signal name="GND2">
<contactref element="ANT" pad="GND2"/>
</signal>
<signal name="GND3">
<contactref element="ANT" pad="GND3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="21"/>
<contactref element="U$1" pad="5"/>
<contactref element="LED1" pad="C"/>
<contactref element="OLED" pad="1"/>
<contactref element="RX5880" pad="4"/>
<contactref element="RX5880" pad="9"/>
<contactref element="ISP1" pad="6"/>
<contactref element="RS232" pad="2"/>
<contactref element="IR1" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="SW3" pad="P$1"/>
<contactref element="SW2" pad="P$1"/>
<contactref element="ANT" pad="GND4"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="OLED" pad="2"/>
<contactref element="RX5880" pad="5"/>
<contactref element="ISP1" pad="2"/>
<contactref element="RS232" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="IR1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="26"/>
<contactref element="IC1" pad="3"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="1">
<contactref element="U$1" pad="14"/>
<contactref element="RX5880" pad="1"/>
</signal>
<signal name="2">
<contactref element="U$1" pad="15"/>
<contactref element="RX5880" pad="2"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="3">
<contactref element="U$1" pad="16"/>
<contactref element="RX5880" pad="3"/>
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="RSSI">
<contactref element="U$1" pad="23"/>
<contactref element="RX5880" pad="6"/>
</signal>
<signal name="SCL">
<contactref element="OLED" pad="3"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="SDA">
<contactref element="OLED" pad="4"/>
<contactref element="U$1" pad="27"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="29"/>
<contactref element="ISP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="RS232" pad="4"/>
<contactref element="U$1" pad="30"/>
</signal>
<signal name="RX">
<contactref element="RS232" pad="3"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="SIG">
<contactref element="IR1" pad="1"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="JP1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="SW1" pad="P$2"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="SW2">
<contactref element="SW2" pad="P$2"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="SW3">
<contactref element="SW3" pad="P$2"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="ANT" pad="ANTENNA"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
