(kicad_pcb (version 20170123) (host pcbnew "(2017-07-13 revision 0633d90)-master")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 455)
    (zones 0)
    (modules 26)
    (nets 74)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.4064)
    (user_trace_width 0.762)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 30.353 96.647)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(D1-Pad2)")
  (net 3 GND)
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad5)")
  (net 7 "Net-(J2-Pad7)")
  (net 8 "Net-(J2-Pad8)")
  (net 9 "Net-(J2-Pad10)")
  (net 10 "Net-(J2-Pad11)")
  (net 11 "Net-(J2-Pad12)")
  (net 12 "Net-(J2-Pad13)")
  (net 13 "Net-(J2-Pad15)")
  (net 14 "Net-(J2-Pad16)")
  (net 15 "Net-(J2-Pad17)")
  (net 16 "Net-(J2-Pad18)")
  (net 17 "Net-(J2-Pad19)")
  (net 18 "Net-(J2-Pad21)")
  (net 19 "Net-(J2-Pad23)")
  (net 20 "Net-(J2-Pad24)")
  (net 21 "Net-(J2-Pad26)")
  (net 22 "Net-(J2-Pad27)")
  (net 23 "Net-(J2-Pad28)")
  (net 24 "Net-(J2-Pad31)")
  (net 25 "Net-(J2-Pad32)")
  (net 26 "Net-(J2-Pad33)")
  (net 27 "Net-(J2-Pad36)")
  (net 28 "Net-(J2-Pad37)")
  (net 29 "Net-(J2-Pad38)")
  (net 30 "Net-(J2-Pad40)")
  (net 31 "Net-(R1-Pad1)")
  (net 32 "Net-(R2-Pad1)")
  (net 33 "Net-(R3-Pad1)")
  (net 34 "Net-(R4-Pad1)")
  (net 35 "Net-(R5-Pad1)")
  (net 36 "Net-(R10-Pad1)")
  (net 37 "Net-(U2-Pad2)")
  (net 38 "Net-(U3-Pad1)")
  (net 39 "Net-(U4-Pad2)")
  (net 40 "Net-(U4-Pad4)")
  (net 41 "Net-(U4-Pad6)")
  (net 42 "Net-(U4-Pad8)")
  (net 43 "Net-(R7-Pad1)")
  (net 44 "Net-(RN2-Pad6)")
  (net 45 "Net-(RN2-Pad7)")
  (net 46 "Net-(RN2-Pad8)")
  (net 47 /25V_DC)
  (net 48 /120V_AC)
  (net 49 /Motor_down)
  (net 50 /Motor_up)
  (net 51 /Neutral)
  (net 52 /Light)
  (net 53 /Close_limit)
  (net 54 /Open_limit)
  (net 55 /Wall_console)
  (net 56 "Net-(U5-Pad3)")
  (net 57 "Net-(U4-Pad7)")
  (net 58 "Net-(U4-Pad10)")
  (net 59 "Net-(U4-Pad9)")
  (net 60 "Net-(Q1-Pad2)")
  (net 61 "Net-(R6-Pad2)")
  (net 62 "Net-(R8-Pad1)")
  (net 63 "Net-(R9-Pad1)")
  (net 64 "Net-(RN2-Pad5)")
  (net 65 "Net-(J3-Pad2)")
  (net 66 "Net-(J3-Pad4)")
  (net 67 "Net-(J3-Pad6)")
  (net 68 /5V_OUT)
  (net 69 "Net-(J3-Pad8)")
  (net 70 "Net-(J3-Pad5)")
  (net 71 /lock)
  (net 72 /door)
  (net 73 /light)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /Close_limit)
    (add_net /Open_limit)
    (add_net /Wall_console)
    (add_net /door)
    (add_net /light)
    (add_net /lock)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(RN2-Pad7)")
    (add_net "Net-(RN2-Pad8)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad3)")
  )
  (net_class 120V_AC ""
    (clearance 0.3048)
    (trace_width 0.762)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /120V_AC)
    (add_net /Light)
    (add_net /Motor_down)
    (add_net /Motor_up)
    (add_net /Neutral)
  )
  (net_class 25V ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /25V_DC)
  )
  (net_class 5V ""
    (clearance 0.1524)
    (trace_width 0.4064)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /5V_OUT)
    (add_net GND)
    (add_net VCC)
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 596BD1A8)
    (at 48.26 37.465)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 4.064 -2.286 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 3.81 -0.127) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 596519D9)
    (at 60.833 46.99)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value HE751A0510 (at 3.937 8.001 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 59651AA2)
    (at 91.44 63.373)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U5 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LM339 (at 3.937 7.493 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /door))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /Open_limit))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 /lock))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R8-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(U5-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R10-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R7-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /light))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R9-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5974D66F)
    (at 87.757 54.864 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 4.445 -0.127) (layer F.SilkS))
    (fp_text value 47 (at 1.27 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5974D664)
    (at 87.757 49.784 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -2.413 0) (layer F.SilkS))
    (fp_text value 220 (at 1.27 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /Wall_console))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5973EB9F)
    (at 80.391 71.501 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 1.27 2.159 180) (layer F.SilkS))
    (fp_text value 18k (at 1.27 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module my-modules:OKI-78SR (layer F.Cu) (tedit 597DEF24)
    (at 48.514 95.123)
    (descr OKI-78SR)
    (tags "Undefined or Miscellaneous")
    (fp_text reference U1 (at -1.778 -6.477 -180) (layer F.SilkS))
    (fp_text value OKI-78SR-5_1.5-W36-C (at 7.71296 0.0541) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.45999 1.45999) (drill 0.95987) (layers *.Cu *.Mask F.SilkS)
      (net 47 /25V_DC))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.45999 1.45999) (drill 0.95987) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.45999 1.45999) (drill 0.95987) (layers *.Cu *.Mask F.SilkS)
      (net 68 /5V_OUT))
    (model "/Users/sveit/Dropbox/Library/Application Support/kicad/packages3d/Converters.3dshapes/mps_dcdc_oki_78sr_a.igs"
      (at (xyz -0.1169291338582677 0.1055118110236221 0.07874015748031496))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP5 (layer F.Cu) (tedit 596D0198)
    (at 85.979 67.183 270)
    (descr "5-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at -2.286 0) (layer F.SilkS))
    (fp_text value 47k (at 6.35 2.4 270) (layer F.Fab))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R8-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R9-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R10-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Resistors_THT.3dshapes/R_Array_SIP5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module my-modules:SHDR10W183P0X396_1X10_3962X762X1105P (layer F.Cu) (tedit 5974D7BC)
    (at 39.243 90.043 90)
    (descr 640445-8)
    (tags Connector)
    (fp_text reference J1 (at 38.481 -3.81 180) (layer F.SilkS))
    (fp_text value 1-640445-0 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole circle (at 3.96 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 /25V_DC))
    (pad 3 thru_hole circle (at 7.92 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 /120V_AC))
    (pad 4 thru_hole circle (at 11.88 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 /Motor_down))
    (pad 5 thru_hole circle (at 15.84 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 /Motor_up))
    (pad 6 thru_hole circle (at 19.8 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 /Neutral))
    (pad 7 thru_hole circle (at 23.76 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 /Light))
    (pad 8 thru_hole circle (at 27.72 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 /Close_limit))
    (pad 9 thru_hole circle (at 31.68 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 /Open_limit))
    (pad 10 thru_hole circle (at 35.64 0 180) (size 3.075 3.075) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 55 /Wall_console))
    (model "/Users/sveit/Dropbox/Library/Application Support/kicad/packages3d/Headers.3dshapes/009652108.iges"
      (at (xyz 1.872047244094488 -0.1822834645669291 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module my-modules:G5RL-1A-E-HR (layer F.Cu) (tedit 5974D7CF)
    (at 46.101 39.751 270)
    (descr G5RL-1A-E-HR)
    (tags "Relay or Contactor")
    (fp_text reference K1 (at 1.778 -6.604) (layer F.SilkS))
    (fp_text value G5RL-1A-E-HR_5DC (at 13.97 -5.08 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 2.3 -2.6) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole circle (at 22.3 -2.6) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 /120V_AC))
    (pad 4 thru_hole circle (at 27.3 -2.6) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 52 /Light))
    (pad 5 thru_hole circle (at 27.3 -10.1) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 52 /Light))
    (pad 6 thru_hole circle (at 22.3 -10.1) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 /120V_AC))
    (pad 8 thru_hole circle (at 2.3 -10.1) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (model "/Users/sveit/Dropbox/Library/Application Support/kicad/packages3d/Relays.3dshapes/G5RL_1A_E_LN.igs"
      (at (xyz 0.0905511811023622 0.1019685039370079 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical (layer F.Cu) (tedit 5974D640)
    (at 53.34 73.025 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Vertical pin pitch 5.08mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R1 (at 2.667 3.048 180) (layer F.SilkS))
    (fp_text value 82k (at 2.54 3.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 52 /Light))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(R1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical (layer F.Cu) (tedit 5974D647)
    (at 53.34 79.121 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Vertical pin pitch 5.08mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at 2.667 3.175 180) (layer F.SilkS))
    (fp_text value 82k (at 2.54 3.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 /Motor_up))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical (layer F.Cu) (tedit 5974D64C)
    (at 53.34 85.217 180)
    (descr "Resistor, Axial_DIN0414 series, Axial, Vertical, pin pitch=5.08mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Vertical pin pitch 5.08mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R3 (at 2.667 3.175 180) (layer F.SilkS))
    (fp_text value 82k (at 2.54 3.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 /Motor_down))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(R3-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E2D)
    (at 76.327 44.704)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U4 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LTV-847 (at 3.81 20.17) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad8)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U4-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(RN2-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R4-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U4-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(RN2-Pad7)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(U4-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U4-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(U4-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(RN2-Pad8)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E2C)
    (at 91.44 43.053)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U7 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value SN7407N (at 3.81 17.63) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad6)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad5)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad11)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U4-Pad4)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(J3-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad13)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad16)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U4-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Wide_Oval_Reverse (layer F.Cu) (tedit 5974D616)
    (at 62.865 41.91 90)
    (descr "TO-92 leads molded, wide, reverse, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 6.096 -1.905 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 2.54 4.57 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.3 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.5 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 2.54 180) (size 2 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide_Oval_Reverse.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 59791D83)
    (at 63.754 66.04)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.143 -2.159 180) (layer F.SilkS))
    (fp_text value 1k (at 1.27 2.31) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E2D)
    (at 64.516 71.12)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U3 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LTV-844 (at 3.81 20.17) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(R6-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /Neutral))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(Q1-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R3-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad21)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /Neutral))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R2-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad23)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /Neutral))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R1-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad31)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(RN2-Pad5)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5973EBC6)
    (at 80.391 80.137 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 1.27 2.159 180) (layer F.SilkS))
    (fp_text value 47k (at 1.27 2.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R8-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5973EB9A)
    (at 80.391 75.819 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 1.27 2.159 180) (layer F.SilkS))
    (fp_text value 3.9k (at 1.27 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R9-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5973EB64)
    (at 80.391 67.183 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 1.143 2.159 180) (layer F.SilkS))
    (fp_text value 120k (at 1.27 2.31 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R10-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 58CC8E33)
    (at 91.44 83.947)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U6 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LM393 (at 3.81 10.01) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad37)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(R8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /Close_limit))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my-modules:MountingHoles (layer F.Cu) (tedit 59765E52)
    (at 36.5 96.5 90)
    (descr 3-1761603-3)
    (tags Connector)
    (fp_text reference M1 (at 16.51 0 90) (layer F.SilkS) hide)
    (fp_text value Mounting (at 8.89 0 90) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
    (pad "" np_thru_hole circle (at 58 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
  )
  (module Resistors_THT:R_Array_SIP8 (layer F.Cu) (tedit 57FA3974)
    (at 72.39 62.103 90)
    (descr "8-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 10.16 -2.4 90) (layer F.SilkS))
    (fp_text value 390 (at 10.16 2.4 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(RN2-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(RN2-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(RN2-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(RN2-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(J3-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(J3-Pad6)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Resistors_THT.3dshapes/R_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:IDC_Header_Straight_8pins (layer F.Cu) (tedit 597C99CE)
    (at 64.389 96.393)
    (descr "8 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J3 (at -3.175 -4.191) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 4 5) (layer F.Fab))
    (fp_text user 1 (at 0.02 1.72) (layer F.SilkS))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "Net-(J3-Pad8)"))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "Net-(J3-Pad6)"))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 /5V_OUT))
    (model "/Users/sveit/Dropbox/Library/Application Support/kicad/packages3d/Headers.3dshapes/702460801.stp"
      (at (xyz 0.1507874015748032 0.05078740157480315 0.2322834645669292))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module my-modules:HDRV40W79P254_2X20_5842X883X922P (layer F.Cu) (tedit 597E0E5A)
    (at 105.23 43.37 270)
    (descr 3-1761603-3)
    (tags Connector)
    (fp_text reference J2 (at -2.349 2.233) (layer F.SilkS))
    (fp_text value Adafruit-2823 (at 24.13 3.81 270) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 53.13 21.73 270) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
    (pad "" np_thru_hole circle (at -4.87 21.73 270) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
    (pad "" np_thru_hole circle (at 53.13 -1.27 270) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
    (pad "" np_thru_hole circle (at -4.87 -1.27 270) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.625) (clearance 1.625) (zone_connect 0) (thermal_width 1.625) (thermal_gap 1.625))
    (pad 1 thru_hole rect (at 0 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J2-Pad3)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J2-Pad5)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J2-Pad7)"))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad11)"))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad13)"))
    (pad 15 thru_hole circle (at 17.78 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J2-Pad15)"))
    (pad 17 thru_hole circle (at 20.32 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad17)"))
    (pad 19 thru_hole circle (at 22.86 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J2-Pad19)"))
    (pad 21 thru_hole circle (at 25.4 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J2-Pad21)"))
    (pad 23 thru_hole circle (at 27.94 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad23)"))
    (pad 25 thru_hole circle (at 30.48 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 27 thru_hole circle (at 33.02 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J2-Pad27)"))
    (pad 29 thru_hole circle (at 35.56 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 71 /lock))
    (pad 31 thru_hole circle (at 38.1 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J2-Pad31)"))
    (pad 33 thru_hole circle (at 40.64 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J2-Pad33)"))
    (pad 35 thru_hole circle (at 43.18 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 72 /door))
    (pad 37 thru_hole circle (at 45.72 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J2-Pad37)"))
    (pad 39 thru_hole circle (at 48.26 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad8)"))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad10)"))
    (pad 12 thru_hole circle (at 12.7 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad12)"))
    (pad 14 thru_hole circle (at 15.24 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 16 thru_hole circle (at 17.78 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad16)"))
    (pad 18 thru_hole circle (at 20.32 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad18)"))
    (pad 20 thru_hole circle (at 22.86 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 22 thru_hole circle (at 25.4 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 73 /light))
    (pad 24 thru_hole circle (at 27.94 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad24)"))
    (pad 26 thru_hole circle (at 30.48 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J2-Pad26)"))
    (pad 28 thru_hole circle (at 33.02 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad28)"))
    (pad 30 thru_hole circle (at 35.56 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 32 thru_hole circle (at 38.1 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad32)"))
    (pad 34 thru_hole circle (at 40.64 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 36 thru_hole circle (at 43.18 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J2-Pad36)"))
    (pad 38 thru_hole circle (at 45.72 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J2-Pad38)"))
    (pad 40 thru_hole circle (at 48.26 -2.54) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J2-Pad40)"))
    (model "/Users/sveit/Dropbox/Library/Application Support/kicad/packages3d/Headers.3dshapes/66953-020LF.igs"
      (at (xyz 0.9488188976377954 0.04960629921259843 -0.07874015748031496))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_arc (start 36 38) (end 33 38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107 38) (end 107 35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 107 97) (end 110 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 36 97) (end 36 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 33 38) (end 33 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107 35) (end 36 35) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 97) (end 110 38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 36 100) (end 107 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 96.52) (xy 80.391 96.52) (xy 80.391 99.568) (xy 86.487 99.568) (xy 86.487 93.472)
        (xy 80.391 93.472) (xy 80.391 96.52)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 38.481) (xy 86.487 38.481) (xy 86.487 41.529) (xy 80.518 41.529) (xy 80.518 35.56)
        (xy 86.487 35.56) (xy 86.487 38.481)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 38.481) (xy 83.439 35.56) (xy 86.487 35.56) (xy 86.487 38.481) (xy 86.487 41.529)
        (xy 80.518 41.529) (xy 80.518 35.56) (xy 83.439 35.56)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.439 96.52) (xy 83.439 93.472) (xy 86.487 93.472) (xy 86.487 99.568) (xy 80.391 99.568)
        (xy 80.391 93.472) (xy 83.439 93.472)
      )
    )
  )
)
