<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="1" y1="1" x2="33" y2="1" width="0" layer="20"/>
<wire x1="33" y1="1" x2="33" y2="33" width="0" layer="20"/>
<wire x1="33" y1="33" x2="1" y2="33" width="0" layer="20"/>
<wire x1="1" y1="33" x2="1" y2="1" width="0" layer="20"/>
<text>Hacker Badge R1</text>
<text>Designed at Noisebridge</text>
<text>Built by a hacker</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="CR1220-THM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="adafruit" package="CR1220-THM" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="+1"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="U$1" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
