(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 15)
    (no_connects 3)
    (area 139.238667 101.589 162.262154 124.371494)
    (thickness 1.6)
    (drawings 14)
    (tracks 78)
    (zones 0)
    (modules 6)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 CS)
  (net 4 SCLK)
  (net 5 MOSI)
  (net 6 MISO)
  (net 7 Z)
  (net 8 B)
  (net 9 A)
  (net 10 "Net-(U1-Pad1)")
  (net 11 "Net-(U1-Pad9)")
  (net 12 "Net-(U1-Pad10)")
  (net 13 "Net-(U1-Pad11)")
  (net 14 "Net-(U1-Pad14)")
  (net 15 "Net-(U1-Pad15)")
  (net 16 "Net-(U1-Pad16)")
  (net 17 "Net-(U1-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A)
    (add_net B)
    (add_net CS)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad9)")
    (add_net SCLK)
    (add_net VCC)
    (add_net Z)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57DB91D4)
    (at 148.59 106.8705)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.032 1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 57DC060E)
    (at 148.59 110.744 90)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 2.286 -2.032 180) (layer F.SilkS))
    (fp_text value MA700 (at 0 2.85 90) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad1)"))
    (pad 2 smd oval (at -1.475 -0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 A))
    (pad 3 smd oval (at -1.475 0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 Z))
    (pad 4 smd oval (at -1.475 0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 MOSI))
    (pad 5 smd oval (at -0.75 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 CS))
    (pad 6 smd oval (at -0.25 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 B))
    (pad 7 smd oval (at 0.25 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 MISO))
    (pad 8 smd oval (at 0.75 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd oval (at 1.475 0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad9)"))
    (pad 10 smd oval (at 1.475 0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad10)"))
    (pad 11 smd oval (at 1.475 -0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad11)"))
    (pad 12 smd oval (at 1.475 -0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SCLK))
    (pad 13 smd oval (at 0.75 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 14 smd oval (at 0.25 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad14)"))
    (pad 15 smd oval (at -0.25 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad15)"))
    (pad 16 smd oval (at -0.75 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 0.45 0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad17)") (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer B.Cu) (tedit 57DC0691)
    (at 152.908 105.664 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -1.016 -9.652 360) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 CS))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 SCLK))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 MOSI))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 MISO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer B.Cu) (tedit 57DC064D)
    (at 144.272 105.664 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -2.286 -11.43 360) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 Z))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 B))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 A))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 57DC09CD)
    (at 147.32 114.046)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference W1 (at -1.3208 -0.9652) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 16 "Net-(U1-Pad16)"))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 151.384 114.554 45)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (autoplace_cost90 4)
    (attr virtual)
    (fp_text reference REF*** (at 0 0 45) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 45) (layer F.Fab) hide)
  )
  (gr_text "MA700 Breakout\n9/16/16 - v1" (at 151.13 116.586) (layer B.SilkS))
  (gr_text GND (at 147.0025 105.6005) (layer B.SilkS))
  (gr_text CS (at 150.368 105.664) (layer B.SilkS))
  (gr_text SCLK (at 149.86 108.204) (layer B.SilkS))
  (gr_text MOSI (at 149.86 110.744) (layer B.SilkS))
  (gr_text MISO (at 149.86 113.538) (layer B.SilkS))
  (gr_text A (at 146.558 115.824) (layer B.SilkS))
  (gr_text B (at 146.558 113.284) (layer B.SilkS))
  (gr_text Z (at 146.558 110.744) (layer B.SilkS))
  (gr_text 3.3V (at 147.066 107.7595) (layer B.SilkS))
  (gr_line (start 154.94 117.602) (end 154.94 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 117.602) (end 154.94 117.602) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 103.632) (end 142.24 117.602) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 103.632) (end 142.24 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.622 112.776) (xy 146.558 112.776) (xy 146.558 108.712) (xy 150.622 108.712)
      )
    )
  )
)
