(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")

  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 213)
    (zones 0)
    (modules 41)
    (nets 29)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.7)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 PUMP_A)
  (net 5 "Net-(C3-Pad1)")
  (net 6 PUMP_B)
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C7-Pad1)")
  (net 11 "Net-(C8-Pad1)")
  (net 12 "Net-(C9-Pad1)")
  (net 13 "Net-(C10-Pad1)")
  (net 14 "Net-(C11-Pad1)")
  (net 15 VCC)
  (net 16 "Net-(D6-Pad1)")
  (net 17 "Net-(D7-Pad2)")
  (net 18 ICSPDAT)
  (net 19 ICSPCLK)
  (net 20 -MCLR)
  (net 21 RAW)
  (net 22 "Net-(Q2-Pad3)")
  (net 23 B+)
  (net 24 "Net-(R5-Pad1)")
  (net 25 LED_A)
  (net 26 "Net-(D10-Pad1)")
  (net 27 RNG)
  (net 28 LED_B)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net -MCLR)
    (add_net B+)
    (add_net GND)
    (add_net ICSPCLK)
    (add_net ICSPDAT)
    (add_net LED_A)
    (add_net LED_B)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(R5-Pad1)")
    (add_net PUMP_A)
    (add_net PUMP_B)
    (add_net RAW)
    (add_net RNG)
    (add_net VCC)
  )

  (module modules:POGO_5_PIN (layer F.Cu) (tedit 5CC02629) (tstamp 5CBFF693)
    (at 191.135 41.91)
    (path /5CD54106)
    (fp_text reference J2 (at -3.81 2.54) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value ICSP (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 5 smd circle (at 6.35 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 ICSPCLK))
    (pad 4 smd circle (at 3.81 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 ICSPDAT))
    (pad 3 smd circle (at 1.27 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd circle (at -1.27 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (pad 1 smd rect (at -3.81 2.54) (size 1.7 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 -MCLR))
  )

  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5CC03641) (tstamp 5CC058AA)
    (at 203.073 44.069)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0.254 0) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "" (at 0 3.5) (layer F.Fab) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.75 0) (layer F.CrtYd) (width 0.05))
    (fp_circle (center 0 0) (end 2.5 0) (layer Cmts.User) (width 0.15))
    (fp_text user "" (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03244) (tstamp 5CBFF582)
    (at 180.34 22.86 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5CBF1847)
    (attr smd)
    (fp_text reference D1 (at -0.0254 1.6764 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS20 (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC03187) (tstamp 5CBFF4B2)
    (at 182.626 37.211 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5BE3EB1D)
    (attr smd)
    (fp_text reference C1 (at 3.0226 -0.0254) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value .1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030A4) (tstamp 5CBFF4C3)
    (at 200.66 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAC0)
    (attr smd)
    (fp_text reference C2 (at 2.9464 -0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 3.2004 0 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 PUMP_A))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030A0) (tstamp 5CBFF4D4)
    (at 198.12 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAC6)
    (attr smd)
    (fp_text reference C3 (at 2.9464 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 PUMP_B))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030B2) (tstamp 5CBFF4E5)
    (at 195.58 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDACC)
    (attr smd)
    (fp_text reference C4 (at 2.9972 0 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 3.0988 -0.0508 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 PUMP_A))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030C8) (tstamp 5CBFF4F6)
    (at 193.04 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAD2)
    (attr smd)
    (fp_text reference C5 (at 2.9464 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 PUMP_B))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030C4) (tstamp 5CBFF507)
    (at 190.5 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAD8)
    (attr smd)
    (fp_text reference C6 (at 2.9464 -0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 PUMP_A))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030EF) (tstamp 5CBFF518)
    (at 187.96 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAE6)
    (attr smd)
    (fp_text reference C7 (at -2.8956 -0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 PUMP_B))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030DC) (tstamp 5CBFF529)
    (at 185.42 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAEC)
    (attr smd)
    (fp_text reference C8 (at 2.9464 -0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 PUMP_A))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC030D7) (tstamp 5CBFF53A)
    (at 182.88 29.21 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBEDAF2)
    (attr smd)
    (fp_text reference C9 (at 2.9464 0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 PUMP_B))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC03246) (tstamp 5CBFF54B)
    (at 177.8 22.86 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CBF2E0C)
    (attr smd)
    (fp_text reference C10 (at -0.1016 -1.4732 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC0327A) (tstamp 5CBFF55C)
    (at 167.64 34.29 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5BDE1924)
    (attr smd)
    (fp_text reference C11 (at -0.1524 1.6764 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5CC0314B) (tstamp 5CBFF56D)
    (at 201.93 36.83 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (path /5CC020D8)
    (attr smd)
    (fp_text reference C12 (at -2.9972 -0.0508 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value .1u (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.25 0.87) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.25 0.87) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end -2.25 0.87) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.25 -0.88) (end 2.25 -0.88) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.5 0.85) (end 0.5 0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.5 -0.85) (end -0.5 -0.85) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC031E5) (tstamp 5CBFF597)
    (at 200.66 22.86 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEC5C2)
    (attr smd)
    (fp_text reference D2 (at 1.8796 1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC031E9) (tstamp 5CBFF5AC)
    (at 195.58 22.86 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEC7AA)
    (attr smd)
    (fp_text reference D3 (at 1.8542 1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC0312C) (tstamp 5CBFF5C1)
    (at 190.5 22.86 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEC82C)
    (attr smd)
    (fp_text reference D4 (at 1.8288 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC0301B) (tstamp 5CBFF5D6)
    (at 185.42 22.86 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEC8B0)
    (attr smd)
    (fp_text reference D5 (at 1.8288 -1.27 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value BAS40 (at 0 2.5 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C9-Pad1)"))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5CC03263) (tstamp 5CBFF5EF)
    (at 173.99 29.21 90)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5BDDE369)
    (fp_text reference D6 (at 3.81 0.0254 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 20V (at 3.81 2.41 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 3.81 0 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.15 -1.28) (end 1.15 -1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 -1.41) (end 6.47 -1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.47 -1.41) (end 6.47 -1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 1.28) (end 1.15 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 1.41) (end 6.47 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.47 1.41) (end 6.47 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.41) (end 1.99 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -1.7) (end -1.35 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 1.7) (end 9 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9 1.7) (end 9 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9 -1.7) (end -1.35 -1.7) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module Diodes_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5CC03275) (tstamp 5CBFF608)
    (at 167.64 39.37)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (path /5BDE1880)
    (fp_text reference D7 (at 3.81 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10V (at 3.81 2.41) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 9 -1.7) (end -1.35 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 9 1.7) (end 9 -1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 1.7) (end 9 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 -1.7) (end -1.35 1.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.99 -1.41) (end 1.99 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.47 1.41) (end 6.47 1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 1.41) (end 6.47 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 1.28) (end 1.15 1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.47 -1.41) (end 6.47 -1.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 -1.41) (end 6.47 -1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.15 -1.28) (end 1.15 -1.41) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.99 -1.35) (end 1.99 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 7.62 0) (end 6.41 0) (layer F.Fab) (width 0.1))
    (fp_line (start 0 0) (end 1.21 0) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 -1.35) (end 1.21 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 6.41 1.35) (end 6.41 -1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 1.35) (end 6.41 1.35) (layer F.Fab) (width 0.1))
    (fp_line (start 1.21 -1.35) (end 1.21 1.35) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 3.81 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 2 thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E) (tstamp 5CBFF61D)
    (at 199.2376 26.162)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEB010)
    (attr smd)
    (fp_text reference D8 (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BAS40 (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.7 1.75) (end 2.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end -2.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 VCC))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 PUMP_A))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E) (tstamp 5CBFF632)
    (at 187.706 26.0604)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CBEB58A)
    (attr smd)
    (fp_text reference D9 (at 0 2.5) (layer B.SilkS)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value BAS40 (at 0 -2.5) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start 0.76 -1.58) (end -0.7 -1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -0.7 -1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start 0.7 1.52) (end 0.7 -1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.15 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.15 1.52) (end 0.7 1.52) (layer B.Fab) (width 0.1))
    (fp_line (start -0.7 0.95) (end -0.7 -1.5) (layer B.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -2.4 1.58) (layer B.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end -2.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end -2.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end 2.7 -1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end 2.7 1.75) (layer B.CrtYd) (width 0.05))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer B.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer B.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 -90) (layer B.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)) (justify mirror))
    )
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 PUMP_B))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 VCC))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5CC031CB) (tstamp 5CBFF647)
    (at 204.47 22.86 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5CBE34BC)
    (attr smd)
    (fp_text reference D10 (at -0.0254 1.397 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value GRN (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -0.75) (end -2.2 0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -0.75) (end 1 -0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 0.75) (end -2.2 0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 LED_A))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 5CC031CF) (tstamp 5CBFF65C)
    (at 204.47 29.21 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5CC07FB3)
    (attr smd)
    (fp_text reference D11 (at -0.1016 1.4986 270) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value RED (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.2 -0.75) (end -2.2 0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -0.75) (end 1 -0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 1 0.75) (end -2.2 0.75) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 -0.4) (end 0.2 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.2 0.4) (end -0.4 0) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 0) (end 0.2 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.4 -0.4) (end -0.4 0.4) (layer F.Fab) (width 0.1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D10-Pad1)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 LED_A))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CC0C252) (tstamp 5CBFF6A8)
    (at 188.214 33.274)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (path /5CC0AE66)
    (fp_text reference J3 (at -0.1016 0.1016) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TP1 (at 0 2.33) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_text user TP1 (at -2.7432 0.6223 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 RAW))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC03251) (tstamp 5CBFF6D2)
    (at 178.7144 30.9372)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5CC37484)
    (attr smd)
    (fp_text reference Q1 (at 1.9304 -1.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2N2222 (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5CC03184) (tstamp 5CBFF6E7)
    (at 179.07 36.83 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (path /5BDE175C)
    (attr smd)
    (fp_text reference Q2 (at -3.429 0.0762 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2N2222 (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start 0.76 1.58) (end 0.76 0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.76 -1.58) (end 0.76 -0.65) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.7 -1.75) (end 2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 -1.75) (end 2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.7 1.75) (end -2.7 1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.7 1.75) (end -2.7 -1.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.76 -1.58) (end -2.4 -1.58) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.7 -0.95) (end -0.7 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.15 -1.52) (end 0.7 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 -0.95) (end -0.15 -1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.7 -1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start -0.7 1.52) (end 0.7 1.52) (layer F.Fab) (width 0.1))
    (fp_line (start 0.76 1.58) (end -0.7 1.58) (layer F.SilkS) (width 0.12))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC0332F) (tstamp 5CBFF6F8)
    (at 170.18 28.448 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDD0039)
    (attr smd)
    (fp_text reference R1 (at -3.0099 0.1397 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 B+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC0333C) (tstamp 5CBFF709)
    (at 170.18 22.86 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDD0133)
    (attr smd)
    (fp_text reference R2 (at -2.8067 -0.0254 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10K (at 0 1.75 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 B+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03255) (tstamp 5CBFF71A)
    (at 179.0192 27.0764)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5CC4C53E)
    (attr smd)
    (fp_text reference R3 (at 0.1016 -1.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100K (at 0 1.75) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC0326E) (tstamp 5CBFF72B)
    (at 172.72 33.02 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDE1BD7)
    (attr smd)
    (fp_text reference R4 (at -3.3528 -0.2032 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 15K (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03322) (tstamp 5CBFF73C)
    (at 167.64 28.448 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDE7D9F)
    (attr smd)
    (fp_text reference R5 (at 2.9972 -0.0381) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 150K (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03191) (tstamp 5CBFF74D)
    (at 189.23 37.211 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDEB83A)
    (attr smd)
    (fp_text reference R6 (at 3.1242 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 2.2K (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 RAW))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03271) (tstamp 5CBFF75E)
    (at 172.72 35.56 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDE17D0)
    (attr smd)
    (fp_text reference R7 (at -3.3528 -0.0508 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 10K (at 0 1.75 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC03337) (tstamp 5CBFF76F)
    (at 167.64 22.86 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5BDE7E15)
    (attr smd)
    (fp_text reference R8 (at 2.8067 -0.0635) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 100K (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5CC0314F) (tstamp 5CBFF780)
    (at 204.47 36.83 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (path /5CD60CEF)
    (attr smd)
    (fp_text reference R9 (at -2.9972 0.0508) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 1K (at 0 1.75 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.35 0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.35 0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end -2.35 0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.35 -0.9) (end 2.35 -0.9) (layer F.CrtYd) (width 0.05))
    (fp_line (start -0.6 -0.88) (end 0.6 -0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.6 0.88) (end -0.6 0.88) (layer F.SilkS) (width 0.12))
    (fp_line (start -1 -0.62) (end 1 -0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 -0.62) (end 1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start 1 0.62) (end -1 0.62) (layer F.Fab) (width 0.1))
    (fp_line (start -1 0.62) (end -1 -0.62) (layer F.Fab) (width 0.1))
    (fp_text user %R (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 LED_B))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5CC0318D) (tstamp 5CBFF7B7)
    (at 185.928 37.211 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (path /5BDE16C6)
    (attr smd)
    (fp_text reference U1 (at -3.1496 0.1524 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TL331 (at 0 2.9 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 2.38 1.8) (end -2.38 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.38 1.8) (end 2.38 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.38 -1.8) (end -2.38 1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.38 -1.8) (end 2.38 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.9 -1.55) (end 0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 1.55) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.9 1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.55) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -0.9) (end -0.25 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 0.9 -1.61) (end -1.55 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.9 1.61) (end 0.9 1.61) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 180) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 5 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 RAW))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 5CC031A1) (tstamp 5CBFF7DA)
    (at 195.58 36.83 270)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (path /5CC01B75)
    (attr smd)
    (fp_text reference U2 (at 4.4704 -0.254) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value PIC16F1615 (at 0 5.375 270) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.075 -4.425) (end -3.45 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end 2.075 4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end 2.075 -4.45) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 4.45) (end -2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 4.45) (end 2.075 4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.075 -4.45) (end 2.075 -4.335) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.075 -4.45) (end -2.075 -4.425) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.7 4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end 3.7 -4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -4.65) (end 3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 -4.65) (end -3.7 4.65) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.95 -3.35) (end -0.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -1.95 4.35) (end -1.95 -3.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 4.35) (end -1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start 1.95 -4.35) (end 1.95 4.35) (layer F.Fab) (width 0.15))
    (fp_line (start -0.95 -4.35) (end 1.95 -4.35) (layer F.Fab) (width 0.15))
    (fp_text user "" (at 0 0 270) (layer F.Fab)
      (effects (font (size 0.9 0.9) (thickness 0.135)))
    )
    (pad 14 smd rect (at 2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 ICSPDAT))
    (pad 12 smd rect (at 2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 ICSPCLK))
    (pad 11 smd rect (at 2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 RNG))
    (pad 10 smd rect (at 2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 RNG))
    (pad 9 smd rect (at 2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 LED_A))
    (pad 8 smd rect (at 2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 LED_B))
    (pad 7 smd rect (at -2.7 3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 RAW))
    (pad 6 smd rect (at -2.7 2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 PUMP_A))
    (pad 5 smd rect (at -2.7 1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 PUMP_B))
    (pad 4 smd rect (at -2.7 0 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 -MCLR))
    (pad 3 smd rect (at -2.7 -1.27 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 B+))
    (pad 2 smd rect (at -2.7 -2.54 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.7 -3.81 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 VCC))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5CC03646) (tstamp 5CC05544)
    (at 168.91 44.069)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0.254 0) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "" (at 0 3.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "" (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.5 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.75 0) (layer F.CrtYd) (width 0.05))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )

  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5CC02427) (tstamp 5CC0BC8C)
    (at 175.895 44.45 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /5CC06385)
    (fp_text reference J1 (at -0.0508 -2.7432 180) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 0.1" (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81 180) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 LED_A))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 RNG))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text OK (at 183.4134 42.1132) (layer B.SilkS) (tstamp 5CC040C5)
    (effects (font (size 0.75 0.75) (thickness 0.1875)) (justify mirror))
  )
  (gr_text OUT (at 181.0004 42.1259) (layer B.SilkS) (tstamp 5CC040C1)
    (effects (font (size 0.75 0.75) (thickness 0.1875)) (justify mirror))
  )
  (gr_text GND (at 178.3715 42.0751) (layer B.SilkS) (tstamp 5CC040BF)
    (effects (font (size 0.75 0.75) (thickness 0.1875)) (justify mirror))
  )
  (gr_text VCC (at 175.6664 42.1132) (layer B.SilkS) (tstamp 5CC040BD)
    (effects (font (size 0.75 0.75) (thickness 0.1875)) (justify mirror))
  )
  (gr_circle (center 188.5315 44.2722) (end 190.303366 44.2722) (layer B.SilkS) (width 0.3))
  (gr_text - (at 188.4934 44.1452) (layer B.SilkS)
    (effects (font (size 2 2) (thickness 0.5)) (justify mirror))
  )
  (gr_text Z (at 188.4807 44.3738) (layer B.SilkS)
    (effects (font (size 2 2) (thickness 0.5)) (justify mirror))
  )
  (gr_line (start 202.9714 30.7848) (end 203.5429 31.3182) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 202.4126 31.3309) (end 202.9714 30.7848) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 203.5556 31.3309) (end 202.4126 31.3309) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 203.0349 24.511) (end 203.5556 25.019) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 202.5777 25.0317) (end 203.0349 24.511) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 203.5556 25.0317) (end 202.5777 25.0317) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_text J422 (at 196.4944 44.4881) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_text "Random Generator" (at 188.3664 21.9075) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.3)) (justify mirror))
  )
  (gr_line (start 181.9783 21.4884) (end 181.4576 21.0185) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 182.4736 21.0185) (end 181.9783 21.4884) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 181.4449 21.0185) (end 182.4736 21.0185) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_text OK (at 183.4515 42.1259) (layer F.SilkS) (tstamp 5CC1341D)
    (effects (font (size 0.75 0.75) (thickness 0.1875)))
  )
  (gr_text OUT (at 180.9877 42.1005) (layer F.SilkS) (tstamp 5CC13418)
    (effects (font (size 0.75 0.75) (thickness 0.1875)))
  )
  (gr_text GND (at 178.3842 42.0878) (layer F.SilkS) (tstamp 5CC13414)
    (effects (font (size 0.75 0.75) (thickness 0.1875)))
  )
  (gr_text VCC (at 175.6664 42.0878) (layer F.SilkS)
    (effects (font (size 0.75 0.75) (thickness 0.1875)))
  )
  (gr_line (start 200.025 34.798) (end 199.9996 33.401) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 200.8378 34.0614) (end 200.025 34.798) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 200.0504 33.3756) (end 200.8378 34.0614) (angle 90) (layer F.SilkS) (width 0.2))
  (gr_line (start 206 47) (end 166 47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206 20) (end 206 47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 20) (end 206 20) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166 47) (end 166 20) (angle 90) (layer Edge.Cuts) (width 0.15))

  (segment (start 167.64 21.51) (end 170.18 21.51) (width 0.635) (layer F.Cu) (net 1) (status C00000))
  (segment (start 170.18 21.51) (end 173.91 21.51) (width 0.635) (layer F.Cu) (net 1) (tstamp 5CC100B6) (status C00000))
  (segment (start 173.91 21.51) (end 173.99 21.59) (width 0.635) (layer F.Cu) (net 1) (tstamp 5CC100B7) (status C00000))
  (segment (start 167.64 33.04) (end 167.66 33.02) (width 0.635) (layer F.Cu) (net 1) (status C00000))
  (via (at 168.656 33.02) (size 1) (drill 0.7) (layers F.Cu B.Cu) (net 1))
  (segment (start 167.66 33.02) (end 168.656 33.02) (width 0.635) (layer F.Cu) (net 1) (tstamp 5CC100BC) (status 400000))
  (segment (start 180.02 38.33) (end 180.02 39.558) (width 0.381) (layer F.Cu) (net 1) (status 400000))
  (via (at 180.0352 39.5732) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 180.02 39.558) (end 180.0352 39.5732) (width 0.381) (layer F.Cu) (net 1) (tstamp 5CC102F0))
  (via (at 192.405 44.45) (size 1) (drill 0.7) (layers F.Cu B.Cu) (net 1) (status C00000))
  (segment (start 192.405 44.45) (end 192.4304 44.45) (width 0.381) (layer B.Cu) (net 1) (tstamp 5CC103A1) (status 400000))
  (segment (start 201.93 38.08) (end 201.93 39.0652) (width 0.381) (layer F.Cu) (net 1) (status 400000))
  (via (at 201.93 39.0652) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 199.39 39.53) (end 199.39 38.5064) (width 0.381) (layer F.Cu) (net 1) (status 400000))
  (via (at 199.39 38.5064) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 185.928 38.561) (end 185.928 39.5732) (width 0.381) (layer F.Cu) (net 1) (status 400000))
  (via (at 182.6768 39.5224) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 1))
  (segment (start 182.6768 38.5118) (end 182.6768 39.5224) (width 0.381) (layer F.Cu) (net 1) (tstamp 5CC12D36) (status 400000))
  (segment (start 182.6768 38.5118) (end 182.626 38.461) (width 0.381) (layer F.Cu) (net 1) (status C00000))
  (segment (start 185.928 39.5732) (end 185.6232 39.878) (width 0.381) (layer F.Cu) (net 1) (tstamp 5CC12D31))
  (segment (start 185.6232 39.878) (end 183.0324 39.878) (width 0.381) (layer F.Cu) (net 1) (tstamp 5CC12D32))
  (segment (start 183.0324 39.878) (end 182.6768 39.5224) (width 0.381) (layer F.Cu) (net 1) (tstamp 5CC12D33))
  (segment (start 173.99 21.59) (end 174.01 21.61) (width 0.635) (layer F.Cu) (net 1) (status C00000))
  (segment (start 174.01 21.61) (end 177.8 21.61) (width 0.635) (layer F.Cu) (net 1) (tstamp 5CC12D42) (status C00000))
  (segment (start 167.64 29.798) (end 170.18 29.798) (width 0.381) (layer F.Cu) (net 2) (status C00000))
  (segment (start 170.18 29.798) (end 171.37 30.988) (width 0.381) (layer F.Cu) (net 2) (status 400000))
  (segment (start 171.37 30.988) (end 171.37 31.3436) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC03201))
  (segment (start 171.37 31.3436) (end 171.37 33.02) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC03207) (status 800000))
  (segment (start 177.2144 31.8872) (end 176.6708 31.3436) (width 0.381) (layer F.Cu) (net 2) (status 400000))
  (segment (start 176.6708 31.3436) (end 171.37 31.3436) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC03204))
  (segment (start 177.2144 31.8872) (end 178.6012 33.274) (width 0.381) (layer F.Cu) (net 2) (status 400000))
  (segment (start 182.626 34.798) (end 182.626 35.961) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC05EF2) (status 800000))
  (segment (start 181.102 33.274) (end 182.626 34.798) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC05EF1))
  (segment (start 178.6012 33.274) (end 181.102 33.274) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC05EF0))
  (segment (start 184.978 35.861) (end 182.726 35.861) (width 0.381) (layer F.Cu) (net 2) (status C00000))
  (segment (start 182.726 35.861) (end 182.626 35.961) (width 0.381) (layer F.Cu) (net 2) (tstamp 5CC05EF5) (status C00000))
  (segment (start 200.66 27.96) (end 200.66 24.36) (width 0.381) (layer F.Cu) (net 3) (status C00000))
  (segment (start 200.66 30.46) (end 200.66 31.4452) (width 0.381) (layer F.Cu) (net 4) (status 400000))
  (segment (start 195.58 31.4452) (end 195.58 30.46) (width 0.381) (layer F.Cu) (net 4) (tstamp 5CC03729) (status 800000))
  (via (at 195.58 31.4452) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 200.66 31.4452) (end 195.58 31.4452) (width 0.381) (layer B.Cu) (net 4) (tstamp 5CC03726))
  (via (at 200.66 31.4452) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 195.58 31.4452) (end 190.5 31.4452) (width 0.381) (layer B.Cu) (net 4))
  (segment (start 190.5 31.4452) (end 190.5 30.46) (width 0.381) (layer F.Cu) (net 4) (tstamp 5CC0372F) (status 800000))
  (via (at 190.5 31.4452) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 190.5 31.4452) (end 185.42 31.4452) (width 0.381) (layer B.Cu) (net 4))
  (via (at 185.42 31.4452) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 4))
  (segment (start 185.42 31.4452) (end 185.42 30.46) (width 0.381) (layer F.Cu) (net 4) (tstamp 5CC03734) (status 800000))
  (segment (start 193.04 34.13) (end 193.04 33.02) (width 0.381) (layer F.Cu) (net 4) (status 400000))
  (segment (start 191.4652 31.4452) (end 190.5 31.4452) (width 0.381) (layer F.Cu) (net 4) (tstamp 5CC05F0B))
  (segment (start 193.04 33.02) (end 191.4652 31.4452) (width 0.381) (layer F.Cu) (net 4) (tstamp 5CC05F0A))
  (segment (start 200.66 31.4452) (end 200.7376 31.3676) (width 0.381) (layer B.Cu) (net 4))
  (segment (start 200.7376 31.3676) (end 200.7376 26.162) (width 0.381) (layer B.Cu) (net 4) (tstamp 5CC12D20) (status 800000))
  (segment (start 196.53 21.36) (end 198.12 21.36) (width 0.381) (layer F.Cu) (net 5) (status 400000))
  (segment (start 198.12 21.36) (end 199.71 21.36) (width 0.381) (layer F.Cu) (net 5) (tstamp 5CC00653) (status 800000))
  (segment (start 198.12 27.96) (end 198.12 21.36) (width 0.381) (layer F.Cu) (net 5) (status 400000))
  (segment (start 198.12 21.36) (end 198.12 21.336) (width 0.381) (layer F.Cu) (net 5) (tstamp 5CC0064E))
  (segment (start 198.12 21.336) (end 198.12 21.36) (width 0.381) (layer F.Cu) (net 5) (tstamp 5CC00652))
  (segment (start 182.88 30.46) (end 183.7744 30.46) (width 0.381) (layer F.Cu) (net 6) (status 400000))
  (segment (start 188.8436 30.46) (end 187.96 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC0375C) (status 800000))
  (segment (start 188.8744 30.4292) (end 188.8436 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC0375B))
  (via (at 188.8744 30.4292) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 183.8452 30.4292) (end 188.8744 30.4292) (width 0.381) (layer B.Cu) (net 6) (tstamp 5CC03759))
  (segment (start 183.7944 30.48) (end 183.8452 30.4292) (width 0.381) (layer B.Cu) (net 6) (tstamp 5CC03758))
  (via (at 183.7944 30.48) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 183.7744 30.46) (end 183.7944 30.48) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC03756))
  (segment (start 188.8744 30.4292) (end 193.9544 30.4292) (width 0.381) (layer B.Cu) (net 6))
  (segment (start 193.9236 30.46) (end 193.04 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC03762) (status 800000))
  (segment (start 193.9544 30.4292) (end 193.9236 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC03761))
  (via (at 193.9544 30.4292) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 193.9544 30.4292) (end 199.0344 30.4292) (width 0.381) (layer B.Cu) (net 6))
  (segment (start 199.0036 30.46) (end 198.12 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC03768) (status 800000))
  (segment (start 199.0344 30.4292) (end 199.0036 30.46) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC03767))
  (via (at 199.0344 30.4292) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 194.31 34.13) (end 194.31 30.7848) (width 0.381) (layer F.Cu) (net 6) (status 400000))
  (segment (start 194.31 30.7848) (end 193.9544 30.4292) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC05F05))
  (segment (start 189.23 26.0844) (end 189.206 26.0604) (width 0.381) (layer B.Cu) (net 6) (tstamp 5CC12D1D) (status C00000))
  (segment (start 189.23 26.7208) (end 189.23 26.0844) (width 0.381) (layer B.Cu) (net 6) (tstamp 5CC12D1C) (status 800000))
  (via (at 189.23 26.7208) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 6))
  (segment (start 189.23 30.0736) (end 189.23 26.7208) (width 0.381) (layer F.Cu) (net 6) (tstamp 5CC12D1A))
  (segment (start 188.8744 30.4292) (end 189.23 30.0736) (width 0.381) (layer F.Cu) (net 6))
  (segment (start 195.58 27.96) (end 195.58 24.36) (width 0.381) (layer F.Cu) (net 7) (status C00000))
  (segment (start 194.63 21.36) (end 193.04 21.36) (width 0.381) (layer F.Cu) (net 8) (status 400000))
  (segment (start 193.04 21.36) (end 191.45 21.36) (width 0.381) (layer F.Cu) (net 8) (tstamp 5CC00659) (status 800000))
  (segment (start 193.04 27.96) (end 193.04 21.36) (width 0.381) (layer F.Cu) (net 8) (status 400000))
  (segment (start 193.04 21.36) (end 193.04 21.4884) (width 0.381) (layer F.Cu) (net 8) (tstamp 5CC00655))
  (segment (start 193.04 21.4884) (end 193.04 21.36) (width 0.381) (layer F.Cu) (net 8) (tstamp 5CC00658))
  (segment (start 190.5 27.96) (end 190.5 24.36) (width 0.381) (layer F.Cu) (net 9) (status C00000))
  (segment (start 189.55 21.36) (end 187.96 21.36) (width 0.381) (layer F.Cu) (net 10) (status 400000))
  (segment (start 187.96 21.36) (end 186.37 21.36) (width 0.381) (layer F.Cu) (net 10) (tstamp 5CC00661) (status 800000))
  (segment (start 187.96 27.96) (end 187.96 21.36) (width 0.381) (layer F.Cu) (net 10) (status 400000))
  (segment (start 185.42 27.96) (end 185.42 24.36) (width 0.381) (layer F.Cu) (net 11) (status C00000))
  (segment (start 182.88 27.96) (end 182.88 22.95) (width 0.381) (layer F.Cu) (net 12) (status 400000))
  (segment (start 182.88 22.95) (end 184.47 21.36) (width 0.381) (layer F.Cu) (net 12) (tstamp 5CC005F2) (status 800000))
  (segment (start 180.34 21.51) (end 181.44 21.51) (width 0.381) (layer F.Cu) (net 12) (status 400000))
  (segment (start 181.44 21.51) (end 182.88 22.95) (width 0.381) (layer F.Cu) (net 12) (tstamp 5CC0213C))
  (segment (start 180.2144 30.9372) (end 180.3692 30.7824) (width 0.381) (layer F.Cu) (net 13) (status C00000))
  (segment (start 180.3692 30.7824) (end 180.3692 27.0764) (width 0.381) (layer F.Cu) (net 13) (tstamp 5CC02145) (status C00000))
  (segment (start 180.34 24.21) (end 180.24 24.11) (width 0.381) (layer F.Cu) (net 13) (status C00000))
  (segment (start 180.24 24.11) (end 177.8 24.11) (width 0.381) (layer F.Cu) (net 13) (tstamp 5CC02148) (status C00000))
  (segment (start 180.34 24.21) (end 180.3692 24.2392) (width 0.381) (layer F.Cu) (net 13) (status C00000))
  (segment (start 180.3692 24.2392) (end 180.3692 27.0764) (width 0.381) (layer F.Cu) (net 13) (tstamp 5CC0214B) (status C00000))
  (segment (start 167.64 39.37) (end 167.64 35.54) (width 0.381) (layer F.Cu) (net 14) (status C00000))
  (segment (start 167.64 35.54) (end 167.66 35.56) (width 0.381) (layer F.Cu) (net 14) (status C00000))
  (segment (start 167.66 35.56) (end 171.37 35.56) (width 0.381) (layer F.Cu) (net 14) (tstamp 5CC031BB) (status C00000))
  (segment (start 197.7376 25.212) (end 198.4604 25.212) (width 0.381) (layer B.Cu) (net 15) (status C00000))
  (segment (start 202.1572 21.36) (end 201.61 21.36) (width 0.381) (layer F.Cu) (net 15) (tstamp 5CC12D0E) (status 800000))
  (segment (start 202.2348 21.4376) (end 202.1572 21.36) (width 0.381) (layer F.Cu) (net 15) (tstamp 5CC12D0D))
  (via (at 202.2348 21.4376) (size 1) (drill 0.7) (layers F.Cu B.Cu) (net 15))
  (segment (start 198.4604 25.212) (end 202.2348 21.4376) (width 0.381) (layer B.Cu) (net 15) (tstamp 5CC12D0B) (status 400000))
  (segment (start 197.636 25.1104) (end 197.7376 25.212) (width 0.381) (layer B.Cu) (net 15) (tstamp 5CC12D08) (status C00000))
  (segment (start 186.206 25.1104) (end 197.636 25.1104) (width 0.381) (layer B.Cu) (net 15) (status C00000))
  (segment (start 177.2144 29.9872) (end 177.2144 28.5496) (width 0.381) (layer F.Cu) (net 16) (status 400000))
  (segment (start 177.2144 28.5496) (end 177.2144 27.5312) (width 0.381) (layer F.Cu) (net 16) (tstamp 5CC02156) (status 800000))
  (segment (start 177.2144 27.5312) (end 177.6692 27.0764) (width 0.381) (layer F.Cu) (net 16) (tstamp 5CC02142) (status C00000))
  (segment (start 173.99 29.21) (end 174.6504 28.5496) (width 0.381) (layer F.Cu) (net 16) (status C00000))
  (segment (start 174.6504 28.5496) (end 177.2144 28.5496) (width 0.381) (layer F.Cu) (net 16) (tstamp 5CC02153) (status 400000))
  (segment (start 178.12 38.33) (end 177.08 39.37) (width 0.381) (layer F.Cu) (net 17) (status 400000))
  (segment (start 177.08 39.37) (end 175.26 39.37) (width 0.381) (layer F.Cu) (net 17) (tstamp 5CC031C7) (status 800000))
  (segment (start 194.945 44.45) (end 194.945 42.9514) (width 0.381) (layer F.Cu) (net 18) (status 400000))
  (segment (start 198.12 42.2656) (end 198.12 39.53) (width 0.381) (layer F.Cu) (net 18) (tstamp 5CC102CE) (status 800000))
  (via (at 198.12 42.2656) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 18))
  (segment (start 195.6308 42.2656) (end 198.12 42.2656) (width 0.381) (layer B.Cu) (net 18) (tstamp 5CC102CB))
  (via (at 195.6308 42.2656) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 18))
  (segment (start 194.945 42.9514) (end 195.6308 42.2656) (width 0.381) (layer F.Cu) (net 18) (tstamp 5CC102C9))
  (segment (start 196.85 39.53) (end 196.85 43.815) (width 0.381) (layer F.Cu) (net 19) (status 400000))
  (segment (start 196.85 43.815) (end 197.485 44.45) (width 0.381) (layer F.Cu) (net 19) (tstamp 5CC102C6) (status 800000))
  (segment (start 195.58 34.13) (end 195.58 35.3568) (width 0.381) (layer F.Cu) (net 20) (tstamp 5CC0D043) (status 400000))
  (segment (start 190.754 41.021) (end 187.325 44.45) (width 0.381) (layer F.Cu) (net 20) (tstamp 5CC102C2) (status 800000))
  (segment (start 190.754 36.7792) (end 190.754 41.021) (width 0.381) (layer F.Cu) (net 20))
  (segment (start 190.754 36.7792) (end 191.6176 35.9156) (width 0.381) (layer F.Cu) (net 20) (tstamp 5CC0D040))
  (segment (start 191.6176 35.9156) (end 195.0212 35.9156) (width 0.381) (layer F.Cu) (net 20) (tstamp 5CC0D041))
  (segment (start 195.0212 35.9156) (end 195.58 35.3568) (width 0.381) (layer F.Cu) (net 20) (tstamp 5CC0D042))
  (segment (start 186.878 35.861) (end 189.23 35.861) (width 0.381) (layer F.Cu) (net 21) (status C00000))
  (segment (start 191.77 34.13) (end 190.961 34.13) (width 0.381) (layer F.Cu) (net 21) (status 400000))
  (segment (start 190.961 34.13) (end 190.42 34.671) (width 0.381) (layer F.Cu) (net 21) (tstamp 5CC05EFA))
  (segment (start 190.42 34.671) (end 189.23 35.861) (width 0.381) (layer F.Cu) (net 21) (tstamp 5CC05F00) (status 800000))
  (segment (start 188.214 33.274) (end 189.023 33.274) (width 0.381) (layer F.Cu) (net 21) (status C00000))
  (segment (start 189.023 33.274) (end 190.42 34.671) (width 0.381) (layer F.Cu) (net 21) (tstamp 5CC05EFD) (status 400000))
  (segment (start 174.07 33.02) (end 174.07 35.56) (width 0.381) (layer F.Cu) (net 22) (status C00000))
  (segment (start 174.07 35.56) (end 174.3 35.33) (width 0.381) (layer F.Cu) (net 22) (status C00000))
  (segment (start 174.3 35.33) (end 179.07 35.33) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC031C4) (status C00000))
  (segment (start 179.07 35.33) (end 180.491 35.33) (width 0.381) (layer F.Cu) (net 22) (status 400000))
  (segment (start 186.878 40.071) (end 186.878 38.561) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F30) (status 800000))
  (segment (start 186.3344 40.6146) (end 186.878 40.071) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F2F))
  (segment (start 182.4736 40.6146) (end 186.3344 40.6146) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F2E))
  (segment (start 181.356 39.497) (end 182.4736 40.6146) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F2D))
  (segment (start 181.356 36.195) (end 181.356 39.497) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F2C))
  (segment (start 180.491 35.33) (end 181.356 36.195) (width 0.381) (layer F.Cu) (net 22) (tstamp 5CC05F2B))
  (segment (start 170.18 24.21) (end 170.18 27.098) (width 0.381) (layer F.Cu) (net 23) (status C00000))
  (segment (start 170.18 27.098) (end 171.243 27.098) (width 0.381) (layer F.Cu) (net 23) (status 400000))
  (segment (start 196.85 33.147) (end 196.85 34.13) (width 0.381) (layer F.Cu) (net 23) (tstamp 5CC05F1A) (status 800000))
  (via (at 196.85 33.147) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 23))
  (segment (start 195.199 33.147) (end 196.85 33.147) (width 0.381) (layer B.Cu) (net 23) (tstamp 5CC05F17))
  (segment (start 193.294 35.052) (end 195.199 33.147) (width 0.381) (layer B.Cu) (net 23) (tstamp 5CC05F15))
  (segment (start 176.403 35.052) (end 193.294 35.052) (width 0.381) (layer B.Cu) (net 23) (tstamp 5CC05F13))
  (segment (start 171.958 30.607) (end 176.403 35.052) (width 0.381) (layer B.Cu) (net 23) (tstamp 5CC05F12))
  (segment (start 171.958 29.591) (end 171.958 30.607) (width 0.381) (layer B.Cu) (net 23) (tstamp 5CC05F11))
  (via (at 171.958 29.591) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 23))
  (segment (start 171.958 27.813) (end 171.958 29.591) (width 0.381) (layer F.Cu) (net 23) (tstamp 5CC05F0F))
  (segment (start 171.243 27.098) (end 171.958 27.813) (width 0.381) (layer F.Cu) (net 23) (tstamp 5CC05F0E))
  (segment (start 167.64 24.21) (end 167.64 27.225) (width 0.381) (layer F.Cu) (net 24) (status C00000))
  (segment (start 167.64 27.098) (end 168.576 27.098) (width 0.381) (layer F.Cu) (net 24) (status 400000))
  (segment (start 184.451 38.561) (end 184.978 38.561) (width 0.381) (layer F.Cu) (net 24) (tstamp 5CC05F28) (status 800000))
  (segment (start 184.404 38.608) (end 184.451 38.561) (width 0.381) (layer F.Cu) (net 24) (tstamp 5CC05F27))
  (via (at 184.404 38.608) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 24))
  (segment (start 181.991 36.195) (end 184.404 38.608) (width 0.381) (layer B.Cu) (net 24) (tstamp 5CC05F24))
  (segment (start 176.022 36.195) (end 181.991 36.195) (width 0.381) (layer B.Cu) (net 24) (tstamp 5CC05F22))
  (segment (start 168.656 28.829) (end 176.022 36.195) (width 0.381) (layer B.Cu) (net 24) (tstamp 5CC05F20))
  (segment (start 168.656 27.178) (end 168.656 28.829) (width 0.381) (layer B.Cu) (net 24) (tstamp 5CC05F1F))
  (via (at 168.656 27.178) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 24))
  (segment (start 168.576 27.098) (end 168.656 27.178) (width 0.381) (layer F.Cu) (net 24) (tstamp 5CC05F1D))
  (segment (start 204.47 27.86) (end 204.47 26.5176) (width 0.381) (layer F.Cu) (net 25) (status 400000))
  (segment (start 204.47 26.5176) (end 204.47 26.1112) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC12D75))
  (segment (start 204.47 26.1112) (end 204.47 24.21) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC0D065) (status 800000))
  (via (at 193.04 42.2148) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 25))
  (segment (start 193.04 42.2148) (end 193.04 39.53) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC0CF09) (status 800000))
  (segment (start 193.04 42.2148) (end 185.7502 42.2148) (width 0.381) (layer B.Cu) (net 25))
  (segment (start 183.515 44.45) (end 185.7502 42.2148) (width 0.381) (layer B.Cu) (net 25) (tstamp 5CC102DE) (status 400000))
  (via (at 198.0184 35.7632) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 25))
  (segment (start 204.47 26.5176) (end 204.8256 26.5176) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC12D71))
  (via (at 204.8256 26.5176) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 25))
  (segment (start 204.8256 31.1912) (end 204.8256 26.5176) (width 0.381) (layer B.Cu) (net 25) (tstamp 5CC12D6E))
  (segment (start 202.8444 33.1724) (end 204.8256 31.1912) (width 0.381) (layer B.Cu) (net 25))
  (segment (start 198.0184 35.7632) (end 198.0184 34.1376) (width 0.381) (layer B.Cu) (net 25) (tstamp 5CC0D05A))
  (segment (start 196.7484 37.0332) (end 198.0184 35.7632) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC0D058))
  (segment (start 193.04 37.8968) (end 193.9036 37.0332) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC0D056))
  (segment (start 193.04 37.8968) (end 193.04 39.53) (width 0.381) (layer F.Cu) (net 25) (status 800000))
  (segment (start 193.9036 37.0332) (end 196.7484 37.0332) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC0D057))
  (segment (start 198.0184 34.1376) (end 198.9836 33.1724) (width 0.381) (layer B.Cu) (net 25))
  (segment (start 198.9836 33.1724) (end 202.8444 33.1724) (width 0.381) (layer B.Cu) (net 25) (tstamp 5CC100E8))
  (segment (start 204.47 26.5176) (end 204.4192 26.5176) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC12D72))
  (segment (start 204.4192 26.5176) (end 204.47 26.5176) (width 0.381) (layer F.Cu) (net 25) (tstamp 5CC12D74))
  (segment (start 204.47 30.56) (end 204.47 35.48) (width 0.381) (layer F.Cu) (net 26) (status C00000))
  (segment (start 204.47 21.51) (end 203.8388 21.51) (width 0.381) (layer F.Cu) (net 26) (status C00000))
  (segment (start 203.7372 30.56) (end 204.47 30.56) (width 0.381) (layer F.Cu) (net 26) (tstamp 5CC12D7A) (status 800000))
  (segment (start 203.3016 30.1244) (end 203.7372 30.56) (width 0.381) (layer F.Cu) (net 26) (tstamp 5CC12D79))
  (segment (start 203.3016 22.0472) (end 203.3016 30.1244) (width 0.381) (layer F.Cu) (net 26) (tstamp 5CC12D78))
  (segment (start 203.8388 21.51) (end 203.3016 22.0472) (width 0.381) (layer F.Cu) (net 26) (tstamp 5CC12D77) (status 400000))
  (segment (start 194.31 41.148) (end 194.31 39.53) (width 0.381) (layer F.Cu) (net 27) (tstamp 5CC0CF01) (status 800000))
  (segment (start 194.3608 41.1988) (end 194.31 41.148) (width 0.381) (layer F.Cu) (net 27) (tstamp 5CC0CF00))
  (via (at 194.3608 41.1988) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 27))
  (segment (start 180.975 44.45) (end 184.2262 41.1988) (width 0.381) (layer B.Cu) (net 27) (tstamp 5CC102E2) (status 400000))
  (segment (start 184.2262 41.1988) (end 194.3608 41.1988) (width 0.381) (layer B.Cu) (net 27))
  (segment (start 195.58 39.53) (end 195.58 40.64) (width 0.381) (layer F.Cu) (net 27) (status 400000))
  (segment (start 195.0212 41.1988) (end 194.3608 41.1988) (width 0.381) (layer F.Cu) (net 27) (tstamp 5CC0D053))
  (segment (start 195.58 40.64) (end 195.0212 41.1988) (width 0.381) (layer F.Cu) (net 27) (tstamp 5CC0D052))
  (segment (start 191.77 39.53) (end 191.77 38.4556) (width 0.381) (layer F.Cu) (net 28) (status 400000))
  (segment (start 204.47 40.0304) (end 204.47 38.18) (width 0.381) (layer F.Cu) (net 28) (tstamp 5CC103E3) (status 800000))
  (via (at 204.47 40.0304) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 28))
  (segment (start 193.3448 40.0304) (end 204.47 40.0304) (width 0.381) (layer B.Cu) (net 28) (tstamp 5CC103E0))
  (segment (start 191.77 38.4556) (end 193.3448 40.0304) (width 0.381) (layer B.Cu) (net 28) (tstamp 5CC103DF))
  (via (at 191.77 38.4556) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 28))

  (zone (net 1) (net_name GND) (layer B.Cu) (tstamp 5CC100A9) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166 20) (xy 166 47) (xy 206 47) (xy 206 20)
      )
    )
    (filled_polygon
      (pts
        (xy 172.300817 21.193877) (xy 172.418396 21.463) (xy 173.863 21.463) (xy 173.863 21.443) (xy 174.117 21.443)
        (xy 174.117 21.463) (xy 175.561604 21.463) (xy 175.679183 21.193877) (xy 175.459201 20.71) (xy 201.357267 20.71)
        (xy 201.272593 20.794674) (xy 201.0998 21.211834) (xy 201.0998 21.405167) (xy 198.340408 24.16456) (xy 196.7876 24.16456)
        (xy 196.539835 24.213843) (xy 196.433492 24.2849) (xy 187.635397 24.2849) (xy 187.613809 24.252591) (xy 187.403765 24.112243)
        (xy 187.156 24.06296) (xy 185.256 24.06296) (xy 185.008235 24.112243) (xy 184.798191 24.252591) (xy 184.657843 24.462635)
        (xy 184.60856 24.7104) (xy 184.60856 25.5104) (xy 184.657843 25.758165) (xy 184.798191 25.968209) (xy 184.931694 26.057413)
        (xy 184.896302 26.072073) (xy 184.717673 26.250701) (xy 184.621 26.48409) (xy 184.621 26.72465) (xy 184.77975 26.8834)
        (xy 186.079 26.8834) (xy 186.079 26.8634) (xy 186.333 26.8634) (xy 186.333 26.8834) (xy 187.63225 26.8834)
        (xy 187.717781 26.797869) (xy 187.798191 26.918209) (xy 188.008235 27.058557) (xy 188.256 27.10784) (xy 188.270041 27.10784)
        (xy 188.352569 27.30708) (xy 188.64372 27.598231) (xy 189.024126 27.7558) (xy 189.435874 27.7558) (xy 189.81628 27.598231)
        (xy 190.016761 27.39775) (xy 196.1526 27.39775) (xy 196.1526 27.63831) (xy 196.249273 27.871699) (xy 196.427902 28.050327)
        (xy 196.661291 28.147) (xy 197.45185 28.147) (xy 197.6106 27.98825) (xy 197.6106 27.239) (xy 197.8646 27.239)
        (xy 197.8646 27.98825) (xy 198.02335 28.147) (xy 198.813909 28.147) (xy 199.047298 28.050327) (xy 199.225927 27.871699)
        (xy 199.3226 27.63831) (xy 199.3226 27.39775) (xy 199.16385 27.239) (xy 197.8646 27.239) (xy 197.6106 27.239)
        (xy 196.31135 27.239) (xy 196.1526 27.39775) (xy 190.016761 27.39775) (xy 190.107431 27.30708) (xy 190.193008 27.100479)
        (xy 190.403765 27.058557) (xy 190.613809 26.918209) (xy 190.754157 26.708165) (xy 190.80344 26.4604) (xy 190.80344 25.9359)
        (xy 196.240315 25.9359) (xy 196.329791 26.069809) (xy 196.463294 26.159013) (xy 196.427902 26.173673) (xy 196.249273 26.352301)
        (xy 196.1526 26.58569) (xy 196.1526 26.82625) (xy 196.31135 26.985) (xy 197.6106 26.985) (xy 197.6106 26.965)
        (xy 197.8646 26.965) (xy 197.8646 26.985) (xy 199.16385 26.985) (xy 199.249381 26.899469) (xy 199.329791 27.019809)
        (xy 199.539835 27.160157) (xy 199.7876 27.20944) (xy 199.912101 27.20944) (xy 199.9121 29.84357) (xy 199.911831 29.84292)
        (xy 199.62068 29.551769) (xy 199.240274 29.3942) (xy 198.828526 29.3942) (xy 198.44812 29.551769) (xy 198.396189 29.6037)
        (xy 194.592611 29.6037) (xy 194.54068 29.551769) (xy 194.160274 29.3942) (xy 193.748526 29.3942) (xy 193.36812 29.551769)
        (xy 193.316189 29.6037) (xy 189.512611 29.6037) (xy 189.46068 29.551769) (xy 189.080274 29.3942) (xy 188.668526 29.3942)
        (xy 188.28812 29.551769) (xy 188.236189 29.6037) (xy 184.381811 29.6037) (xy 184.38068 29.602569) (xy 184.000274 29.445)
        (xy 183.588526 29.445) (xy 183.20812 29.602569) (xy 182.916969 29.89372) (xy 182.7594 30.274126) (xy 182.7594 30.685874)
        (xy 182.916969 31.06628) (xy 183.20812 31.357431) (xy 183.588526 31.515) (xy 184.000274 31.515) (xy 184.38068 31.357431)
        (xy 184.385 31.353111) (xy 184.385 31.651074) (xy 184.542569 32.03148) (xy 184.83372 32.322631) (xy 185.214126 32.4802)
        (xy 185.625874 32.4802) (xy 186.00628 32.322631) (xy 186.058211 32.2707) (xy 186.747053 32.2707) (xy 186.71656 32.424)
        (xy 186.71656 34.124) (xy 186.736948 34.2265) (xy 176.744933 34.2265) (xy 173.475872 30.95744) (xy 175.09 30.95744)
        (xy 175.337765 30.908157) (xy 175.547809 30.767809) (xy 175.688157 30.557765) (xy 175.73744 30.31) (xy 175.73744 28.11)
        (xy 175.688157 27.862235) (xy 175.547809 27.652191) (xy 175.337765 27.511843) (xy 175.09 27.46256) (xy 172.89 27.46256)
        (xy 172.642235 27.511843) (xy 172.432191 27.652191) (xy 172.291843 27.862235) (xy 172.24256 28.11) (xy 172.24256 28.588593)
        (xy 172.163874 28.556) (xy 171.752126 28.556) (xy 171.37172 28.713569) (xy 171.080569 29.00472) (xy 170.923 29.385126)
        (xy 170.923 29.796874) (xy 171.016121 30.021689) (xy 169.4815 28.487068) (xy 169.4815 27.816211) (xy 169.533431 27.76428)
        (xy 169.691 27.383874) (xy 169.691 27.29615) (xy 184.621 27.29615) (xy 184.621 27.53671) (xy 184.717673 27.770099)
        (xy 184.896302 27.948727) (xy 185.129691 28.0454) (xy 185.92025 28.0454) (xy 186.079 27.88665) (xy 186.079 27.1374)
        (xy 186.333 27.1374) (xy 186.333 27.88665) (xy 186.49175 28.0454) (xy 187.282309 28.0454) (xy 187.515698 27.948727)
        (xy 187.694327 27.770099) (xy 187.791 27.53671) (xy 187.791 27.29615) (xy 187.63225 27.1374) (xy 186.333 27.1374)
        (xy 186.079 27.1374) (xy 184.77975 27.1374) (xy 184.621 27.29615) (xy 169.691 27.29615) (xy 169.691 26.972126)
        (xy 169.533431 26.59172) (xy 169.24228 26.300569) (xy 168.861874 26.143) (xy 168.450126 26.143) (xy 168.06972 26.300569)
        (xy 167.778569 26.59172) (xy 167.621 26.972126) (xy 167.621 27.383874) (xy 167.778569 27.76428) (xy 167.8305 27.816211)
        (xy 167.830501 28.747694) (xy 167.814328 28.829) (xy 167.878397 29.151094) (xy 168.060849 29.424152) (xy 168.129775 29.470207)
        (xy 175.380793 36.721226) (xy 175.426848 36.790152) (xy 175.699906 36.972604) (xy 175.940697 37.0205) (xy 175.940701 37.0205)
        (xy 176.021999 37.036671) (xy 176.103297 37.0205) (xy 181.649068 37.0205) (xy 183.369 38.740433) (xy 183.369 38.813874)
        (xy 183.526569 39.19428) (xy 183.81772 39.485431) (xy 184.198126 39.643) (xy 184.609874 39.643) (xy 184.99028 39.485431)
        (xy 185.281431 39.19428) (xy 185.439 38.813874) (xy 185.439 38.402126) (xy 185.281431 38.02172) (xy 184.99028 37.730569)
        (xy 184.609874 37.573) (xy 184.536433 37.573) (xy 182.840932 35.8775) (xy 193.212699 35.8775) (xy 193.294 35.893672)
        (xy 193.375301 35.8775) (xy 193.375303 35.8775) (xy 193.616094 35.829604) (xy 193.889152 35.647152) (xy 193.935209 35.578223)
        (xy 195.540933 33.9725) (xy 196.211789 33.9725) (xy 196.26372 34.024431) (xy 196.644126 34.182) (xy 197.055874 34.182)
        (xy 197.177955 34.131433) (xy 197.176728 34.1376) (xy 197.192901 34.218906) (xy 197.1929 35.124989) (xy 197.140969 35.17692)
        (xy 196.9834 35.557326) (xy 196.9834 35.969074) (xy 197.140969 36.34948) (xy 197.43212 36.640631) (xy 197.812526 36.7982)
        (xy 198.224274 36.7982) (xy 198.60468 36.640631) (xy 198.895831 36.34948) (xy 199.0534 35.969074) (xy 199.0534 35.557326)
        (xy 198.895831 35.17692) (xy 198.8439 35.124989) (xy 198.8439 34.479532) (xy 199.325533 33.9979) (xy 202.763099 33.9979)
        (xy 202.8444 34.014072) (xy 202.925701 33.9979) (xy 202.925703 33.9979) (xy 203.166494 33.950004) (xy 203.439552 33.767552)
        (xy 203.485609 33.698623) (xy 205.29 31.894232) (xy 205.290001 39.38669) (xy 205.05628 39.152969) (xy 204.675874 38.9954)
        (xy 204.264126 38.9954) (xy 203.88372 39.152969) (xy 203.831789 39.2049) (xy 193.686733 39.2049) (xy 192.805 38.323168)
        (xy 192.805 38.249726) (xy 192.647431 37.86932) (xy 192.35628 37.578169) (xy 191.975874 37.4206) (xy 191.564126 37.4206)
        (xy 191.18372 37.578169) (xy 190.892569 37.86932) (xy 190.735 38.249726) (xy 190.735 38.661474) (xy 190.892569 39.04188)
        (xy 191.18372 39.333031) (xy 191.564126 39.4906) (xy 191.637568 39.4906) (xy 192.520267 40.3733) (xy 184.307497 40.3733)
        (xy 184.226199 40.357129) (xy 184.144901 40.3733) (xy 184.144897 40.3733) (xy 183.904106 40.421196) (xy 183.631048 40.603648)
        (xy 183.584993 40.672574) (xy 181.264145 42.993422) (xy 181.121256 42.965) (xy 180.828744 42.965) (xy 180.395582 43.051161)
        (xy 179.904375 43.379375) (xy 179.691157 43.698478) (xy 179.630183 43.568642) (xy 179.201924 43.178355) (xy 178.79189 43.008524)
        (xy 178.562 43.129845) (xy 178.562 44.323) (xy 178.582 44.323) (xy 178.582 44.577) (xy 178.562 44.577)
        (xy 178.562 45.770155) (xy 178.79189 45.891476) (xy 179.201924 45.721645) (xy 179.630183 45.331358) (xy 179.691157 45.201522)
        (xy 179.904375 45.520625) (xy 180.395582 45.848839) (xy 180.828744 45.935) (xy 181.121256 45.935) (xy 181.554418 45.848839)
        (xy 182.045625 45.520625) (xy 182.245 45.222239) (xy 182.444375 45.520625) (xy 182.935582 45.848839) (xy 183.368744 45.935)
        (xy 183.661256 45.935) (xy 184.094418 45.848839) (xy 184.585625 45.520625) (xy 184.913839 45.029418) (xy 185.029092 44.45)
        (xy 184.971578 44.160855) (xy 186.092133 43.0403) (xy 192.401789 43.0403) (xy 192.45372 43.092231) (xy 192.834126 43.2498)
        (xy 193.245874 43.2498) (xy 193.62628 43.092231) (xy 193.917431 42.80108) (xy 194.075 42.420674) (xy 194.075 42.200694)
        (xy 194.154926 42.2338) (xy 194.566674 42.2338) (xy 194.5958 42.221736) (xy 194.5958 42.471474) (xy 194.753369 42.85188)
        (xy 195.04452 43.143031) (xy 195.424926 43.3006) (xy 195.836674 43.3006) (xy 196.21708 43.143031) (xy 196.269011 43.0911)
        (xy 197.481789 43.0911) (xy 197.53372 43.143031) (xy 197.914126 43.3006) (xy 198.325874 43.3006) (xy 198.70628 43.143031)
        (xy 198.997431 42.85188) (xy 199.155 42.471474) (xy 199.155 42.059726) (xy 198.997431 41.67932) (xy 198.70628 41.388169)
        (xy 198.325874 41.2306) (xy 197.914126 41.2306) (xy 197.53372 41.388169) (xy 197.481789 41.4401) (xy 196.269011 41.4401)
        (xy 196.21708 41.388169) (xy 195.836674 41.2306) (xy 195.424926 41.2306) (xy 195.3958 41.242664) (xy 195.3958 40.992926)
        (xy 195.339042 40.8559) (xy 203.831789 40.8559) (xy 203.88372 40.907831) (xy 204.264126 41.0654) (xy 204.675874 41.0654)
        (xy 205.05628 40.907831) (xy 205.290001 40.67411) (xy 205.290001 41.852442) (xy 204.848835 41.411276) (xy 203.69659 40.934)
        (xy 202.44941 40.934) (xy 201.297165 41.411276) (xy 200.415276 42.293165) (xy 199.938 43.44541) (xy 199.938 44.69259)
        (xy 200.415276 45.844835) (xy 200.860441 46.29) (xy 171.122559 46.29) (xy 171.567724 45.844835) (xy 172.045 44.69259)
        (xy 172.045 43.6) (xy 174.39756 43.6) (xy 174.39756 45.3) (xy 174.446843 45.547765) (xy 174.587191 45.757809)
        (xy 174.797235 45.898157) (xy 175.045 45.94744) (xy 176.745 45.94744) (xy 176.992765 45.898157) (xy 177.202809 45.757809)
        (xy 177.343157 45.547765) (xy 177.363739 45.444292) (xy 177.668076 45.721645) (xy 178.07811 45.891476) (xy 178.308 45.770155)
        (xy 178.308 44.577) (xy 178.288 44.577) (xy 178.288 44.323) (xy 178.308 44.323) (xy 178.308 43.129845)
        (xy 178.07811 43.008524) (xy 177.668076 43.178355) (xy 177.363739 43.455708) (xy 177.343157 43.352235) (xy 177.202809 43.142191)
        (xy 176.992765 43.001843) (xy 176.745 42.95256) (xy 175.045 42.95256) (xy 174.797235 43.001843) (xy 174.587191 43.142191)
        (xy 174.446843 43.352235) (xy 174.39756 43.6) (xy 172.045 43.6) (xy 172.045 43.44541) (xy 171.567724 42.293165)
        (xy 170.685835 41.411276) (xy 169.53359 40.934) (xy 169.188544 40.934) (xy 169.197809 40.927809) (xy 169.338157 40.717765)
        (xy 169.38744 40.47) (xy 169.38744 39.37) (xy 173.49101 39.37) (xy 173.625666 40.046963) (xy 174.009135 40.620865)
        (xy 174.583037 41.004334) (xy 175.08912 41.105) (xy 175.43088 41.105) (xy 175.936963 41.004334) (xy 176.510865 40.620865)
        (xy 176.894334 40.046963) (xy 177.02899 39.37) (xy 176.894334 38.693037) (xy 176.510865 38.119135) (xy 175.936963 37.735666)
        (xy 175.43088 37.635) (xy 175.08912 37.635) (xy 174.583037 37.735666) (xy 174.009135 38.119135) (xy 173.625666 38.693037)
        (xy 173.49101 39.37) (xy 169.38744 39.37) (xy 169.38744 38.27) (xy 169.338157 38.022235) (xy 169.197809 37.812191)
        (xy 168.987765 37.671843) (xy 168.74 37.62256) (xy 166.71 37.62256) (xy 166.71 21.986123) (xy 172.300817 21.986123)
        (xy 172.580988 22.602392) (xy 173.075668 23.064534) (xy 173.593878 23.279175) (xy 173.863 23.161125) (xy 173.863 21.717)
        (xy 174.117 21.717) (xy 174.117 23.161125) (xy 174.386122 23.279175) (xy 174.904332 23.064534) (xy 175.399012 22.602392)
        (xy 175.679183 21.986123) (xy 175.561604 21.717) (xy 174.117 21.717) (xy 173.863 21.717) (xy 172.418396 21.717)
        (xy 172.300817 21.986123) (xy 166.71 21.986123) (xy 166.71 20.71) (xy 172.520799 20.71)
      )
    )
  )
  (zone (net 15) (net_name VCC) (layer F.Cu) (tstamp 5CC100C1) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166 20) (xy 166 47) (xy 206 47) (xy 206 20)
      )
    )
    (filled_polygon
      (pts
        (xy 203.17256 20.76) (xy 203.17256 21.008807) (xy 202.775376 21.405991) (xy 202.706448 21.452048) (xy 202.604249 21.604999)
        (xy 202.48625 21.487) (xy 201.737 21.487) (xy 201.737 22.78625) (xy 201.89575 22.945) (xy 202.13631 22.945)
        (xy 202.369699 22.848327) (xy 202.4761 22.741925) (xy 202.476101 30.043094) (xy 202.459928 30.1244) (xy 202.516778 30.4102)
        (xy 202.523997 30.446494) (xy 202.706449 30.719552) (xy 202.775374 30.765607) (xy 203.095993 31.086225) (xy 203.142048 31.155152)
        (xy 203.17256 31.17554) (xy 203.17256 31.31) (xy 203.221843 31.557765) (xy 203.362191 31.767809) (xy 203.572235 31.908157)
        (xy 203.6445 31.922531) (xy 203.644501 34.117469) (xy 203.572235 34.131843) (xy 203.362191 34.272191) (xy 203.221843 34.482235)
        (xy 203.181753 34.683782) (xy 203.093327 34.470302) (xy 202.914699 34.291673) (xy 202.68131 34.195) (xy 202.21575 34.195)
        (xy 202.057 34.35375) (xy 202.057 35.453) (xy 202.077 35.453) (xy 202.077 35.707) (xy 202.057 35.707)
        (xy 202.057 35.727) (xy 201.803 35.727) (xy 201.803 35.707) (xy 200.82875 35.707) (xy 200.67 35.86575)
        (xy 200.67 36.456309) (xy 200.766673 36.689698) (xy 200.90832 36.831346) (xy 200.847191 36.872191) (xy 200.706843 37.082235)
        (xy 200.65756 37.33) (xy 200.65756 38.83) (xy 200.706843 39.077765) (xy 200.847191 39.287809) (xy 200.92288 39.338383)
        (xy 201.052569 39.65148) (xy 201.34372 39.942631) (xy 201.724126 40.1002) (xy 202.135874 40.1002) (xy 202.51628 39.942631)
        (xy 202.807431 39.65148) (xy 202.93712 39.338383) (xy 203.012809 39.287809) (xy 203.153157 39.077765) (xy 203.177554 38.955109)
        (xy 203.221843 39.177765) (xy 203.362191 39.387809) (xy 203.560898 39.520582) (xy 203.435 39.824526) (xy 203.435 40.236274)
        (xy 203.592569 40.61668) (xy 203.88372 40.907831) (xy 204.264126 41.0654) (xy 204.675874 41.0654) (xy 205.05628 40.907831)
        (xy 205.290001 40.67411) (xy 205.290001 41.852442) (xy 204.848835 41.411276) (xy 203.69659 40.934) (xy 202.44941 40.934)
        (xy 201.297165 41.411276) (xy 200.415276 42.293165) (xy 199.938 43.44541) (xy 199.938 44.69259) (xy 200.415276 45.844835)
        (xy 200.860441 46.29) (xy 171.122559 46.29) (xy 171.567724 45.844835) (xy 172.027122 44.73575) (xy 174.41 44.73575)
        (xy 174.41 45.426309) (xy 174.506673 45.659698) (xy 174.685301 45.838327) (xy 174.91869 45.935) (xy 175.60925 45.935)
        (xy 175.768 45.77625) (xy 175.768 44.577) (xy 174.56875 44.577) (xy 174.41 44.73575) (xy 172.027122 44.73575)
        (xy 172.045 44.69259) (xy 172.045 43.473691) (xy 174.41 43.473691) (xy 174.41 44.16425) (xy 174.56875 44.323)
        (xy 175.768 44.323) (xy 175.768 43.12375) (xy 176.022 43.12375) (xy 176.022 44.323) (xy 176.042 44.323)
        (xy 176.042 44.577) (xy 176.022 44.577) (xy 176.022 45.77625) (xy 176.18075 45.935) (xy 176.87131 45.935)
        (xy 177.104699 45.838327) (xy 177.283327 45.659698) (xy 177.349904 45.498967) (xy 177.364375 45.520625) (xy 177.855582 45.848839)
        (xy 178.288744 45.935) (xy 178.581256 45.935) (xy 179.014418 45.848839) (xy 179.505625 45.520625) (xy 179.705 45.222239)
        (xy 179.904375 45.520625) (xy 180.395582 45.848839) (xy 180.828744 45.935) (xy 181.121256 45.935) (xy 181.554418 45.848839)
        (xy 182.045625 45.520625) (xy 182.245 45.222239) (xy 182.444375 45.520625) (xy 182.935582 45.848839) (xy 183.368744 45.935)
        (xy 183.661256 45.935) (xy 184.094418 45.848839) (xy 184.585625 45.520625) (xy 184.913839 45.029418) (xy 185.029092 44.45)
        (xy 184.913839 43.870582) (xy 184.585625 43.379375) (xy 184.094418 43.051161) (xy 183.661256 42.965) (xy 183.368744 42.965)
        (xy 182.935582 43.051161) (xy 182.444375 43.379375) (xy 182.245 43.677761) (xy 182.045625 43.379375) (xy 181.554418 43.051161)
        (xy 181.121256 42.965) (xy 180.828744 42.965) (xy 180.395582 43.051161) (xy 179.904375 43.379375) (xy 179.705 43.677761)
        (xy 179.505625 43.379375) (xy 179.014418 43.051161) (xy 178.581256 42.965) (xy 178.288744 42.965) (xy 177.855582 43.051161)
        (xy 177.364375 43.379375) (xy 177.349904 43.401033) (xy 177.283327 43.240302) (xy 177.104699 43.061673) (xy 176.87131 42.965)
        (xy 176.18075 42.965) (xy 176.022 43.12375) (xy 175.768 43.12375) (xy 175.60925 42.965) (xy 174.91869 42.965)
        (xy 174.685301 43.061673) (xy 174.506673 43.240302) (xy 174.41 43.473691) (xy 172.045 43.473691) (xy 172.045 43.44541)
        (xy 171.567724 42.293165) (xy 170.685835 41.411276) (xy 169.53359 40.934) (xy 169.188544 40.934) (xy 169.197809 40.927809)
        (xy 169.338157 40.717765) (xy 169.38744 40.47) (xy 169.38744 38.27) (xy 169.338157 38.022235) (xy 169.197809 37.812191)
        (xy 168.987765 37.671843) (xy 168.74 37.62256) (xy 168.4655 37.62256) (xy 168.4655 36.897558) (xy 168.512765 36.888157)
        (xy 168.722809 36.747809) (xy 168.863157 36.537765) (xy 168.893444 36.3855) (xy 170.007469 36.3855) (xy 170.021843 36.457765)
        (xy 170.162191 36.667809) (xy 170.372235 36.808157) (xy 170.62 36.85744) (xy 172.12 36.85744) (xy 172.367765 36.808157)
        (xy 172.577809 36.667809) (xy 172.718157 36.457765) (xy 172.72 36.4485) (xy 172.721843 36.457765) (xy 172.862191 36.667809)
        (xy 173.072235 36.808157) (xy 173.32 36.85744) (xy 174.82 36.85744) (xy 175.067765 36.808157) (xy 175.277809 36.667809)
        (xy 175.418157 36.457765) (xy 175.46744 36.21) (xy 175.46744 36.1555) (xy 178.02256 36.1555) (xy 178.02256 36.28)
        (xy 178.071843 36.527765) (xy 178.208684 36.73256) (xy 177.72 36.73256) (xy 177.472235 36.781843) (xy 177.262191 36.922191)
        (xy 177.121843 37.132235) (xy 177.07256 37.38) (xy 177.07256 38.210007) (xy 176.772247 38.510321) (xy 176.510865 38.119135)
        (xy 175.936963 37.735666) (xy 175.43088 37.635) (xy 175.08912 37.635) (xy 174.583037 37.735666) (xy 174.009135 38.119135)
        (xy 173.625666 38.693037) (xy 173.49101 39.37) (xy 173.625666 40.046963) (xy 174.009135 40.620865) (xy 174.583037 41.004334)
        (xy 175.08912 41.105) (xy 175.43088 41.105) (xy 175.936963 41.004334) (xy 176.510865 40.620865) (xy 176.795085 40.1955)
        (xy 176.998699 40.1955) (xy 177.08 40.211672) (xy 177.161301 40.1955) (xy 177.161303 40.1955) (xy 177.402094 40.147604)
        (xy 177.675152 39.965152) (xy 177.702656 39.92399) (xy 177.72 39.92744) (xy 178.52 39.92744) (xy 178.767765 39.878157)
        (xy 178.977809 39.737809) (xy 179.0002 39.704299) (xy 179.0002 39.779074) (xy 179.157769 40.15948) (xy 179.44892 40.450631)
        (xy 179.829326 40.6082) (xy 180.241074 40.6082) (xy 180.62148 40.450631) (xy 180.881839 40.190272) (xy 181.832393 41.140826)
        (xy 181.878448 41.209752) (xy 182.151506 41.392204) (xy 182.392297 41.4401) (xy 182.392301 41.4401) (xy 182.473599 41.456271)
        (xy 182.554897 41.4401) (xy 186.253099 41.4401) (xy 186.3344 41.456272) (xy 186.415701 41.4401) (xy 186.415703 41.4401)
        (xy 186.656494 41.392204) (xy 186.929552 41.209752) (xy 186.975608 41.140824) (xy 187.404228 40.712205) (xy 187.473152 40.666152)
        (xy 187.56562 40.527765) (xy 187.651102 40.399831) (xy 187.655604 40.393094) (xy 187.7035 40.152303) (xy 187.7035 40.152299)
        (xy 187.719671 40.071001) (xy 187.7035 39.989703) (xy 187.7035 39.734918) (xy 187.801157 39.588765) (xy 187.85044 39.341)
        (xy 187.85044 38.84675) (xy 187.945 38.84675) (xy 187.945 39.437309) (xy 188.041673 39.670698) (xy 188.220301 39.849327)
        (xy 188.45369 39.946) (xy 188.94425 39.946) (xy 189.103 39.78725) (xy 189.103 38.688) (xy 188.10375 38.688)
        (xy 187.945 38.84675) (xy 187.85044 38.84675) (xy 187.85044 37.781) (xy 187.801157 37.533235) (xy 187.660809 37.323191)
        (xy 187.492905 37.211) (xy 187.660809 37.098809) (xy 187.801157 36.888765) (xy 187.84139 36.6865) (xy 187.947578 36.6865)
        (xy 187.981843 36.858765) (xy 188.122191 37.068809) (xy 188.332235 37.209157) (xy 188.360209 37.214721) (xy 188.220301 37.272673)
        (xy 188.041673 37.451302) (xy 187.945 37.684691) (xy 187.945 38.27525) (xy 188.10375 38.434) (xy 189.103 38.434)
        (xy 189.103 38.414) (xy 189.357 38.414) (xy 189.357 38.434) (xy 189.377 38.434) (xy 189.377 38.688)
        (xy 189.357 38.688) (xy 189.357 39.78725) (xy 189.51575 39.946) (xy 189.928501 39.946) (xy 189.928501 40.679066)
        (xy 187.655008 42.95256) (xy 186.475 42.95256) (xy 186.227235 43.001843) (xy 186.017191 43.142191) (xy 185.876843 43.352235)
        (xy 185.82756 43.6) (xy 185.82756 45.3) (xy 185.876843 45.547765) (xy 186.017191 45.757809) (xy 186.227235 45.898157)
        (xy 186.475 45.94744) (xy 188.175 45.94744) (xy 188.422765 45.898157) (xy 188.632809 45.757809) (xy 188.773157 45.547765)
        (xy 188.783859 45.493958) (xy 189.000647 45.493958) (xy 189.08092 45.745259) (xy 189.636279 45.946718) (xy 190.226458 45.920315)
        (xy 190.64908 45.745259) (xy 190.729353 45.493958) (xy 189.865 44.629605) (xy 189.000647 45.493958) (xy 188.783859 45.493958)
        (xy 188.819672 45.313915) (xy 188.821042 45.314353) (xy 189.685395 44.45) (xy 189.671253 44.435858) (xy 189.850858 44.256253)
        (xy 189.865 44.270395) (xy 190.729353 43.406042) (xy 190.64908 43.154741) (xy 190.093721 42.953282) (xy 189.984253 42.958179)
        (xy 191.280226 41.662207) (xy 191.349152 41.616152) (xy 191.531604 41.343094) (xy 191.5795 41.102303) (xy 191.5795 41.102299)
        (xy 191.595671 41.021001) (xy 191.5795 40.939703) (xy 191.5795 40.92744) (xy 192.07 40.92744) (xy 192.2145 40.898697)
        (xy 192.2145 41.576589) (xy 192.162569 41.62852) (xy 192.005 42.008926) (xy 192.005 42.420674) (xy 192.162569 42.80108)
        (xy 192.326489 42.965) (xy 192.109615 42.965) (xy 191.563815 43.191078) (xy 191.146078 43.608815) (xy 191.126845 43.655247)
        (xy 190.908958 43.585647) (xy 190.044605 44.45) (xy 190.908958 45.314353) (xy 191.126845 45.244753) (xy 191.146078 45.291185)
        (xy 191.563815 45.708922) (xy 192.109615 45.935) (xy 192.700385 45.935) (xy 193.246185 45.708922) (xy 193.663922 45.291185)
        (xy 193.675 45.26444) (xy 193.686078 45.291185) (xy 194.103815 45.708922) (xy 194.649615 45.935) (xy 195.240385 45.935)
        (xy 195.786185 45.708922) (xy 196.203922 45.291185) (xy 196.215 45.26444) (xy 196.226078 45.291185) (xy 196.643815 45.708922)
        (xy 197.189615 45.935) (xy 197.780385 45.935) (xy 198.326185 45.708922) (xy 198.743922 45.291185) (xy 198.97 44.745385)
        (xy 198.97 44.154615) (xy 198.743922 43.608815) (xy 198.403538 43.268431) (xy 198.70628 43.143031) (xy 198.997431 42.85188)
        (xy 199.155 42.471474) (xy 199.155 42.059726) (xy 198.997431 41.67932) (xy 198.9455 41.627389) (xy 198.9455 40.898697)
        (xy 199.09 40.92744) (xy 199.69 40.92744) (xy 199.937765 40.878157) (xy 200.147809 40.737809) (xy 200.288157 40.527765)
        (xy 200.33744 40.28) (xy 200.33744 38.923663) (xy 200.425 38.712274) (xy 200.425 38.300526) (xy 200.267431 37.92012)
        (xy 199.97628 37.628969) (xy 199.595874 37.4714) (xy 199.184126 37.4714) (xy 198.80372 37.628969) (xy 198.512569 37.92012)
        (xy 198.424226 38.1334) (xy 198.42 38.13256) (xy 197.82 38.13256) (xy 197.572235 38.181843) (xy 197.485 38.240132)
        (xy 197.397765 38.181843) (xy 197.15 38.13256) (xy 196.55 38.13256) (xy 196.302235 38.181843) (xy 196.215 38.240132)
        (xy 196.127765 38.181843) (xy 195.88 38.13256) (xy 195.28 38.13256) (xy 195.032235 38.181843) (xy 194.945 38.240132)
        (xy 194.857765 38.181843) (xy 194.61 38.13256) (xy 194.01 38.13256) (xy 193.962156 38.142077) (xy 194.245533 37.8587)
        (xy 196.667099 37.8587) (xy 196.7484 37.874872) (xy 196.829701 37.8587) (xy 196.829703 37.8587) (xy 197.070494 37.810804)
        (xy 197.343552 37.628352) (xy 197.389609 37.559423) (xy 198.150833 36.7982) (xy 198.224274 36.7982) (xy 198.60468 36.640631)
        (xy 198.895831 36.34948) (xy 199.0534 35.969074) (xy 199.0534 35.557326) (xy 199.035868 35.515) (xy 199.10425 35.515)
        (xy 199.263 35.35625) (xy 199.263 34.257) (xy 199.517 34.257) (xy 199.517 35.35625) (xy 199.67575 35.515)
        (xy 199.81631 35.515) (xy 200.049699 35.418327) (xy 200.228327 35.239698) (xy 200.325 35.006309) (xy 200.325 34.703691)
        (xy 200.67 34.703691) (xy 200.67 35.29425) (xy 200.82875 35.453) (xy 201.803 35.453) (xy 201.803 34.35375)
        (xy 201.64425 34.195) (xy 201.17869 34.195) (xy 200.945301 34.291673) (xy 200.766673 34.470302) (xy 200.67 34.703691)
        (xy 200.325 34.703691) (xy 200.325 34.41575) (xy 200.16625 34.257) (xy 199.517 34.257) (xy 199.263 34.257)
        (xy 199.243 34.257) (xy 199.243 34.003) (xy 199.263 34.003) (xy 199.263 32.90375) (xy 199.517 32.90375)
        (xy 199.517 34.003) (xy 200.16625 34.003) (xy 200.325 33.84425) (xy 200.325 33.253691) (xy 200.228327 33.020302)
        (xy 200.049699 32.841673) (xy 199.81631 32.745) (xy 199.67575 32.745) (xy 199.517 32.90375) (xy 199.263 32.90375)
        (xy 199.10425 32.745) (xy 198.96369 32.745) (xy 198.746972 32.834768) (xy 198.667765 32.781843) (xy 198.42 32.73256)
        (xy 197.82 32.73256) (xy 197.800238 32.736491) (xy 197.727431 32.56072) (xy 197.43628 32.269569) (xy 197.055874 32.112)
        (xy 196.644126 32.112) (xy 196.26372 32.269569) (xy 195.972569 32.56072) (xy 195.899762 32.736491) (xy 195.88 32.73256)
        (xy 195.28 32.73256) (xy 195.1355 32.761303) (xy 195.1355 32.381358) (xy 195.374126 32.4802) (xy 195.785874 32.4802)
        (xy 196.16628 32.322631) (xy 196.457431 32.03148) (xy 196.58712 31.718383) (xy 196.662809 31.667809) (xy 196.803157 31.457765)
        (xy 196.85 31.222267) (xy 196.896843 31.457765) (xy 197.037191 31.667809) (xy 197.247235 31.808157) (xy 197.495 31.85744)
        (xy 198.745 31.85744) (xy 198.992765 31.808157) (xy 199.202809 31.667809) (xy 199.343157 31.457765) (xy 199.351 31.418336)
        (xy 199.423063 31.388487) (xy 199.436843 31.457765) (xy 199.577191 31.667809) (xy 199.65288 31.718383) (xy 199.782569 32.03148)
        (xy 200.07372 32.322631) (xy 200.454126 32.4802) (xy 200.865874 32.4802) (xy 201.24628 32.322631) (xy 201.537431 32.03148)
        (xy 201.66712 31.718383) (xy 201.742809 31.667809) (xy 201.883157 31.457765) (xy 201.93244 31.21) (xy 201.93244 29.71)
        (xy 201.883157 29.462235) (xy 201.742809 29.252191) (xy 201.679666 29.21) (xy 201.742809 29.167809) (xy 201.883157 28.957765)
        (xy 201.93244 28.71) (xy 201.93244 27.21) (xy 201.883157 26.962235) (xy 201.742809 26.752191) (xy 201.532765 26.611843)
        (xy 201.4855 26.602442) (xy 201.4855 25.789397) (xy 201.517809 25.767809) (xy 201.658157 25.557765) (xy 201.70744 25.31)
        (xy 201.70744 23.41) (xy 201.658157 23.162235) (xy 201.517809 22.952191) (xy 201.397469 22.871781) (xy 201.483 22.78625)
        (xy 201.483 21.487) (xy 201.463 21.487) (xy 201.463 21.233) (xy 201.483 21.233) (xy 201.483 21.213)
        (xy 201.737 21.213) (xy 201.737 21.233) (xy 202.48625 21.233) (xy 202.645 21.07425) (xy 202.645 20.71)
        (xy 203.182506 20.71)
      )
    )
  )
)
