(kicad_pcb (version 20171130) (host pcbnew 6.0.0-rc1-unknown-32d262b~66~ubuntu14.04.1)
  (general
    (thickness 1.6)
    (drawings 71)
    (tracks 124)
    (zones 0)
    (modules 26)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFE79F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D14-Pad2)")
  (net 4 "Net-(D15-Pad2)")
  (net 5 "Net-(D10-Pad1)")
  (net 6 "Net-(D13-Pad1)")
  (net 7 "Net-(D10-Pad2)")
  (net 8 "Net-(D11-Pad2)")
  (net 9 "Net-(D12-Pad2)")
  (net 10 "Net-(J1-Pad7)")
  (net 11 "Net-(J1-Pad8)")
  (net 12 "Net-(J1-Pad9)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_9pol (layer F.Cu) (tedit 5BB3C72B)
    (at 168.91 93.98)
    (descr "9-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 10.16 -4.50088) (layer F.SilkS) hide)
    (fp_text value Digital_8-13 (at 10.16 4.50088) (layer F.Fab) hide)
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "Net-(D10-Pad2)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(D15-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(D12-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_9pol.wrl
      (offset (xyz 10.15999984741211 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 158.75 85.09 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 196.85 85.09 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D15 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 180.34 71.12)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D11 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 203.2 93.98)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J6 (at 0 -3.048) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer B.Cu) (tedit 5861332C)
    (at 203.2 52.07)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J5 (at 0 3.048) (layer B.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -3) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 154.94 93.98)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J4 (at 0 -3.048) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer B.Cu) (tedit 5BB3C37C)
    (at 154.94 52.07)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 3.048) (layer B.SilkS))
    (fp_text value Conn_01x01_Male (at 0 -3) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5B85F052)
    (at 167.64 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.54 -1.86 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad7)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5B85F052)
    (at 187.96 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.86 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad8)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5B85F052)
    (at 190.5 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.86 270) (layer F.SilkS))
    (fp_text value R (at 2.54 1.86 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 177.8 71.12 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D8 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 196.85 57.15 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D13 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 158.75 57.15 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 158.75 71.12 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 161.29 57.15)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 161.29 71.12)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 161.29 85.09)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D12-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 177.8 57.15 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D7 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 177.8 85.09 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D9 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 180.34 57.15)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D10 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 180.34 85.09)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D12 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D12-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 196.85 71.12 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D14 (at 1.27 2.96 180) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 199.39 57.15)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D16 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 199.39 71.12)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D17 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer B.Cu) (tedit 587A3A7B)
    (at 199.39 85.09)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D18 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D12-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 12 (at 171.45 91.44) (layer F.SilkS))
  (gr_text G (at 162.56 59.436) (layer F.SilkS))
  (gr_text G (at 162.56 73.406) (layer F.SilkS))
  (gr_text R (at 157.48 88.138) (layer F.SilkS))
  (gr_text R (at 157.48 73.406) (layer F.SilkS))
  (gr_text G (at 162.56 88.138) (layer F.SilkS))
  (gr_text R (at 157.48 59.436) (layer F.SilkS))
  (gr_text 11 (at 174.244 91.44) (layer F.SilkS))
  (gr_text 13 (at 169.164 91.44) (layer F.SilkS))
  (gr_text 8 (at 181.864 91.44) (layer F.SilkS))
  (gr_text 9 (at 179.324 91.44) (layer F.SilkS))
  (gr_text 10 (at 176.53 91.44) (layer F.SilkS))
  (gr_text 7 (at 184.404 91.44) (layer F.SilkS))
  (gr_text 6 (at 186.69 91.44) (layer F.SilkS))
  (gr_text 5 (at 189.484 91.44) (layer F.SilkS))
  (gr_text Cols (at 185.42 90.17) (layer F.SilkS))
  (gr_text "Red Rows" (at 179.07 90.17) (layer F.SilkS))
  (gr_text "Green Rows" (at 171.45 90.17) (layer F.SilkS))
  (gr_line (start 152.4 49.53) (end 205.74 49.53) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 205.74 49.53) (end 205.74 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.4 49.53) (end 152.4 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 205.74 96.52) (end 152.4 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_text O (at 179.07 86.995) (layer B.SilkS))
  (gr_text O (at 161.925 86.995) (layer B.SilkS))
  (gr_text O (at 161.925 71.12) (layer B.SilkS))
  (gr_text X (at 161.925 55.88) (layer B.SilkS))
  (gr_text X (at 196.215 86.995) (layer B.SilkS))
  (gr_text X (at 179.07 71.12) (layer B.SilkS))
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 198.12 79.98) (layer Dwgs.User))
    (feature1 (pts (xy 201.93 91.44) (xy 201.93 80.693579)))
    (feature2 (pts (xy 194.31 91.44) (xy 194.31 80.693579)))
    (crossbar (pts (xy 194.31 81.28) (xy 201.93 81.28)))
    (arrow1a (pts (xy 201.93 81.28) (xy 200.803496 81.866421)))
    (arrow1b (pts (xy 201.93 81.28) (xy 200.803496 80.693579)))
    (arrow2a (pts (xy 194.31 81.28) (xy 195.436504 81.866421)))
    (arrow2b (pts (xy 194.31 81.28) (xy 195.436504 80.693579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 160.02 79.98) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 91.44) (xy 163.83 80.693579)))
    (feature2 (pts (xy 156.21 91.44) (xy 156.21 80.693579)))
    (crossbar (pts (xy 156.21 81.28) (xy 163.83 81.28)))
    (arrow1a (pts (xy 163.83 81.28) (xy 162.703496 81.866421)))
    (arrow1b (pts (xy 163.83 81.28) (xy 162.703496 80.693579)))
    (arrow2a (pts (xy 156.21 81.28) (xy 157.336504 81.866421)))
    (arrow2b (pts (xy 156.21 81.28) (xy 157.336504 80.693579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 160.02 63.47) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 71.12) (xy 163.83 64.183579)))
    (feature2 (pts (xy 156.21 71.12) (xy 156.21 64.183579)))
    (crossbar (pts (xy 156.21 64.77) (xy 163.83 64.77)))
    (arrow1a (pts (xy 163.83 64.77) (xy 162.703496 65.356421)))
    (arrow1b (pts (xy 163.83 64.77) (xy 162.703496 64.183579)))
    (arrow2a (pts (xy 156.21 64.77) (xy 157.336504 65.356421)))
    (arrow2b (pts (xy 156.21 64.77) (xy 157.336504 64.183579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 198.12 63.47) (layer Dwgs.User))
    (feature1 (pts (xy 194.31 68.58) (xy 194.31 64.183579)))
    (feature2 (pts (xy 201.93 68.58) (xy 201.93 64.183579)))
    (crossbar (pts (xy 201.93 64.77) (xy 194.31 64.77)))
    (arrow1a (pts (xy 194.31 64.77) (xy 195.436504 64.183579)))
    (arrow1b (pts (xy 194.31 64.77) (xy 195.436504 65.356421)))
    (arrow2a (pts (xy 201.93 64.77) (xy 200.803496 64.183579)))
    (arrow2b (pts (xy 201.93 64.77) (xy 200.803496 65.356421)))
  )
  (dimension 27.93 (width 0.15) (layer Dwgs.User)
    (gr_text "27.930 mm" (at 200.645 115.66) (layer Dwgs.User))
    (feature1 (pts (xy 186.68 112.74) (xy 186.68 114.946421)))
    (feature2 (pts (xy 214.61 112.74) (xy 214.61 114.946421)))
    (crossbar (pts (xy 214.61 114.36) (xy 186.68 114.36)))
    (arrow1a (pts (xy 186.68 114.36) (xy 187.806504 113.773579)))
    (arrow1b (pts (xy 186.68 114.36) (xy 187.806504 114.946421)))
    (arrow2a (pts (xy 214.61 114.36) (xy 213.483496 113.773579)))
    (arrow2b (pts (xy 214.61 114.36) (xy 213.483496 114.946421)))
  )
  (dimension 63.440013 (width 0.15) (layer Dwgs.User)
    (gr_text "63.440 mm" (at 182.82234 118.61123) (layer Dwgs.User))
    (feature1 (pts (xy 151.1 114.92) (xy 151.10189 117.91765)))
    (feature2 (pts (xy 214.54 114.88) (xy 214.54189 117.87765)))
    (crossbar (pts (xy 214.54152 117.29123) (xy 151.10152 117.33123)))
    (arrow1a (pts (xy 151.10152 117.33123) (xy 152.227654 116.744099)))
    (arrow1b (pts (xy 151.10152 117.33123) (xy 152.228393 117.91694)))
    (arrow2a (pts (xy 214.54152 117.29123) (xy 213.414647 116.70552)))
    (arrow2b (pts (xy 214.54152 117.29123) (xy 213.415386 117.878361)))
  )
  (dimension 63.470007 (width 0.15) (layer Dwgs.User)
    (gr_text "63.470 mm" (at 182.838903 17.984841 0.02708166468) (layer Dwgs.User))
    (feature1 (pts (xy 151.11 30.9) (xy 151.10424 18.713421)))
    (feature2 (pts (xy 214.58 30.87) (xy 214.57424 18.683421)))
    (crossbar (pts (xy 214.574517 19.269841) (xy 151.104517 19.299841)))
    (arrow1a (pts (xy 151.104517 19.299841) (xy 152.230743 18.712888)))
    (arrow1b (pts (xy 151.104517 19.299841) (xy 152.231298 19.885729)))
    (arrow2a (pts (xy 214.574517 19.269841) (xy 213.447736 18.683953)))
    (arrow2b (pts (xy 214.574517 19.269841) (xy 213.448291 19.856794)))
  )
  (dimension 41.660043 (width 0.15) (layer Dwgs.User)
    (gr_text "41.660 mm" (at 193.758753 22.960634 0.1) (layer Dwgs.User))
    (feature1 (pts (xy 172.94 30.8) (xy 172.92978 23.704213)))
    (feature2 (pts (xy 214.6 30.74) (xy 214.58978 23.644213)))
    (crossbar (pts (xy 214.590625 24.230633) (xy 172.930625 24.290633)))
    (arrow1a (pts (xy 172.930625 24.290633) (xy 174.056283 23.70259)))
    (arrow1b (pts (xy 172.930625 24.290633) (xy 174.057972 24.875431)))
    (arrow2a (pts (xy 214.590625 24.230633) (xy 213.463278 23.645835)))
    (arrow2b (pts (xy 214.590625 24.230633) (xy 213.464967 24.818676)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 149.77 101.81) (layer Dwgs.User))
    (feature1 (pts (xy 151.04 99.94) (xy 151.04 101.096421)))
    (feature2 (pts (xy 148.5 99.94) (xy 148.5 101.096421)))
    (crossbar (pts (xy 148.5 100.51) (xy 151.04 100.51)))
    (arrow1a (pts (xy 151.04 100.51) (xy 149.913496 101.096421)))
    (arrow1b (pts (xy 151.04 100.51) (xy 149.913496 99.923579)))
    (arrow2a (pts (xy 148.5 100.51) (xy 149.626504 101.096421)))
    (arrow2b (pts (xy 148.5 100.51) (xy 149.626504 99.923579)))
  )
  (dimension 2.54002 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 143.404676 97.220038 89.77442723) (layer Dwgs.User))
    (feature1 (pts (xy 145.94 95.96) (xy 144.123249 95.952847)))
    (feature2 (pts (xy 145.93 98.5) (xy 144.113249 98.492847)))
    (crossbar (pts (xy 144.699666 98.495156) (xy 144.709666 95.955156)))
    (arrow1a (pts (xy 144.709666 95.955156) (xy 145.291647 97.08396)))
    (arrow1b (pts (xy 144.709666 95.955156) (xy 144.118815 97.079342)))
    (arrow2a (pts (xy 144.699666 98.495156) (xy 145.290517 97.37097)))
    (arrow2b (pts (xy 144.699666 98.495156) (xy 144.117685 97.366352)))
  )
  (dimension 2.540492 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 144.456054 46.476318 271.127724) (layer Dwgs.User))
    (feature1 (pts (xy 147.85 47.68) (xy 145.194495 47.732274)))
    (feature2 (pts (xy 147.8 45.14) (xy 145.144495 45.192274)))
    (crossbar (pts (xy 145.730802 45.180732) (xy 145.780802 47.720732)))
    (arrow1a (pts (xy 145.780802 47.720732) (xy 145.172324 46.605988)))
    (arrow1b (pts (xy 145.780802 47.720732) (xy 146.344938 46.582905)))
    (arrow2a (pts (xy 145.730802 45.180732) (xy 145.166666 46.318559)))
    (arrow2b (pts (xy 145.730802 45.180732) (xy 146.33928 46.295476)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 149.78 42.008) (layer Dwgs.User))
    (feature1 (pts (xy 151.05 44.07) (xy 151.05 42.721579)))
    (feature2 (pts (xy 148.51 44.07) (xy 148.51 42.721579)))
    (crossbar (pts (xy 148.51 43.308) (xy 151.05 43.308)))
    (arrow1a (pts (xy 151.05 43.308) (xy 149.923496 43.894421)))
    (arrow1b (pts (xy 151.05 43.308) (xy 149.923496 42.721579)))
    (arrow2a (pts (xy 148.51 43.308) (xy 149.636504 43.894421)))
    (arrow2b (pts (xy 148.51 43.308) (xy 149.636504 42.721579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 179.07 64.740001) (layer Dwgs.User))
    (feature1 (pts (xy 182.88 71.12) (xy 182.88 65.45358)))
    (feature2 (pts (xy 175.26 71.12) (xy 175.26 65.45358)))
    (crossbar (pts (xy 175.26 66.040001) (xy 182.88 66.040001)))
    (arrow1a (pts (xy 182.88 66.040001) (xy 181.753496 66.626422)))
    (arrow1b (pts (xy 182.88 66.040001) (xy 181.753496 65.45358)))
    (arrow2a (pts (xy 175.26 66.040001) (xy 176.386504 66.626422)))
    (arrow2b (pts (xy 175.26 66.040001) (xy 176.386504 65.45358)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 207.04 61.595 90) (layer Dwgs.User))
    (feature1 (pts (xy 203.2 52.07) (xy 206.326421 52.07)))
    (feature2 (pts (xy 203.2 71.12) (xy 206.326421 71.12)))
    (crossbar (pts (xy 205.74 71.12) (xy 205.74 52.07)))
    (arrow1a (pts (xy 205.74 52.07) (xy 206.326421 53.196504)))
    (arrow1b (pts (xy 205.74 52.07) (xy 205.153579 53.196504)))
    (arrow2a (pts (xy 205.74 71.12) (xy 206.326421 69.993496)))
    (arrow2b (pts (xy 205.74 71.12) (xy 205.153579 69.993496)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 207.04 80.645 90) (layer Dwgs.User))
    (feature1 (pts (xy 203.2 71.12) (xy 206.326421 71.12)))
    (feature2 (pts (xy 203.2 90.17) (xy 206.326421 90.17)))
    (crossbar (pts (xy 205.74 90.17) (xy 205.74 71.12)))
    (arrow1a (pts (xy 205.74 71.12) (xy 206.326421 72.246504)))
    (arrow1b (pts (xy 205.74 71.12) (xy 205.153579 72.246504)))
    (arrow2a (pts (xy 205.74 90.17) (xy 206.326421 89.043496)))
    (arrow2b (pts (xy 205.74 90.17) (xy 205.153579 89.043496)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 151.1 61.595 90) (layer Dwgs.User))
    (feature1 (pts (xy 154.94 52.07) (xy 151.813579 52.07)))
    (feature2 (pts (xy 154.94 71.12) (xy 151.813579 71.12)))
    (crossbar (pts (xy 152.4 71.12) (xy 152.4 52.07)))
    (arrow1a (pts (xy 152.4 52.07) (xy 152.986421 53.196504)))
    (arrow1b (pts (xy 152.4 52.07) (xy 151.813579 53.196504)))
    (arrow2a (pts (xy 152.4 71.12) (xy 152.986421 69.993496)))
    (arrow2b (pts (xy 152.4 71.12) (xy 151.813579 69.993496)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 151.1 80.645 90) (layer Dwgs.User))
    (feature1 (pts (xy 154.94 71.12) (xy 151.813579 71.12)))
    (feature2 (pts (xy 154.94 90.17) (xy 151.813579 90.17)))
    (crossbar (pts (xy 152.4 90.17) (xy 152.4 71.12)))
    (arrow1a (pts (xy 152.4 71.12) (xy 152.986421 72.246504)))
    (arrow1b (pts (xy 152.4 71.12) (xy 151.813579 72.246504)))
    (arrow2a (pts (xy 152.4 90.17) (xy 152.986421 89.043496)))
    (arrow2b (pts (xy 152.4 90.17) (xy 151.813579 89.043496)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 184.785 82.52) (layer Dwgs.User))
    (feature1 (pts (xy 194.31 91.44) (xy 194.31 83.233579)))
    (feature2 (pts (xy 175.26 91.44) (xy 175.26 83.233579)))
    (crossbar (pts (xy 175.26 83.82) (xy 194.31 83.82)))
    (arrow1a (pts (xy 194.31 83.82) (xy 193.183496 84.406421)))
    (arrow1b (pts (xy 194.31 83.82) (xy 193.183496 83.233579)))
    (arrow2a (pts (xy 175.26 83.82) (xy 176.386504 84.406421)))
    (arrow2b (pts (xy 175.26 83.82) (xy 176.386504 83.233579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 179.07 85.06) (layer Dwgs.User))
    (feature1 (pts (xy 182.88 91.44) (xy 182.88 85.773579)))
    (feature2 (pts (xy 175.26 91.44) (xy 175.26 85.773579)))
    (crossbar (pts (xy 175.26 86.36) (xy 182.88 86.36)))
    (arrow1a (pts (xy 182.88 86.36) (xy 181.753496 86.946421)))
    (arrow1b (pts (xy 182.88 86.36) (xy 181.753496 85.773579)))
    (arrow2a (pts (xy 175.26 86.36) (xy 176.386504 86.946421)))
    (arrow2b (pts (xy 175.26 86.36) (xy 176.386504 85.773579)))
  )
  (dimension 19.05 (width 0.15) (layer Dwgs.User)
    (gr_text "19.050 mm" (at 165.735 82.52) (layer Dwgs.User))
    (feature1 (pts (xy 175.26 91.44) (xy 175.26 83.233579)))
    (feature2 (pts (xy 156.21 91.44) (xy 156.21 83.233579)))
    (crossbar (pts (xy 156.21 83.82) (xy 175.26 83.82)))
    (arrow1a (pts (xy 175.26 83.82) (xy 174.133496 84.406421)))
    (arrow1b (pts (xy 175.26 83.82) (xy 174.133496 83.233579)))
    (arrow2a (pts (xy 156.21 83.82) (xy 157.336504 84.406421)))
    (arrow2b (pts (xy 156.21 83.82) (xy 157.336504 83.233579)))
  )
  (dimension 4.060012 (width 0.15) (layer Dwgs.User)
    (gr_text "4.060 mm" (at 170.893514 39.401509 0.1411223243) (layer Dwgs.User))
    (feature1 (pts (xy 172.93 42.03) (xy 172.925271 40.110086)))
    (feature2 (pts (xy 168.87 42.04) (xy 168.865271 40.120086)))
    (crossbar (pts (xy 168.866716 40.706505) (xy 172.926716 40.696505)))
    (arrow1a (pts (xy 172.926716 40.696505) (xy 171.80166 41.285699)))
    (arrow1b (pts (xy 172.926716 40.696505) (xy 171.798771 40.112861)))
    (arrow2a (pts (xy 168.866716 40.706505) (xy 169.994661 41.290149)))
    (arrow2b (pts (xy 168.866716 40.706505) (xy 169.991772 40.117311)))
  )
  (dimension 5.08 (width 0.15) (layer Dwgs.User)
    (gr_text "5.080 mm" (at 166.31 104.888337) (layer Dwgs.User))
    (feature1 (pts (xy 168.85 101.62) (xy 168.85 104.174758)))
    (feature2 (pts (xy 163.77 101.62) (xy 163.77 104.174758)))
    (crossbar (pts (xy 163.77 103.588337) (xy 168.85 103.588337)))
    (arrow1a (pts (xy 168.85 103.588337) (xy 167.723496 104.174758)))
    (arrow1b (pts (xy 168.85 103.588337) (xy 167.723496 103.001916)))
    (arrow2a (pts (xy 163.77 103.588337) (xy 164.896504 104.174758)))
    (arrow2b (pts (xy 163.77 103.588337) (xy 164.896504 103.001916)))
  )
  (gr_text www.mathcodeprint.com (at 179.07 63.246) (layer F.SilkS))
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "15.240 mm" (at 207.01 36.800001) (layer Dwgs.User))
    (feature1 (pts (xy 199.39 41.91) (xy 199.39 37.51358)))
    (feature2 (pts (xy 214.63 41.91) (xy 214.63 37.51358)))
    (crossbar (pts (xy 214.63 38.100001) (xy 199.39 38.100001)))
    (arrow1a (pts (xy 199.39 38.100001) (xy 200.516504 37.51358)))
    (arrow1b (pts (xy 199.39 38.100001) (xy 200.516504 38.686422)))
    (arrow2a (pts (xy 214.63 38.100001) (xy 213.503496 37.51358)))
    (arrow2b (pts (xy 214.63 38.100001) (xy 213.503496 38.686422)))
  )
  (dimension 15.24 (width 0.15) (layer Dwgs.User)
    (gr_text "15.240 mm" (at 156.21 36.8) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 41.91) (xy 163.83 37.513579)))
    (feature2 (pts (xy 148.59 41.91) (xy 148.59 37.513579)))
    (crossbar (pts (xy 148.59 38.1) (xy 163.83 38.1)))
    (arrow1a (pts (xy 163.83 38.1) (xy 162.703496 38.686421)))
    (arrow1b (pts (xy 163.83 38.1) (xy 162.703496 37.513579)))
    (arrow2a (pts (xy 148.59 38.1) (xy 149.716504 38.686421)))
    (arrow2b (pts (xy 148.59 38.1) (xy 149.716504 37.513579)))
  )
  (dimension 17.78 (width 0.15) (layer Dwgs.User)
    (gr_text "17.780 mm" (at 172.72 36.8) (layer Dwgs.User))
    (feature1 (pts (xy 163.83 41.91) (xy 163.83 37.513579)))
    (feature2 (pts (xy 181.61 41.91) (xy 181.61 37.513579)))
    (crossbar (pts (xy 181.61 38.1) (xy 163.83 38.1)))
    (arrow1a (pts (xy 163.83 38.1) (xy 164.956504 37.513579)))
    (arrow1b (pts (xy 163.83 38.1) (xy 164.956504 38.686421)))
    (arrow2a (pts (xy 181.61 38.1) (xy 180.483496 37.513579)))
    (arrow2b (pts (xy 181.61 38.1) (xy 180.483496 38.686421)))
  )
  (dimension 17.78 (width 0.15) (layer Dwgs.User)
    (gr_text "17.780 mm" (at 190.5 36.8) (layer Dwgs.User))
    (feature1 (pts (xy 181.61 41.91) (xy 181.61 37.513579)))
    (feature2 (pts (xy 199.39 41.91) (xy 199.39 37.513579)))
    (crossbar (pts (xy 199.39 38.1) (xy 181.61 38.1)))
    (arrow1a (pts (xy 181.61 38.1) (xy 182.736504 37.513579)))
    (arrow1b (pts (xy 181.61 38.1) (xy 182.736504 38.686421)))
    (arrow2a (pts (xy 199.39 38.1) (xy 198.263496 37.513579)))
    (arrow2b (pts (xy 199.39 38.1) (xy 198.263496 38.686421)))
  )
  (dimension 8.89 (width 0.12) (layer Dwgs.User)
    (gr_text "8.890 mm" (at 226.06 93.345 270) (layer Dwgs.User))
    (feature1 (pts (xy 219.71 97.79) (xy 225.376421 97.79)))
    (feature2 (pts (xy 219.71 88.9) (xy 225.376421 88.9)))
    (crossbar (pts (xy 224.79 88.9) (xy 224.79 97.79)))
    (arrow1a (pts (xy 224.79 97.79) (xy 224.203579 96.663496)))
    (arrow1b (pts (xy 224.79 97.79) (xy 225.376421 96.663496)))
    (arrow2a (pts (xy 224.79 88.9) (xy 224.203579 90.026504)))
    (arrow2b (pts (xy 224.79 88.9) (xy 225.376421 90.026504)))
  )
  (dimension 8.89 (width 0.12) (layer Dwgs.User)
    (gr_text "8.890 mm" (at 226.06 48.895 90) (layer Dwgs.User))
    (feature1 (pts (xy 219.71 44.45) (xy 225.376421 44.45)))
    (feature2 (pts (xy 219.71 53.34) (xy 225.376421 53.34)))
    (crossbar (pts (xy 224.79 53.34) (xy 224.79 44.45)))
    (arrow1a (pts (xy 224.79 44.45) (xy 225.376421 45.576504)))
    (arrow1b (pts (xy 224.79 44.45) (xy 224.203579 45.576504)))
    (arrow2a (pts (xy 224.79 53.34) (xy 225.376421 52.213496)))
    (arrow2b (pts (xy 224.79 53.34) (xy 224.203579 52.213496)))
  )
  (gr_text Xs&Os (at 180.34 78.74) (layer F.SilkS))
  (gr_text @mathcodeprint (at 204.47 71.12 270) (layer F.SilkS))
  (dimension 17.78 (width 0.12) (layer Dwgs.User)
    (gr_text "17.780 mm" (at 226.06 62.23 90) (layer Dwgs.User))
    (feature1 (pts (xy 219.71 53.34) (xy 225.376421 53.34)))
    (feature2 (pts (xy 219.71 71.12) (xy 225.376421 71.12)))
    (crossbar (pts (xy 224.79 71.12) (xy 224.79 53.34)))
    (arrow1a (pts (xy 224.79 53.34) (xy 225.376421 54.466504)))
    (arrow1b (pts (xy 224.79 53.34) (xy 224.203579 54.466504)))
    (arrow2a (pts (xy 224.79 71.12) (xy 225.376421 69.993496)))
    (arrow2b (pts (xy 224.79 71.12) (xy 224.203579 69.993496)))
  )
  (dimension 17.78 (width 0.12) (layer Dwgs.User)
    (gr_text "17.780 mm" (at 226.06 80.01 270) (layer Dwgs.User))
    (feature1 (pts (xy 219.71 88.9) (xy 225.376421 88.9)))
    (feature2 (pts (xy 219.71 71.12) (xy 225.376421 71.12)))
    (crossbar (pts (xy 224.79 71.12) (xy 224.79 88.9)))
    (arrow1a (pts (xy 224.79 88.9) (xy 224.203579 87.773496)))
    (arrow1b (pts (xy 224.79 88.9) (xy 225.376421 87.773496)))
    (arrow2a (pts (xy 224.79 71.12) (xy 224.203579 72.246504)))
    (arrow2b (pts (xy 224.79 71.12) (xy 225.376421 72.246504)))
  )
  (dimension 53.34 (width 0.12) (layer Dwgs.User)
    (gr_text "53.340 mm" (at 133.35 71.12 90) (layer Dwgs.User))
    (feature1 (pts (xy 140.97 44.45) (xy 134.033579 44.45)))
    (feature2 (pts (xy 140.97 97.79) (xy 134.033579 97.79)))
    (crossbar (pts (xy 134.62 97.79) (xy 134.62 44.45)))
    (arrow1a (pts (xy 134.62 44.45) (xy 135.206421 45.576504)))
    (arrow1b (pts (xy 134.62 44.45) (xy 134.033579 45.576504)))
    (arrow2a (pts (xy 134.62 97.79) (xy 135.206421 96.663496)))
    (arrow2b (pts (xy 134.62 97.79) (xy 134.033579 96.663496)))
  )
  (dimension 68.58 (width 0.12) (layer Dwgs.User)
    (gr_text "68.580 mm" (at 182.88 111.760468) (layer Dwgs.User))
    (feature1 (pts (xy 217.17 102.87) (xy 217.17 111.076889)))
    (feature2 (pts (xy 148.59 102.87) (xy 148.59 111.076889)))
    (crossbar (pts (xy 148.59 110.490468) (xy 217.17 110.490468)))
    (arrow1a (pts (xy 217.17 110.490468) (xy 216.043496 111.076889)))
    (arrow1b (pts (xy 217.17 110.490468) (xy 216.043496 109.904047)))
    (arrow2a (pts (xy 148.59 110.490468) (xy 149.716504 111.076889)))
    (arrow2b (pts (xy 148.59 110.490468) (xy 149.716504 109.904047)))
  )
)
