(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 135)
    (no_connects 1)
    (area 144.924999 49.924999 245.075001 72.075001)
    (thickness 1.6)
    (drawings 22)
    (tracks 466)
    (zones 0)
    (modules 68)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory PDF/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +170v)
  (net 4 +5V)
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C5-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 +12V)
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C10-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 +3V3)
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C15-Pad1)")
  (net 15 "Net-(D3-Pad2)")
  (net 16 BL)
  (net 17 LE)
  (net 18 ~DATA)
  (net 19 ~CLK)
  (net 20 ESP_RX)
  (net 21 ESP_TX)
  (net 22 ESP_EN)
  (net 23 ESP_BOOT)
  (net 24 "Net-(Q1-Pad4)")
  (net 25 "Net-(Q1-Pad1)")
  (net 26 "Net-(Q2-Pad1)")
  (net 27 "Net-(Q3-Pad1)")
  (net 28 "Net-(Q4-Pad1)")
  (net 29 "Net-(Q5-Pad1)")
  (net 30 "Net-(Q26-Pad1)")
  (net 31 ~HV_ENABLE)
  (net 32 "Net-(R3-Pad2)")
  (net 33 ~BL)
  (net 34 DATA)
  (net 35 ~LE)
  (net 36 CLK)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +170v)
    (add_net +3V3)
    (add_net +5V)
    (add_net BL)
    (add_net CLK)
    (add_net DATA)
    (add_net ESP_BOOT)
    (add_net ESP_EN)
    (add_net ESP_RX)
    (add_net ESP_TX)
    (add_net GND)
    (add_net LE)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q26-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net ~BL)
    (add_net ~CLK)
    (add_net ~DATA)
    (add_net ~HV_ENABLE)
    (add_net ~LE)
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 5B432F1A)
    (at 198 52.8 180)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at 0 -3.24 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 5.01 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35 270) (size 2 0.4) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -0.65 -1.35 270) (size 2 0.4) (layers F.Cu F.Mask))
    (pad 3 smd rect (at 0 -1.35 270) (size 2 0.4) (layers F.Cu F.Mask))
    (pad 4 smd rect (at 0.65 -1.35 270) (size 2 0.4) (layers F.Cu F.Mask))
    (pad 5 smd rect (at 1.3 -1.35 270) (size 2 0.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 -1.35 270) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.5 -1.35 270) (size 1.3 1.3) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -3.5 1.35 270) (size 1.65 1.65) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 3.5 1.35 270) (size 1.65 1.65) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module footprints:ESP32-wroom (layer F.Cu) (tedit 5B432EDF)
    (at 229 49)
    (fp_text reference U4 (at 0 5.4) (layer F.Fab) hide)
    (fp_text value ESP32-Wroom (at 0 3) (layer F.SilkS))
    (pad 1 smd rect (at -9.49 2.54) (size 2 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -9.49 3.81) (size 2 0.9) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (pad 3 smd rect (at -9.49 5.08) (size 2 0.9) (layers F.Cu F.Mask)
      (net 22 ESP_EN))
    (pad 4 smd rect (at -9.49 6.35) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 5 smd rect (at -9.49 7.62) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 6 smd rect (at -9.49 8.89) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 7 smd rect (at -9.49 10.16) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 8 smd rect (at -9.49 11.43) (size 2 0.9) (layers F.Cu F.Mask)
      (net 33 ~BL))
    (pad 9 smd rect (at -9.49 12.7) (size 2 0.9) (layers F.Cu F.Mask)
      (net 35 ~LE))
    (pad 10 smd rect (at -9.49 13.97) (size 2 0.9) (layers F.Cu F.Mask)
      (net 36 CLK))
    (pad 11 smd rect (at -9.49 15.24) (size 2 0.9) (layers F.Cu F.Mask)
      (net 34 DATA))
    (pad 12 smd rect (at -9.49 16.51) (size 2 0.9) (layers F.Cu F.Mask)
      (net 31 ~HV_ENABLE))
    (pad 13 smd rect (at -9.49 17.78) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 14 smd rect (at -9.49 19.05) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 15 smd rect (at -5.715 21.09) (size 0.9 2) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -4.445 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 17 smd rect (at -3.175 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 18 smd rect (at -1.905 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 19 smd rect (at -0.635 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 20 smd rect (at 0.635 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 21 smd rect (at 1.905 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 22 smd rect (at 3.175 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 23 smd rect (at 4.445 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 24 smd rect (at 5.715 21.09) (size 0.9 2) (layers F.Cu F.Mask))
    (pad 25 smd rect (at 9.545 19.05) (size 2 0.9) (layers F.Cu F.Mask)
      (net 23 ESP_BOOT))
    (pad 26 smd rect (at 9.545 17.78) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 27 smd rect (at 9.545 16.51) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 28 smd rect (at 9.545 15.24) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 29 smd rect (at 9.545 13.97) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 30 smd rect (at 9.545 12.7) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 31 smd rect (at 9.545 11.43) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 32 smd rect (at 9.545 10.16) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 33 smd rect (at 9.545 8.89) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 34 smd rect (at 9.545 7.62) (size 2 0.9) (layers F.Cu F.Mask)
      (net 20 ESP_RX))
    (pad 35 smd rect (at 9.545 6.35) (size 2 0.9) (layers F.Cu F.Mask)
      (net 21 ESP_TX))
    (pad 36 smd rect (at 9.545 5.08) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 37 smd rect (at 9.545 3.81) (size 2 0.9) (layers F.Cu F.Mask))
    (pad 38 smd rect (at 9.545 2.54) (size 2 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Diodes_SMD:D_SMA (layer B.Cu) (tedit 586432E5)
    (at 168 61.6 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D1 (at 4.424 -0.122 180) (layer B.SilkS))
    (fp_text value ES1D (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 191.6 68.4 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 3.1 0.4 180) (layer F.SilkS))
    (fp_text value BAT54 (at 0.1 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5B40E85D)
    (at 186.864 52.07 180)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference BOOT (at 2.206 -2.794 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 180) (layer F.Fab))
    (pad 2 smd rect (at 5 0 180) (size 2 1.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5 0 180) (size 2 1.4) (layers F.Cu F.Mask)
      (net 23 ESP_BOOT))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQPE1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 5B412985)
    (at 174.244 52.07 180)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference RESET (at 2.54 -2.794 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 180) (layer F.Fab))
    (pad 2 smd rect (at 5 0 180) (size 2 1.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -5 0 180) (size 2 1.4) (layers F.Cu F.Mask)
      (net 22 ESP_EN))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_EVQPE1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 188 59.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.538 0.548 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 30 "Net-(Q26-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer B.Cu) (tedit 58AA8525)
    (at 167.2 55 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C1 (at 0.136 -0.068 90) (layer B.SilkS))
    (fp_text value "1u 250V" (at 0 -2.75 90) (layer B.Fab))
    (fp_text user %R (at 0 2.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MBRM140T3G (layer B.Cu) (tedit 5B3E0FB1)
    (at 201.2 62.8 180)
    (fp_text reference D3 (at 0.286 2.094 180) (layer B.SilkS))
    (fp_text value MBRM140T3G (at -0.1 2.5 180) (layer B.Fab))
    (fp_text user A (at 2.1 -0.8 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.9 0 180) (size 1.27 1.27) (layers B.Cu B.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2.3 0 180) (size 2.54 2.54) (layers B.Cu B.Mask)
      (net 8 +12V))
  )
  (module footprints:murata10uH (layer B.Cu) (tedit 5B3E0CDE)
    (at 195.8 63.4)
    (fp_text reference L1 (at 0 -1.8) (layer B.SilkS))
    (fp_text value 10u (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 1.3 0) (size 1.5 2) (layers B.Cu B.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -1.4 0) (size 1.5 2) (layers B.Cu B.Mask)
      (net 4 +5V))
  )
  (module WE33uHcut (layer F.Cu) (tedit 5B4320AD)
    (at 156 61)
    (fp_text reference L3 (at -4 7) (layer F.Fab) hide)
    (fp_text value 33u (at -7 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -7.2) (size 5 2) (layers F.Cu F.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0 7.2) (size 5 2) (layers F.Cu F.Mask)
      (net 9 "Net-(C9-Pad1)"))
  )
  (module Capacitors_SMD:C_1812_HandSoldering (layer B.Cu) (tedit 58AA8525)
    (at 170.6 55 90)
    (descr "Capacitor SMD 1812, hand soldering")
    (tags "capacitor 1812")
    (attr smd)
    (fp_text reference C2 (at 0.136 0.088 90) (layer B.SilkS))
    (fp_text value "1u 250V" (at 0 -2.75 90) (layer B.Fab))
    (fp_text user %R (at 0 2.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2.9 0 90) (size 2.2 3) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.9 0 90) (size 2.2 3) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1812.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 152.2 51.6)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.248 0.216) (layer B.SilkS))
    (fp_text value "0.1u 250V" (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 3 +170v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 191.4 66.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.094 -1.662 90) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 177 53)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.216 -1.692) (layer B.SilkS))
    (fp_text value 220p (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 175.6 56.6 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -3.09 -0.34 90) (layer B.SilkS))
    (fp_text value "100p 250V" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 179.2 68.8 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.124 -1.812 180) (layer B.SilkS))
    (fp_text value 430p (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 205 67 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.056 -2.01 270) (layer B.SilkS))
    (fp_text value 10u (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 8 +12V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 167 66.2)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 0 -2.25) (layer F.SilkS))
    (fp_text value "100u 16V" (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B3F85D6)
    (at 177.546 64.4 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.8 0.2 270) (layer F.SilkS))
    (fp_text value "0.1u 16V" (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 174.4 68.8 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -0.098 -1.812 180) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 173.8 56.6 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 4.022 0.19 90) (layer B.SilkS))
    (fp_text value "0.1u 250V" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 210.6 59.8 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0.11 1.998 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5B3F85DC)
    (at 182.2 64.4 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C14 (at 0.4 -2.4 270) (layer F.SilkS))
    (fp_text value "47u 16V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 167.6 69.4)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 1.25) (layer B.SilkS))
    (fp_text value "560p 250V" (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.25) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 190.8 60 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C16 (at 4.008 0.808 360) (layer F.SilkS))
    (fp_text value "100u 16V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 207.4 60.8 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C17 (at 3.142 -2.422 90) (layer F.SilkS))
    (fp_text value 100u (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 193.4 60 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B3F842C)
    (at 147 58.54 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at -2.098 0.688 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +170v))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B3F8437)
    (at 147 63.46)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 2.098 0.608 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 205 52 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J5 (at 0.184 12.17 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 ESP_BOOT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 ESP_EN))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 ESP_TX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 ESP_RX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 180.2 60)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value "60Ohm 100MHz" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 152.2 53.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L5 (at -3.102 0.448) (layer B.SilkS))
    (fp_text value "60Ohm 100MHz" (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 3 +170v))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer B.Cu) (tedit 0)
    (at 167.8 66.4 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference Q1 (at 0 -0.094 270) (layer B.SilkS))
    (fp_text value FDS2672 (at 0 -1.27 270) (layer B.Fab))
    (pad 8 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 7 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 6 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 5 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 14 "Net-(C15-Pad1)"))
    (pad 4 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 24 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 25 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 25 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers B.Cu B.Mask)
      (net 25 "Net-(Q1-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 229 53.6)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 2.14 -1.784) (layer B.SilkS))
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 26 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 16 BL))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 229 61.6)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 2.14 2.154) (layer B.SilkS))
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 27 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 18 ~DATA))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 229 57.6)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 1.886 1.836) (layer B.SilkS))
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 28 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 17 LE))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 229 65.6)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 2.5) (layer B.SilkS))
    (fp_text value BSS138 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 29 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Mask)
      (net 19 ~CLK))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 194.4 65.6)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q26 (at 0.926 2.472) (layer F.SilkS))
    (fp_text value MMBTA42 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Mask)
      (net 30 "Net-(Q26-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 208.6 67.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 30 "Net-(Q26-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 31 ~HV_ENABLE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 179.8 65 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.484 -1.81 270) (layer B.SilkS))
    (fp_text value 60.4K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 201.2 65.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -5.302 1.792 180) (layer B.SilkS))
    (fp_text value 40.2K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 +12V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 201.2 68.2)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 234.4 53.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 16 BL))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 185.4 60.6 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -1.418 1.758 270) (layer F.SilkS))
    (fp_text value 2K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 175.4 65 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.024 0.648 270) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 25 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B3F85D0)
    (at 179.578 64.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.6 -0.2 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 173.2 65 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -3.532 0.226 270) (layer B.SilkS))
    (fp_text value "0.1 1/2W" (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 25 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 234.4 61.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 18 ~DATA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 177.6 65 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.786 -0.562 90) (layer B.SilkS))
    (fp_text value 4.12K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 223.8 54.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 26 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 33 ~BL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 223.8 62.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 27 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 34 DATA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 177.6 56.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at -3.598 0.708 90) (layer B.SilkS))
    (fp_text value 634K (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 179.4 56.6 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0.042 -1.702 270) (layer B.SilkS))
    (fp_text value 7.68K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 234.4 57.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 17 LE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 234.4 65.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 19 ~CLK))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 8 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 223.8 58.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 28 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 35 ~LE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 223.8 66.6 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 29 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Mask)
      (net 36 CLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5B3F859F)
    (at 180 54.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 1.8) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 22 ESP_EN))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189 54.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 23 ESP_BOOT))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 170.8 58.6 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -3.63 -0.112 180) (layer F.SilkS))
    (fp_text value UCC3803 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 10 "Net-(C10-Pad1)"))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 9 "Net-(C9-Pad1)"))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 24 "Net-(Q1-Pad4)"))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 6 "Net-(C5-Pad2)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 195.8 67 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U2 (at 0 -2.596 180) (layer B.SilkS))
    (fp_text value MIC2288 (at 0 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Mask)
      (net 32 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Mask)
      (net 4 +5V))
    (pad 5 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-5 (layer F.Cu) (tedit 591C8E70)
    (at 201.4 62.2 90)
    (descr "module CMS SOT223 5 pins, http://ww1.microchip.com/downloads/en/DeviceDoc/51751a.pdf")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0.0625 -4.5 90) (layer F.SilkS))
    (fp_text value LP38690 (at 0.0625 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 4 smd rect (at -3.05 2.25 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at -3.05 -0.75 90) (size 2.2 1) (layers F.Cu F.Mask))
    (pad 5 smd rect (at 3.25 0 90) (size 1.8 3.4) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.05 0.75 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 12 +3V3))
    (pad 1 smd rect (at -3.05 -2.25 90) (size 2.2 1) (layers F.Cu F.Mask)
      (net 4 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223-5.wrl
      (at (xyz 0.0024606299 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B40E8D0)
    (at 243 52)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B40E8CD)
    (at 243 70)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B40E7FA)
    (at 147 70)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0.066 3.66) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 5B431D4C)
    (at 147 52)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380_Pad (at 1 -4.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 243 66 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 1.954 -0.04 270) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 0 12.49 180) (layer F.Fab))
    (fp_text user %R (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 ~CLK))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 ~DATA))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 LE))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 BL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "High Voltage\nBy surfncircuits.com" (at 185.5 60.5 90) (layer B.SilkS))
  (gr_text "mini-nixie       pierremuth.wordpress.com" (at 185 70.5) (layer F.Mask))
  (gr_text "CUT OUT" (at 156 61) (layer Cmts.User))
  (dimension 22 (width 0.3) (layer Cmts.User)
    (gr_text "22.000 mm" (at 129.65 61 90) (layer Cmts.User))
    (feature1 (pts (xy 145 50) (xy 128.3 50)))
    (feature2 (pts (xy 145 72) (xy 128.3 72)))
    (crossbar (pts (xy 131 72) (xy 131 50)))
    (arrow1a (pts (xy 131 50) (xy 131.586421 51.126504)))
    (arrow1b (pts (xy 131 50) (xy 130.413579 51.126504)))
    (arrow2a (pts (xy 131 72) (xy 131.586421 70.873496)))
    (arrow2b (pts (xy 131 72) (xy 130.413579 70.873496)))
  )
  (dimension 100 (width 0.3) (layer Cmts.User)
    (gr_text "100.000 mm" (at 195 34.65) (layer Cmts.User))
    (feature1 (pts (xy 245 50) (xy 245 33.3)))
    (feature2 (pts (xy 145 50) (xy 145 33.3)))
    (crossbar (pts (xy 145 36) (xy 245 36)))
    (arrow1a (pts (xy 245 36) (xy 243.873496 36.586421)))
    (arrow1b (pts (xy 245 36) (xy 243.873496 35.413579)))
    (arrow2a (pts (xy 145 36) (xy 146.126504 36.586421)))
    (arrow2b (pts (xy 145 36) (xy 146.126504 35.413579)))
  )
  (gr_text RX (at 215.138 54.864 90) (layer F.SilkS))
  (gr_text TX (at 212.598 54.864 90) (layer F.SilkS))
  (gr_text reset (at 210.058 54.864 90) (layer F.SilkS))
  (gr_text boot (at 207.518 54.864 90) (layer F.SilkS))
  (gr_text GND (at 204.978 54.864 90) (layer F.SilkS))
  (gr_line (start 150.062 67) (end 150.062 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.062 67) (end 150.062 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.062 55) (end 162.062 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.062 55) (end 162.062 55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 72) (end 145 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245 72) (end 245 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245 50) (end 145 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245 70) (end 245 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 72) (end 245 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 50) (end 145 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 145.5 50.5) (xy 244.5 50.5) (xy 244.5 71.5) (xy 145.5 71.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 163 53) (xy 163 69) (xy 162 70) (xy 153 70) (xy 150 67)
        (xy 150 55) (xy 153 52) (xy 162 52)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 244.5 50.5) (xy 188 50.5) (xy 188 71.5) (xy 244.5 71.5)
      )
    )
  )
)
