(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 77.196 108.204)
		(grid_origin 77.196 108.204)
		(pcbplotparams
			(layerselection 0x000000c_7ffffff8)
			(plot_on_all_layers_selection 0x0001000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes no)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "CAM/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(U1-IMON_IN)")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "Net-(U1-IMON_OUT)")
	(net 5 "Net-(C5-Pad2)")
	(net 6 "Net-(U1-Vc)")
	(net 7 "Net-(U1-SS)")
	(net 8 "Net-(U1-CSNIN)")
	(net 9 "/VCCx")
	(net 10 "Net-(U1-CSPIN)")
	(net 11 "Net-(C14-Pad1)")
	(net 12 "Net-(U1-LDO33)")
	(net 13 "Net-(C15-Pad1)")
	(net 14 "Net-(D4-K)")
	(net 15 "/CSN")
	(net 16 "/CSP")
	(net 17 "Net-(D5-K)")
	(net 18 "Net-(U1-CSPOUT)")
	(net 19 "Net-(U1-CSNOUT)")
	(net 20 "Net-(U1-SW2)")
	(net 21 "Net-(U1-SW1)")
	(net 22 "unconnected-(L1-Pad3)")
	(net 23 "unconnected-(L3-Pad3)")
	(net 24 "unconnected-(L4-Pad3)")
	(net 25 "Net-(R36-Pad1)")
	(net 26 "Net-(O1-C)")
	(net 27 "Net-(O1-A)")
	(net 28 "Net-(Q1-G)")
	(net 29 "Net-(Q2-S-Pad2)")
	(net 30 "Net-(Q2-G)")
	(net 31 "Net-(Q3-G)")
	(net 32 "/Vin_9_30")
	(net 33 "/Vout_28")
	(net 34 "Net-(Q4-G)")
	(net 35 "/LT8705_ENA")
	(net 36 "Net-(U1-FBIN)")
	(net 37 "/LT8705_SYNC")
	(net 38 "Net-(U1-MODE)")
	(net 39 "Net-(U1-RT)")
	(net 40 "Net-(U1-SWEN)")
	(net 41 "Net-(U1-TG1)")
	(net 42 "Net-(U1-BG1)")
	(net 43 "Net-(U1-BG2)")
	(net 44 "Net-(U1-TG2)")
	(net 45 "Net-(U1-FBOUT)")
	(net 46 "Net-(U1-CLKOUT)")
	(net 47 "Net-(U1-SRVO_FBIN)")
	(net 48 "Net-(U1-SRVO_IIN)")
	(net 49 "Net-(U1-SRVO_FBOUT)")
	(net 50 "Net-(U1-SRVO_IOUT)")
	(net 51 "Net-(J1-Pad1)")
	(net 52 "Net-(D1-A)")
	(net 53 "Net-(D1-K)")
	(net 54 "Net-(R25-Pad1)")
	(net 55 "Net-(R26-Pad1)")
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 96.246 101.727)
		(property "Reference" "TP4"
			(at -2.54 0.1905 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(U1-CLKOUT)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 99.929 87.63)
		(property "Reference" "TP1"
			(at 2.286 0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1-LDO33)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 98.151 92.329 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R38"
			(at 3.048 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 0.9652 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(U1-FBOUT)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 124.059 102.362 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R37"
			(at 2.7305 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "221K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(U1-FBOUT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(R36-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 124.059 99.441 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R36"
			(at -2.8575 -0.0635 90)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(R36-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_1206"
		(layer "F.Cu")
		(at 148.062 75.438)
		(descr "SMT resistor, 1206")
		(property "Reference" "R35"
			(at 3.937 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "2"
			(at 0 1.6002 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(U1-TG2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(Q3-G)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_1206.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_1206"
		(layer "F.Cu")
		(at 148.062 78.232)
		(descr "SMT resistor, 1206")
		(property "Reference" "R33"
			(at 4.445 0.127 360)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.6002 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(U1-BG2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(Q4-G)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_1206.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 116.82 94.615)
		(property "Reference" "TP5"
			(at 0 1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(U1-SRVO_FBIN)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 114.28 94.615)
		(property "Reference" "TP6"
			(at -2.286 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(U1-SRVO_IIN)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 114.28 92.075)
		(property "Reference" "TP7"
			(at -2.286 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(U1-SRVO_FBOUT)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 116.82 92.202)
		(property "Reference" "TP8"
			(at 2.159 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(U1-SRVO_IOUT)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 126.091 98.552)
		(property "Reference" "TP9"
			(at 2.032 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/Vout_28")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 126.091 100.584)
		(property "Reference" "TP10"
			(at 2.4765 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(R36-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_qfn:QFN_38"
		(layer "F.Cu")
		(at 105.771 93.599)
		(property "Reference" "U1"
			(at 2.032 -5 0)
			(layer "F.SilkS")
		)
		(property "Value" "LT8705EUHF"
			(at 0 5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_qfn:QFN_38"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(pad "" smd rect
			(at 0 0)
			(size 3 5)
			(layers "F.Mask")
		)
		(pad "1" smd oval
			(at -2.5 -2.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/LT8705_ENA")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "2" smd oval
			(at -2.5 -2.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/CSN")
			(pinfunction "CSN")
			(pintype "input")
		)
		(pad "3" smd oval
			(at -2.5 -1.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/CSP")
			(pinfunction "CSP")
			(pintype "input")
		)
		(pad "4" smd oval
			(at -2.5 -1.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-LDO33)")
			(pinfunction "LDO33")
			(pintype "input")
		)
		(pad "5" smd oval
			(at -2.5 -0.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(U1-FBIN)")
			(pinfunction "FBIN")
			(pintype "input")
		)
		(pad "6" smd oval
			(at -2.5 -0.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(U1-FBOUT)")
			(pinfunction "FBOUT")
			(pintype "input")
		)
		(pad "7" smd oval
			(at -2.5 0.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-IMON_OUT)")
			(pinfunction "IMON_OUT")
			(pintype "input")
		)
		(pad "8" smd oval
			(at -2.5 0.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-Vc)")
			(pinfunction "Vc")
			(pintype "input")
		)
		(pad "9" smd oval
			(at -2.5 1.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U1-SS)")
			(pinfunction "SS")
			(pintype "input")
		)
		(pad "10" smd oval
			(at -2.5 1.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(U1-CLKOUT)")
			(pinfunction "CLKOUT")
			(pintype "input")
		)
		(pad "11" smd oval
			(at -2.5 2.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/LT8705_SYNC")
			(pinfunction "SYNC")
			(pintype "input")
		)
		(pad "12" smd oval
			(at -2.5 2.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U1-RT)")
			(pinfunction "RT")
			(pintype "input")
		)
		(pad "13" smd oval
			(at -1.5 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "14" smd oval
			(at -1 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(U1-BG1)")
			(pinfunction "BG1")
			(pintype "input")
		)
		(pad "15" smd oval
			(at -0.5 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pinfunction "GATEVcc")
			(pintype "input")
		)
		(pad "16" smd oval
			(at 0 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(U1-BG2)")
			(pinfunction "BG2")
			(pintype "input")
		)
		(pad "17" smd oval
			(at 0.5 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D4-K)")
			(pinfunction "BOOST2")
			(pintype "input")
		)
		(pad "18" smd oval
			(at 1 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(U1-TG2)")
			(pinfunction "TG2")
			(pintype "input")
		)
		(pad "19" smd oval
			(at 1.5 3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(U1-SW2)")
			(pinfunction "SW2")
			(pintype "input")
		)
		(pad "20" smd oval
			(at 2.5 2.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "21" smd oval
			(at 2.5 2.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-SW1)")
			(pinfunction "SW1")
			(pintype "input")
		)
		(pad "22" smd oval
			(at 2.5 1.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U1-TG1)")
			(pinfunction "TG1")
			(pintype "input")
		)
		(pad "23" smd oval
			(at 2.5 1.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(D5-K)")
			(pinfunction "BOOST1")
			(pintype "input")
		)
		(pad "24" smd oval
			(at 2.5 0.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "25" smd oval
			(at 2.5 0.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "Net-(U1-SRVO_FBIN)")
			(pinfunction "SRVO_FBIN")
			(pintype "input")
		)
		(pad "26" smd oval
			(at 2.5 -0.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(U1-SRVO_IIN)")
			(pinfunction "SRVO_IIN")
			(pintype "input")
		)
		(pad "27" smd oval
			(at 2.5 -0.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(U1-SRVO_IOUT)")
			(pinfunction "SRVO_IOUT")
			(pintype "input")
		)
		(pad "28" smd oval
			(at 2.5 -1.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "Net-(U1-SRVO_FBOUT)")
			(pinfunction "SRVO_FBOUT")
			(pintype "input")
		)
		(pad "29" smd oval
			(at 2.5 -1.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pinfunction "EXTVcc")
			(pintype "input")
		)
		(pad "30" smd oval
			(at 2.5 -2.25 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(U1-CSNOUT)")
			(pinfunction "CSNOUT")
			(pintype "input")
		)
		(pad "31" smd oval
			(at 2.5 -2.75 90)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pinfunction "CSPOUT")
			(pintype "input")
		)
		(pad "32" smd oval
			(at 1.5 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pinfunction "CSNIN")
			(pintype "input")
		)
		(pad "33" smd oval
			(at 1 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-CSPIN)")
			(pinfunction "CSPIN")
			(pintype "input")
		)
		(pad "34" smd oval
			(at 0.5 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pinfunction "Vin")
			(pintype "input")
		)
		(pad "35" smd oval
			(at 0 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(D1-A)")
			(pinfunction "INTVcc")
			(pintype "input")
		)
		(pad "36" smd oval
			(at -0.5 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U1-SWEN)")
			(pinfunction "SWEN")
			(pintype "input")
		)
		(pad "37" smd oval
			(at -1 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U1-MODE)")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "38" smd oval
			(at -1.5 -3.5)
			(size 0.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U1-IMON_IN)")
			(pinfunction "IMON_IN")
			(pintype "input")
		)
		(pad "39" smd rect
			(at -0.75 -1.25)
			(size 1.4 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "input")
		)
		(pad "39" smd rect
			(at -0.75 1.25)
			(size 1.4 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "input")
		)
		(pad "39" smd rect
			(at 0.75 -1.25)
			(size 1.4 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "input")
		)
		(pad "39" smd rect
			(at 0.75 1.25)
			(size 1.4 2.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_qfn/QFN-38.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "t_coilcraft:SER1052"
		(layer "F.Cu")
		(at 115.042 57.531)
		(property "Reference" "L3"
			(at 4.191 -7.747 0)
			(layer "F.SilkS")
		)
		(property "Value" "SER1502"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:SER1052"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/44def4ed-de67-43fc-a47d-dc1f7beabb27/ser1052.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -3 4.1)
			(size 3 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 3 4.1)
			(size 3 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pinfunction "2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -4.45)
			(size 3.2 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "unconnected-(L3-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-SER1052.STEP"
			(offset
				(xyz 0 0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_coilcraft:SER1052"
		(layer "F.Cu")
		(at 156.269 57.531)
		(property "Reference" "L4"
			(at -4.064 -7.874 0)
			(layer "F.SilkS")
		)
		(property "Value" "SER1502-102"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:SER1052"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/44def4ed-de67-43fc-a47d-dc1f7beabb27/ser1052.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -3 4.1)
			(size 3 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 3 4.1)
			(size 3 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pinfunction "2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -4.45)
			(size 3.2 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(L4-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-SER1052.STEP"
			(offset
				(xyz 0 0.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_passive_smd:res_0805"
		(layer "F.Cu")
		(at 91.547 77.47 90)
		(descr "SMT resistor, 0805")
		(property "Reference" "R14"
			(at 3.236 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 1.3208 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(J1-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(O1-A)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 99.929 83.947)
		(property "Reference" "TP11"
			(at 0.635 -2.667 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/LT8705_ENA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 106.787 85.471 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C12"
			(at -2.794 0.0635 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 111.232 84.582 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C13"
			(at 4.318 -0.508 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 108.438 102.87 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C14"
			(at 2.7305 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D4-K)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 112.629 99.314)
		(descr "SMT resistor, 0603")
		(property "Reference" "C15"
			(at -2.794 -0.1905 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(D5-K)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 98.278 96.647)
		(descr "SMT resistor, 0603")
		(property "Reference" "C7"
			(at 2.286 0.0635 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000pF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-Vc)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 103.358 70.993 -90)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C8"
			(at 4.826 -6.985 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "PCE4439CT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 90)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 90)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 98.278 99.441)
		(descr "SMT resistor, 0603")
		(property "Reference" "C9"
			(at 2.159 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.011 -0.114 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(U1-SS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 91.547 60.96 90)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C6"
			(at 7.239 4.445 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "PCE4439CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 98.278 98.044)
		(descr "SMT resistor, 0603")
		(property "Reference" "C5"
			(at 2.2225 -0.0635 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.033uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-Vc)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 103.358 57.404 90)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C4"
			(at 7.366 4.826 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "PCE4439CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 98.266 95.25)
		(descr "SMT resistor, 0603")
		(property "Reference" "C3"
			(at 2.2345 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.033uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.115 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-IMON_OUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 94.468 96.647)
		(descr "SMT resistor, 0603")
		(property "Reference" "C2"
			(at -3.2385 1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 103.358 85.471 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C1"
			(at -3.175 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.033uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U1-IMON_IN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_1206"
		(layer "F.Cu")
		(at 122.916 78.359 180)
		(descr "SMT resistor, 1206")
		(property "Reference" "R20"
			(at 4.318 0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.6002 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(U1-BG1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(Q2-G)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_1206.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_1206"
		(layer "F.Cu")
		(at 122.916 75.438 180)
		(descr "SMT resistor, 1206")
		(property "Reference" "R19"
			(at 4.445 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2"
			(at 0 1.6002 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U1-TG1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0 180)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(Q1-G)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_1206.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 112.629 100.838 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R18"
			(at 2.7305 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "1"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-SW1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(C15-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 109.962 102.87 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R17"
			(at -2.7305 0.762 90)
			(layer "F.SilkS")
		)
		(property "Value" "1"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(U1-SW2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(C14-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 101.072 101.6 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R9"
			(at 3.2385 0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "/LT8705_SYNC")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 97.643 85.471 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R6"
			(at 0 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/LT8705_ENA")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 98.24 93.853 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R4"
			(at -2.324 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-IMON_OUT)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 101.834 85.471 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R3"
			(at 2.413 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "20K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.127 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U1-IMON_IN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 94.468 93.853 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R2"
			(at 2.794 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "16.2K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 113.899 97.155)
		(property "Reference" "D5"
			(at -3.6195 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "PMEG6010"
			(at 0.0635 1.8415 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1N5819HW-FDICT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.247 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 97.77 86.868 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C11"
			(at 5.334 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-LDO33)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 178.923 95.504)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C33"
			(at -3.683 -6.223 0)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1572-1047-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 180)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 180)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 96.246 103.886)
		(property "Reference" "TP35"
			(at -3.048 0.3175 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/LT8705_SYNC")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 94.506 98.044 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R5"
			(at 1.2445 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.6K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.038 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(C5-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 106.66 102.87 90)
		(property "Reference" "D4"
			(at -3.429 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "PMEG6010"
			(at 0.0635 1.8415 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1N5819HW-FDICT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.4445 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 110.47 69.342 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C34"
			(at 0 -2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 95.992 69.469 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C35"
			(at 3.81 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.061 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 108.565 85.283 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C36"
			(at 3.622 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.061 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 104.501 101.854 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C37"
			(at 3.6195 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 190.861 73.726 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C38"
			(at 3.617 -0.127 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 188.067 73.726 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C39"
			(at 3.363 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 93.96 69.431 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R15"
			(at 3.34 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "56K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(O1-C)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 105.39 85.471 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R16"
			(at 2.794 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U1-SWEN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(D1-A)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP50"
		(layer "F.Cu")
		(at 106.279 80.264)
		(property "Reference" "TP36"
			(at 0.127 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "TP"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP50"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.27 1.27)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(U1-SWEN)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 179.177 77.216)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C31"
			(at -4.318 -6.985 0)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1572-1047-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 180)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 180)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "t_coilcraft:SER2900"
		(layer "F.Cu")
		(at 135.5398 62.0812)
		(descr "Coilcraft Flat Wire Power Inductor")
		(property "Reference" "L1"
			(at 0.8382 -12.4242 0)
			(layer "F.SilkS")
		)
		(property "Value" "SER2918H-103"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_coilcraft:SER2900"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/a2805f49-c9b8-42c0-9939-b2d75eed7288/ser2900.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -5.1 14.4)
			(size 5.4 5.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-SW1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 5.1 14.4)
			(size 5.4 5.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(U1-SW2)")
			(pinfunction "2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -7.7)
			(size 6.35 5.28)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "unconnected-(L1-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-SER2915L.STEP"
			(offset
				(xyz 0 0 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 102.596 101.6 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R13"
			(at 3.302 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "392K"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U1-RT)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 110.597 88.392 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C10"
			(at 0 1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TCI" "22564-105"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-CSPIN)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 98.151 90.424)
		(descr "SMT resistor, 0603")
		(property "Reference" "R1"
			(at -2.159 0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-LDO33)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(U1-FBIN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 97.77 88.519)
		(descr "SMT resistor, 0603")
		(property "Reference" "R7"
			(at 2.413 0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-LDO33)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U1-MODE)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 95.357 87.63 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R8"
			(at -1.016 -1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "DNI"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.0865 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U1-MODE)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 112.883 87.757)
		(descr "SMT resistor, 0603")
		(property "Reference" "R10"
			(at 0.635 -1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0175 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/Vin_9_30")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-CSPIN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 118.306 89.662)
		(descr "SMT resistor, 0603")
		(property "Reference" "R11"
			(at 0.038 -1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(U1-CSNOUT)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 115.931 88.888 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C21"
			(at -2.02 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.0uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TCI" "22564-105"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(U1-CSNOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:MFP4_2.5x4.4"
		(layer "F.Cu")
		(at 94.722 81.534 90)
		(property "Reference" "O1"
			(at 2.413 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "FODM8801"
			(at 0 -0.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:MFP4_2.5x4.4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.fairchildsemi.com/datasheets/FO/FODM8801A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.635 -3.175 90)
			(size 0.61 1.524)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(O1-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.635 -3.175 90)
			(size 0.61 1.524)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "K")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -0.635 3.175 90)
			(size 0.61 1.524)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "/LT8705_ENA")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.635 3.175 90)
			(size 0.61 1.524)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(O1-C)")
			(pinfunction "C")
			(pintype "input")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 189.21 88.9)
		(property "Reference" "TP23"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 189.21 66.04)
		(property "Reference" "TP26"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/Vout_28")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 82.53 102.87)
		(property "Reference" "TP13"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 189.21 102.87)
		(property "Reference" "TP14"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 189.21 52.07)
		(property "Reference" "TP15"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 82.53 52.07)
		(property "Reference" "TP16"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 82.53 74.93)
		(property "Reference" "TP19"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/Vin_9_30")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_375x144"
		(locked yes)
		(layer "F.Cu")
		(at 82.53 90.17)
		(property "Reference" "TP20"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_MtgHoles:MTG_375x144"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 9.525 9.525)
			(drill 3.6576)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_smd_caps:CP_Elec_10x10"
		(layer "F.Cu")
		(at 178.796 56.769 90)
		(descr "SMT capacitor, aluminium electrolytic, 10x10")
		(property "Reference" "C32"
			(at 6.477 -4.191 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -6.4643 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_smd_caps:CP_Elec_10x10"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1572-1047-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP* SM*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.7785 4.9657 90)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -2.9083 -0.0762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/Vout_28")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_caps/CP_Elec_10x10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 81.641 64.516 180)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at -0.127 4.445 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x1"
			(at 4.385 4.81 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J1-Pad1)")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "power_out")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 121.265 99.822 90)
		(property "Reference" "D1"
			(at -3.683 0.127 270)
			(layer "F.SilkS")
		)
		(property "Value" "1n4148"
			(at 0.0635 1.8415 270)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.4445 0.0635 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 119.233 95.062 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C22"
			(at 0.320001 2.158999 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.3462 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 118.217 99.822 -90)
		(property "Reference" "D2"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1n4148"
			(at 0.0635 1.8415 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.4445 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/VCCx")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 137.394 69.239 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C25"
			(at -4.088 -0.127 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.02 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 119.691 85.763 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C23"
			(at 2.667 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1000pF"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "/CSP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "/CSN")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 125.94 62.23)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C20"
			(at -0.23 -2.794 360)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 360)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.02 360)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 121.469 85.763 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R24"
			(at -2.667 -0.0635 90)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "/CSN")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "/CSP")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 124.059 84.963)
		(descr "SMT resistor, 0603")
		(property "Reference" "R25"
			(at 0 -1.524 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 54 "Net-(R25-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "/CSP")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:WSL3637_VIS"
		(layer "B.Cu")
		(at 133.076 86.233 -90)
		(tags "WSL36373L000FEA ")
		(property "Reference" "R30"
			(at -0.381 -6.985 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.003 Ohms"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:WSL3637_VIS"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "WSL36373L000FEA"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -3.7338 -1.2446 270)
			(size 2.9464 7.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 29 "Net-(Q2-S-Pad2)")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -3.7338 4.2164 270)
			(size 2.9464 1.6764)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 54 "Net-(R25-Pad1)")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 3.7338 4.2164 270)
			(size 2.9464 1.6764)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 55 "Net-(R26-Pad1)")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 3.7338 -1.2446 270)
			(size 2.9464 7.62)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 130.5778 84.4732) (xy 130.5778 88.0928) (xy 137.7242 88.0928) (xy 137.7242 84.4732)
				)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 125.94 65.278 180)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C19"
			(at 3.151 0.254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 180)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.107 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 134.1428 69.215 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C16"
			(at 4.064 0.2032 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.02 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 131.1202 69.191 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C17"
			(at -4.04 -0.0508 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.127 -0.107 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 128.0976 69.191 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C18"
			(at -0.024 -2.7686 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.107 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(U1-CSNIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 140.442 69.239 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C26"
			(at -4.215 0.02 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.02 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 143.49 69.239 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C27"
			(at -0.23 3.175 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.147 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_ECP_eGaN:EPC2088"
		(layer "B.Cu")
		(at 142.012 74.549 180)
		(property "Reference" "Q3"
			(at -3.002 1.397 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EPC2088"
			(at 0.3 -0.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_ECP_eGaN:EPC2088"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2088_datasheet.pdf"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100V eGaN 2.5mOhms"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "REF**"
			(at -1.45 -0.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.5 180)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "input")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -1.5 -0.5 180)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -1 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U1-CSPOUT)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -0.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U1-CSPOUT)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 1 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U1-CSPOUT)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 1.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
	)
	(footprint "t_ECP_eGaN:EPC2088"
		(layer "B.Cu")
		(at 128.982 74.684)
		(property "Reference" "Q1"
			(at -3.018 -1.659 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EPC2088"
			(at 0.3 -0.2 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_ECP_eGaN:EPC2088"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2088_datasheet.pdf"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100V eGaN 2.5mOhms"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at -1.45 -0.5 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.5)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -1.5 -0.5)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -1 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-CSNIN)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -0.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-CSNIN)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 1 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-CSNIN)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 1.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 145.927 62.23 180)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C29"
			(at -0.738 2.286 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 180)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.107 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "B.Cu")
		(at 145.927 65.405)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C28"
			(at 3.278 -0.127 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -2.5 360)
			(layer "B.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfgr" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mfgr PN" "GRM31CR71H475KA12L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "490-6521-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Voltage" "50V"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.02 360)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 2.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(U1-CSPOUT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 124.059 86.487)
		(descr "SMT resistor, 0603")
		(property "Reference" "R26"
			(at -0.0635 1.5875 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.127 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 55 "Net-(R26-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "/CSN")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_logos:Thales_15x2_Cu"
		(locked yes)
		(layer "B.Cu")
		(at 148.697 100.965 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
	)
	(footprint "t_ECP_eGaN:EPC2088"
		(layer "B.Cu")
		(at 128.942 78.232)
		(property "Reference" "Q2"
			(at -2.851 2.159 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EPC2088"
			(at 0.3 -0.2 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_ECP_eGaN:EPC2088"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2088_datasheet.pdf"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100V eGaN 2.5mOhms"
			(at 0.25 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at -1.45 -0.5 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.5)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "input")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -1.5 -0.5)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -1 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -0.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 1 0)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-SW1)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 1.5 0)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
	)
	(footprint "t_ECP_eGaN:EPC2088"
		(layer "B.Cu")
		(at 142.123 78.224 180)
		(property "Reference" "Q4"
			(at -2.891 -1.532 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "EPC2088"
			(at 0.3 -0.2 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_ECP_eGaN:EPC2088"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://epc-co.com/epc/Portals/0/epc/documents/datasheets/EPC2088_datasheet.pdf"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "100V eGaN 2.5mOhms"
			(at 0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "BC_BuckBoost_eGaN.kicad_sch")
		(attr smd)
		(fp_text user "REF**"
			(at -1.45 -0.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.5 180)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(Q4-G)")
			(pinfunction "G")
			(pintype "input")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -1.5 -0.5 180)
			(size 0.25 0.775)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -1 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -0.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 1 0 180)
			(size 0.25 1.625)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-SW2)")
			(pinfunction "D")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 1.5 0 180)
			(size 0.25 1.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q2-S-Pad2)")
			(pinfunction "S")
			(pintype "passive")
			(solder_mask_margin 0.02)
			(thermal_bridge_angle 45)
		)
	)
	(gr_line
		(start 194.544 108.204)
		(end 77.196 108.204)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194.544 46.736)
		(end 194.544 108.204)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.196 46.736)
		(end 194.544 46.736)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.196 108.204)
		(end 77.196 46.736)
		(layer "Edge.Cuts")
	)
	(gr_text "Buck Boost Charger eGaN\n21 March 2024"
		(at 148.443 104.902 0)
		(layer "B.Cu")
	)
	(gr_text "GND"
		(at 87.991 94.869 0)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 81.768 67.31 0)
		(layer "F.SilkS")
	)
	(gr_text "+Vout"
		(at 188.829 59.563 0)
		(layer "F.SilkS")
	)
	(gr_text "GND\n"
		(at 189.21 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "3300497-1\n"
		(at 172.954 105.537 0)
		(layer "F.SilkS")
	)
	(gr_text "+Vin"
		(at 87.229 80.137 0)
		(layer "F.SilkS")
	)
	(gr_text "3101510-501 Rev 2"
		(at 140.823 105.41 0)
		(layer "F.SilkS")
	)
	(gr_text "+Vin"
		(at 73.025 80.01 0)
		(layer "F.Fab")
	)
	(gr_text "-On/Off"
		(at 71.12 69.85 0)
		(layer "F.Fab")
	)
	(gr_text "+On/Off"
		(at 71.12 66.04 0)
		(layer "F.Fab")
	)
	(gr_text "+Vout"
		(at 200.66 66.04 0)
		(layer "F.Fab")
	)
	(gr_text "-Vout"
		(at 200.025 92.075 0)
		(layer "F.Fab")
	)
	(gr_text "+Sense"
		(at 181.61 113.665 90)
		(layer "F.Fab")
	)
	(gr_text "-Sense"
		(at 177.8 113.665 90)
		(layer "F.Fab")
	)
	(gr_text "Trim"
		(at 173.99 111.125 90)
		(layer "F.Fab")
	)
	(gr_text "Parallel\n"
		(at 169.545 113.665 90)
		(layer "F.Fab")
	)
	(gr_text "DC_OK"
		(at 166.37 113.03 90)
		(layer "F.Fab")
	)
	(gr_text "Aux"
		(at 162.56 111.125 90)
		(layer "F.Fab")
	)
	(gr_text "-Vin"
		(at 72.39 89.535 0)
		(layer "F.Fab")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 77.45 46.99) (xy 77.45 107.95)
		)
		(height 6.35)
		(gr_text "2.4000 in"
			(at 69.95 77.47 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 194.29 107.95) (xy 77.45 107.95)
		)
		(height -5.08)
		(gr_text "4.6000 in"
			(at 135.87 111.88 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.655 107.315) (xy 78.085 107.315) (xy 78.085 47.625) (xy 193.655 47.625)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Vout_28")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.528 62.992) (xy 193.528 72.136) (xy 191.75 73.406) (xy 186.797 73.406) (xy 185.527 72.136)
				(xy 182.987 72.136) (xy 179.558 72.136) (xy 178.669 73.025) (xy 178.669 96.393) (xy 177.78 97.282)
				(xy 169.525 97.282) (xy 168.763 96.647) (xy 168.763 68.199) (xy 166.477 66.294) (xy 159.238 66.294)
				(xy 157.968 65.024) (xy 157.968 58.166) (xy 159.111 57.023) (xy 185.527 57.023)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/Vin_9_30")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 113.772 58.42) (xy 113.772 68.072) (xy 112.502 69.342) (xy 92.817 69.469) (xy 92.436 69.85)
				(xy 92.436 72.136) (xy 84.689 79.883) (xy 80.244 79.883) (xy 77.831 77.724) (xy 77.831 71.882) (xy 80.498 69.85)
				(xy 83.165 69.85) (xy 85.197 67.818) (xy 85.324 60.452) (xy 86.086 59.69) (xy 94.341 59.69) (xy 96.373436 57.616529)
				(xy 113.137 57.531)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(U1-SW2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.013 73.66) (xy 139.299 73.66) (xy 139.299 79.375) (xy 137.013 79.375)
			)
		)
	)
	(zone
		(net 21)
		(net_name "Net-(U1-SW1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.933 73.66) (xy 134.219 73.66) (xy 134.219 79.375) (xy 131.933 79.375)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(U1-CSNIN)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.3048)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.566 60.325) (xy 122.281 60.323211) (xy 122.662 60.706) (xy 122.662 68.961) (xy 122.027 69.596)
				(xy 117.074 69.596) (xy 116.566 68.961)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(U1-CSPOUT)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.92 60.071) (xy 149.078 60.071) (xy 148.57 60.579) (xy 148.57 69.596) (xy 149.078 70.231)
				(xy 154.412 70.231) (xy 154.92 69.723)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.655 107.315) (xy 78.085 107.315) (xy 78.085 47.625) (xy 193.655 47.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 193.528 63.119) (xy 194.29 64.77) (xy 194.29 67.056) (xy 193.655 68.961) (xy 191.877 70.612)
				(xy 189.337 71.374) (xy 187.051 70.866) (xy 185.527 69.723) (xy 184.511 68.326) (xy 184.003 66.675)
				(xy 184.13 64.897) (xy 184.638 63.5) (xy 185.654 62.23) (xy 186.924 61.341) (xy 189.337 60.833)
				(xy 191.242 61.214) (xy 192.639 62.103)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 86.848 71.882) (xy 87.61 73.533) (xy 87.61 75.819) (xy 86.975 77.724) (xy 85.197 79.375) (xy 82.657 80.137)
				(xy 80.371 79.629) (xy 78.847 78.486) (xy 77.831 77.089) (xy 77.323 75.438) (xy 77.45 73.66) (xy 77.958 72.263)
				(xy 78.974 70.993) (xy 80.244 70.104) (xy 82.657 69.596) (xy 84.562 69.977) (xy 85.959 70.866)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.655 107.315) (xy 78.085 107.315) (xy 78.085 47.625) (xy 193.655 47.625)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.655 107.315) (xy 78.085 107.315) (xy 78.085 47.625) (xy 193.655 47.625)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/Vin_9_30")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads yes
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 110.978 58.293) (xy 110.978 65.786) (xy 109.835 66.929) (xy 95.611 66.929) (xy 92.817 69.723)
				(xy 92.817 71.755) (xy 84.689 79.883) (xy 80.244 79.883) (xy 77.831 77.724) (xy 77.831 71.882) (xy 80.498 69.85)
				(xy 83.165 69.85) (xy 85.07 67.945) (xy 85.07 60.706) (xy 86.086 59.69) (xy 94.214 59.69) (xy 96.119 57.658)
				(xy 110.343 57.658)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Vout_28")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing chamfer)
		)
		(polygon
			(pts
				(xy 193.528 62.992) (xy 193.528 68.072) (xy 190.861 70.231) (xy 186.289 70.231) (xy 183.241 67.183)
				(xy 162.921 67.183) (xy 161.27 65.659) (xy 161.27 58.547) (xy 162.921 56.896) (xy 185.527 56.896)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(U1-CSNIN)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.693 60.452) (xy 124.44 60.452) (xy 125.04 60.98) (xy 125.075 68.834) (xy 125.837 69.723)
				(xy 135.489 69.723) (xy 135.489 72.009) (xy 133.952786 71.996897) (xy 131.298 74.676) (xy 127.742 74.676)
				(xy 127.742 73.533) (xy 127.488 73.279) (xy 122.281 73.279) (xy 119.233 69.977) (xy 117.074 69.977)
				(xy 116.693 69.596)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.029 84.3788) (xy 138.029 88.392) (xy 127.9198 88.392) (xy 127.9198 84.3788)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(Q2-S-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.615 77.089) (xy 127.567 78.3445) (xy 131.298 78.359) (xy 132.187 79.248) (xy 138.918 79.248)
				(xy 139.934 78.232) (xy 143.871 78.232) (xy 143.871 79.883) (xy 139.553 82.931) (xy 129.393 82.931)
				(xy 126.472 80.391) (xy 125.71 79.629) (xy 125.71 77.343) (xy 125.964 77.089)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(U1-CSPOUT)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.997 72.009) (xy 137.521 72.009) (xy 139.934 74.549) (xy 143.744 74.549) (xy 146.03 74.549)
				(xy 146.03 74.549) (xy 146.411 74.549) (xy 151.364 70.104) (xy 154.539 70.104) (xy 155.047 69.596)
				(xy 155.047 60.198) (xy 147.554 60.198) (xy 146.284 61.468) (xy 146.284 68.834) (xy 145.395 69.723)
				(xy 135.997 69.723)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-(U1-SW2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.744 77.089) (xy 143.498 77.3365) (xy 143.498 77.978) (xy 143.498 77.9845) (xy 139.807 77.978)
				(xy 138.664 79.121) (xy 137.902 79.121) (xy 137.648 78.867) (xy 137.648 73.914) (xy 137.902 73.66)
				(xy 138.791 73.66) (xy 139.807 74.676) (xy 143.363 74.676) (xy 143.387 74.6615) (xy 143.49 74.676)
				(xy 145.141 74.676) (xy 145.395 74.93) (xy 145.395 76.835) (xy 145.141 77.089)
			)
		)
	)
	(zone
		(net 21)
		(net_name "Net-(U1-SW1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.2032)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.607 73.533) (xy 127.607 74.7965) (xy 131.298 74.803) (xy 132.441 73.66) (xy 133.203 73.66)
				(xy 133.457 73.914) (xy 133.457 78.867) (xy 133.203 79.121) (xy 132.314 79.121) (xy 131.298 78.105)
				(xy 127.742 78.105) (xy 127.742 76.835) (xy 127.615 76.708) (xy 125.964 76.708) (xy 125.71 76.454)
				(xy 125.71 73.787) (xy 125.964 73.533)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 156.339158 102.235) (xy 140.527658 102.235) (xy 140.527658 99.5045) (xy 156.339158 99.5045)
			)
		)
	)
)