(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 61)
    (no_connects 1)
    (area 110.589287 99.281 165.912801 142.653932)
    (thickness 1.6002)
    (drawings 8)
    (tracks 303)
    (zones 0)
    (modules 21)
    (nets 41)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.25 1.25)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad10)")
  (net 2 "Net-(U1-Pad9)")
  (net 3 "Net-(U1-Pad5)")
  (net 4 "Net-(U1-Pad7)")
  (net 5 "Net-(IC1-Pad2)")
  (net 6 GND)
  (net 7 "Net-(IC1-Pad26)")
  (net 8 "Net-(IC1-Pad28)")
  (net 9 /MISO)
  (net 10 /SCK)
  (net 11 /MOSI)
  (net 12 VCC)
  (net 13 "Net-(IC1-Pad19)")
  (net 14 "Net-(IC1-Pad7)")
  (net 15 "Net-(IC1-Pad8)")
  (net 16 "Net-(IC1-Pad22)")
  (net 17 /~RST)
  (net 18 "Net-(P2-Pad2)")
  (net 19 "Net-(P2-Pad3)")
  (net 20 "Net-(P2-Pad4)")
  (net 21 "Net-(P2-Pad6)")
  (net 22 "Net-(IC1-Pad32)")
  (net 23 /5V)
  (net 24 /RFDAT)
  (net 25 /CEnRF)
  (net 26 /~CSNnRF)
  (net 27 /SCKnRF)
  (net 28 /MOSInRF)
  (net 29 /MISOnRF)
  (net 30 /IRQnRF)
  (net 31 "Net-(D1-Pad2)")
  (net 32 "Net-(D2-Pad2)")
  (net 33 /IRin)
  (net 34 /int1)
  (net 35 /int0)
  (net 36 "Net-(IC1-Pad20)")
  (net 37 "Net-(R4-Pad1)")
  (net 38 /ADCin)
  (net 39 /espTX)
  (net 40 /expRX)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /ADCin)
    (add_net /CEnRF)
    (add_net /IRQnRF)
    (add_net /IRin)
    (add_net /MISO)
    (add_net /MISOnRF)
    (add_net /MOSI)
    (add_net /MOSInRF)
    (add_net /RFDAT)
    (add_net /SCK)
    (add_net /SCKnRF)
    (add_net /espTX)
    (add_net /expRX)
    (add_net /int0)
    (add_net /int1)
    (add_net /~CSNnRF)
    (add_net /~RST)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 1)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /5V)
    (add_net GND)
    (add_net VCC)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 58E114F5)
    (at 140.843 120.269)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at -0.635 -1.778) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module "spider:USB_Micro-B handsoldering" (layer F.Cu) (tedit 58E145E4)
    (at 124.587 108.331 180)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P2 (at 0.127 1.19 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 5.01 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.65 270) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 /5V))
    (pad 2 smd rect (at -0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste)
      (net 18 "Net-(P2-Pad2)"))
    (pad 3 smd rect (at 0 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.35 270) (size 1.35 0.4) (layers F.Cu F.Paste)
      (net 20 "Net-(P2-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.65 270) (size 2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35 270) (size 1.25 1.25) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad6)"))
    (pad 6 thru_hole circle (at 2.5 -1.35 270) (size 1.25 1.25) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad6)"))
    (pad 7 thru_hole circle (at -3.5 1.35 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.5 1.35 180) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 137.922 107.315)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 3.683) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 1.27 12.49) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /~RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /ADCin))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /5V))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /expRX))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /espTX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.3 (layer F.Cu) (tedit 57FA43A5)
    (at 126.365 118.11)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.3")
    (attr smd)
    (fp_text reference C2 (at 0 -1.397) (layer F.SilkS))
    (fp_text value CP (at 0 -3.5433) (layer F.Fab))
    (fp_text user + (at -1.2065 -0.0762) (layer F.Fab))
    (fp_text user + (at -3.81 -0.254) (layer F.SilkS))
    (pad 1 smd rect (at -1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /5V))
    (pad 2 smd rect (at 1.8 0 180) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module spider:ESP8266-ESP-03 (layer B.Cu) (tedit 54BF7D41)
    (at 128.905 121.285 270)
    (descr "ESP8266 ESP-03 wifi module -- Phillip Pearson")
    (fp_text reference U1 (at 0.635 0.635 540) (layer B.SilkS))
    (fp_text value ESP8266-ESP-03 (at 3.048 1.27 540) (layer B.SilkS))
    (pad 14 smd rect (at -6.1 -5.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 17 /~RST))
    (pad 13 smd rect (at -6.1 -3.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 34 /int1))
    (pad 12 smd rect (at -6.1 -1.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 11 smd rect (at -6.1 0.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 35 /int0))
    (pad 10 smd rect (at -6.1 2.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at -6.1 4.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -6.1 6.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 12 VCC))
    (pad 1 smd rect (at 6.1 -5.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 6.1 -3.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 6.1 -1.9 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 39 /espTX))
    (pad 4 smd rect (at 6.1 0.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 40 /expRX))
    (pad 5 smd rect (at 6.1 2.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 6.1 4.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 12 VCC))
    (pad 7 smd rect (at 6.1 6.1 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(U1-Pad7)"))
  )
  (module spider:RF_Transmitter_433_MHz (layer F.Cu) (tedit 58DDA5EF)
    (at 124.206 133.477 180)
    (fp_text reference RF2 (at -4.826 1.143 180) (layer F.SilkS))
    (fp_text value "433 MHz" (at 0.254 2.032 180) (layer B.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /RFDAT))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /5V))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Housings_SOT:SOT-223-3Lead_TabPin2 (layer F.Cu) (tedit 58E1400C)
    (at 132.334 110.109 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at -0.127 -0.254 180) (layer F.SilkS))
    (fp_text value LD1117S33TR (at 0 4.5 90) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 130.81 126.365 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (attr smd)
    (fp_text reference IC1 (at 0.508 0.127 180) (layer F.SilkS))
    (fp_text value ATMEGA88-A (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.635 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /RFDAT))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /MISOnRF))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /IRQnRF))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /SCKnRF))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /MOSInRF))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /CEnRF))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /~CSNnRF))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /int1))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /int0))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /IRin))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /ADCin))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /~RST))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /espTX))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /expRX))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module spider:NRF24L01_MODULE (layer F.Cu) (tedit 58AA0E77)
    (at 139.573 126.492 270)
    (descr "Footprint for Chinese nRF24L01+ module")
    (tags CONN)
    (fp_text reference U2 (at 0.127 -0.127 270) (layer F.SilkS))
    (fp_text value nRF24L01+ (at -1.016 2.794 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole circle (at -3.81 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 VCC))
    (pad 3 thru_hole circle (at -1.27 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /CEnRF))
    (pad 4 thru_hole circle (at -1.27 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /~CSNnRF))
    (pad 5 thru_hole circle (at 1.27 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /SCKnRF))
    (pad 6 thru_hole circle (at 1.27 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /MOSInRF))
    (pad 7 thru_hole circle (at 3.81 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /MISOnRF))
    (pad 8 thru_hole circle (at 3.81 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /IRQnRF))
    (model pin_array/pins_array_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 131.826 133.62 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.127 -1.778 180) (layer F.SilkS))
    (fp_text value 100nF (at 4.445 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.3 (layer F.Cu) (tedit 57FA43A5)
    (at 133.35 118.11 180)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.3")
    (attr smd)
    (fp_text reference C3 (at 0.127 1.524 180) (layer F.SilkS))
    (fp_text value CP (at 0.3175 1.27 180) (layer F.Fab))
    (fp_text user + (at -1.2065 -0.0762 180) (layer F.Fab))
    (fp_text user + (at -2.7686 2.0066 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 2 smd rect (at 1.8 0) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 135.255 134.3025)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 139.747 134.3025 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.682 1.524 180) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad7)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 124.079 123.825 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.429 0.127 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /~RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 124.206 129.286 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 3.556 1.778 180) (layer F.SilkS))
    (fp_text value IRLED (at 1.27 3.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 121.412 123.825 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.429 -0.127 270) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad26)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.00mm (layer F.Cu) (tedit 5862ED55)
    (at 135.509 130.937)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (fp_text reference P3 (at 1.778 1.397) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.12) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(IC1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 121.031 117.348 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.381 -1.651 270) (layer F.SilkS))
    (fp_text value 220uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E111B2)
    (at 130.429 113.03 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.302 -0.127 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TSOP2438:TSOP2438_long (layer F.Cu) (tedit 58E13E30)
    (at 124.46 113.03 180)
    (fp_text reference U4 (at 1.524 -2.032 180) (layer F.SilkS))
    (fp_text value HS0038 (at 0.254 1.524 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /IRin))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 VCC))
    (model userlibs/libraries/packages3d/TSOP2438_long.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module spider:oshardware (layer B.Cu) (tedit 58E128C1)
    (at 132.969 109.22 180)
    (fp_text reference "© 2017 CC BY-SA" (at -3.302 -23.495 180) (layer B.SilkS))
    (fp_text value "Danny Havenith" (at -3.302 -25.019 180) (layer B.SilkS))
  )
  (gr_line (start 142.367 105.664) (end 120.015 105.664) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.367 135.509) (end 142.367 105.664) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.015 135.509) (end 142.367 135.509) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.015 105.664) (end 120.015 135.509) (layer Edge.Cuts) (width 0.15))
  (dimension 6.097323 (width 0.3) (layer B.Fab)
    (gr_text "6.097 mm" (at 131.239852 138.688581 358.8065106) (layer B.Fab))
    (feature1 (pts (xy 134.366 135.001) (xy 134.259733 140.101788)))
    (feature2 (pts (xy 128.27 134.874) (xy 128.163733 139.974788)))
    (crossbar (pts (xy 128.219971 137.275374) (xy 134.315971 137.402374)))
    (arrow1a (pts (xy 134.315971 137.402374) (xy 133.177497 137.965204)))
    (arrow1b (pts (xy 134.315971 137.402374) (xy 133.201926 136.792617)))
    (arrow2a (pts (xy 128.219971 137.275374) (xy 129.334016 137.885131)))
    (arrow2b (pts (xy 128.219971 137.275374) (xy 129.358445 136.712544)))
  )
  (dimension 7.112 (width 0.3) (layer B.Fab)
    (gr_text "7.112 mm" (at 132.588 100.631) (layer B.Fab))
    (feature1 (pts (xy 136.144 104.14) (xy 136.144 99.281)))
    (feature2 (pts (xy 129.032 104.14) (xy 129.032 99.281)))
    (crossbar (pts (xy 129.032 101.981) (xy 136.144 101.981)))
    (arrow1a (pts (xy 136.144 101.981) (xy 135.017496 102.567421)))
    (arrow1b (pts (xy 136.144 101.981) (xy 135.017496 101.394579)))
    (arrow2a (pts (xy 129.032 101.981) (xy 130.158504 102.567421)))
    (arrow2b (pts (xy 129.032 101.981) (xy 130.158504 101.394579)))
  )
  (dimension 30.226 (width 0.3) (layer B.Fab)
    (gr_text "1.1900 in" (at 116.125 120.523 90) (layer B.Fab))
    (feature1 (pts (xy 121.92 105.41) (xy 114.775 105.41)))
    (feature2 (pts (xy 121.92 135.636) (xy 114.775 135.636)))
    (crossbar (pts (xy 117.475 135.636) (xy 117.475 105.41)))
    (arrow1a (pts (xy 117.475 105.41) (xy 118.061421 106.536504)))
    (arrow1b (pts (xy 117.475 105.41) (xy 116.888579 106.536504)))
    (arrow2a (pts (xy 117.475 135.636) (xy 118.061421 134.509496)))
    (arrow2b (pts (xy 117.475 135.636) (xy 116.888579 134.509496)))
  )
  (dimension 20.574 (width 0.3) (layer B.Fab)
    (gr_text "0.8100 in" (at 132.207 141.303931) (layer B.Fab))
    (feature1 (pts (xy 142.494 136.398) (xy 142.494 142.653931)))
    (feature2 (pts (xy 121.92 136.398) (xy 121.92 142.653931)))
    (crossbar (pts (xy 121.92 139.953931) (xy 142.494 139.953931)))
    (arrow1a (pts (xy 142.494 139.953931) (xy 141.367496 140.540352)))
    (arrow1b (pts (xy 142.494 139.953931) (xy 141.367496 139.36751)))
    (arrow2a (pts (xy 121.92 139.953931) (xy 123.046504 140.540352)))
    (arrow2b (pts (xy 121.92 139.953931) (xy 123.046504 139.36751)))
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.015 105.664) (xy 142.367 105.664) (xy 142.367 135.509) (xy 120.015 135.509)
      )
    )
  )
  (zone (net 12) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.015 105.664) (xy 142.367 105.664) (xy 142.367 135.382) (xy 120.015 135.382)
      )
    )
  )
)
