(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 64)
    (no_connects 0)
    (area 58.41619 90.367142 160.02381 109.695001)
    (thickness 1.6)
    (drawings 49)
    (tracks 163)
    (zones 0)
    (modules 5)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.05)
    (edge_width 0.05)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad64)")
  (net 2 "Net-(P1-Pad62)")
  (net 3 "Net-(P1-Pad60)")
  (net 4 "Net-(P1-Pad58)")
  (net 5 "Net-(P1-Pad56)")
  (net 6 "Net-(P1-Pad54)")
  (net 7 "Net-(P1-Pad52)")
  (net 8 "Net-(P1-Pad50)")
  (net 9 "Net-(P1-Pad48)")
  (net 10 "Net-(P1-Pad46)")
  (net 11 "Net-(P1-Pad44)")
  (net 12 "Net-(P1-Pad42)")
  (net 13 "Net-(P1-Pad40)")
  (net 14 "Net-(P1-Pad38)")
  (net 15 "Net-(P1-Pad36)")
  (net 16 "Net-(P1-Pad34)")
  (net 17 "Net-(P1-Pad32)")
  (net 18 "Net-(P1-Pad30)")
  (net 19 "Net-(P1-Pad28)")
  (net 20 "Net-(P1-Pad26)")
  (net 21 "Net-(P1-Pad63)")
  (net 22 "Net-(P1-Pad61)")
  (net 23 "Net-(P1-Pad59)")
  (net 24 "Net-(P1-Pad57)")
  (net 25 "Net-(P1-Pad55)")
  (net 26 "Net-(P1-Pad53)")
  (net 27 "Net-(P1-Pad51)")
  (net 28 "Net-(P1-Pad49)")
  (net 29 "Net-(P1-Pad47)")
  (net 30 "Net-(P1-Pad45)")
  (net 31 "Net-(P1-Pad43)")
  (net 32 "Net-(P1-Pad41)")
  (net 33 "Net-(P1-Pad39)")
  (net 34 "Net-(P1-Pad37)")
  (net 35 "Net-(P1-Pad24)")
  (net 36 "Net-(P1-Pad22)")
  (net 37 "Net-(P1-Pad20)")
  (net 38 "Net-(P1-Pad18)")
  (net 39 "Net-(P1-Pad16)")
  (net 40 "Net-(P1-Pad14)")
  (net 41 "Net-(P1-Pad12)")
  (net 42 "Net-(P1-Pad10)")
  (net 43 "Net-(P1-Pad8)")
  (net 44 "Net-(P1-Pad6)")
  (net 45 "Net-(P1-Pad4)")
  (net 46 "Net-(P1-Pad2)")
  (net 47 "Net-(P1-Pad35)")
  (net 48 "Net-(P1-Pad33)")
  (net 49 "Net-(P1-Pad31)")
  (net 50 "Net-(P1-Pad29)")
  (net 51 "Net-(P1-Pad27)")
  (net 52 "Net-(P1-Pad25)")
  (net 53 "Net-(P1-Pad23)")
  (net 54 "Net-(P1-Pad21)")
  (net 55 "Net-(P1-Pad19)")
  (net 56 "Net-(P1-Pad17)")
  (net 57 "Net-(P1-Pad15)")
  (net 58 "Net-(P1-Pad13)")
  (net 59 "Net-(P1-Pad11)")
  (net 60 "Net-(P1-Pad9)")
  (net 61 "Net-(P1-Pad7)")
  (net 62 "Net-(P1-Pad5)")
  (net 63 "Net-(P1-Pad3)")
  (net 64 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad25)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad35)")
    (add_net "Net-(P1-Pad37)")
    (add_net "Net-(P1-Pad39)")
    (add_net "Net-(P1-Pad41)")
    (add_net "Net-(P1-Pad43)")
    (add_net "Net-(P1-Pad45)")
    (add_net "Net-(P1-Pad47)")
    (add_net "Net-(P1-Pad49)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad51)")
    (add_net "Net-(P1-Pad53)")
    (add_net "Net-(P1-Pad55)")
    (add_net "Net-(P1-Pad57)")
    (add_net "Net-(P1-Pad59)")
    (add_net "Net-(P1-Pad61)")
    (add_net "Net-(P1-Pad63)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad9)")
  )
  (net_class pwr ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad20)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad30)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(P1-Pad34)")
    (add_net "Net-(P1-Pad36)")
    (add_net "Net-(P1-Pad38)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad40)")
    (add_net "Net-(P1-Pad42)")
    (add_net "Net-(P1-Pad44)")
    (add_net "Net-(P1-Pad46)")
    (add_net "Net-(P1-Pad48)")
    (add_net "Net-(P1-Pad50)")
    (add_net "Net-(P1-Pad52)")
    (add_net "Net-(P1-Pad54)")
    (add_net "Net-(P1-Pad56)")
    (add_net "Net-(P1-Pad58)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad60)")
    (add_net "Net-(P1-Pad62)")
    (add_net "Net-(P1-Pad64)")
    (add_net "Net-(P1-Pad8)")
  )
  (module sds7lib:sds7edge_connector (layer F.Cu) (tedit 5A99645E)
    (at 148.59 105.41)
    (descr "Simmons SDS7 EDGE 2x32")
    (tags "Simmons simmons SDS7 sds7 EDGE edge CONN connector sds snw 41 stillnotworking")
    (autoplace_cost90 10)
    (fp_text reference P1 (at -60.96 -6.99) (layer F.SilkS) hide)
    (fp_text value "SIMMONS SDS7" (at -68.29 -4.71) (layer F.SilkS))
    (fp_text user 20 (at -30.4292 -4.7498 90) (layer B.SilkS))
    (fp_text user 20 (at -30.4292 -4.7498 90) (layer F.SilkS))
    (fp_text user 10 (at -55.8546 -4.7498 90) (layer B.SilkS))
    (fp_text user 10 (at -55.8546 -4.7752 90) (layer F.SilkS))
    (fp_text user VC (at -34.29 -4.6736) (layer B.SilkS))
    (fp_text user CPU (at -14.0462 -4.6736) (layer F.SilkS))
    (fp_text user VC (at -34.29 -4.6736) (layer F.SilkS))
    (pad 64 connect rect (at 0 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 1 "Net-(P1-Pad64)"))
    (pad 62 connect rect (at -2.54 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 2 "Net-(P1-Pad62)"))
    (pad 60 connect rect (at -5.08 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 3 "Net-(P1-Pad60)"))
    (pad 58 connect rect (at -7.62 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 4 "Net-(P1-Pad58)"))
    (pad 56 connect rect (at -10.16 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 5 "Net-(P1-Pad56)"))
    (pad 54 connect rect (at -12.7 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 6 "Net-(P1-Pad54)"))
    (pad 52 connect rect (at -15.24 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 7 "Net-(P1-Pad52)"))
    (pad 50 connect rect (at -17.78 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 8 "Net-(P1-Pad50)"))
    (pad 48 connect rect (at -20.32 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 9 "Net-(P1-Pad48)"))
    (pad 46 connect rect (at -22.86 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 10 "Net-(P1-Pad46)"))
    (pad 44 connect rect (at -25.4 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 11 "Net-(P1-Pad44)"))
    (pad 42 connect rect (at -27.94 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 12 "Net-(P1-Pad42)"))
    (pad 40 connect rect (at -30.48 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 13 "Net-(P1-Pad40)"))
    (pad 38 connect rect (at -33.02 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 14 "Net-(P1-Pad38)"))
    (pad 36 connect rect (at -35.56 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 15 "Net-(P1-Pad36)"))
    (pad 34 connect rect (at -38.1 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 16 "Net-(P1-Pad34)"))
    (pad 32 connect rect (at -40.64 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 17 "Net-(P1-Pad32)"))
    (pad 30 connect rect (at -43.18 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 18 "Net-(P1-Pad30)"))
    (pad 28 connect rect (at -45.72 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 19 "Net-(P1-Pad28)"))
    (pad 26 connect rect (at -48.26 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 20 "Net-(P1-Pad26)"))
    (pad 63 connect rect (at 0 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 21 "Net-(P1-Pad63)"))
    (pad 61 connect rect (at -2.54 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 22 "Net-(P1-Pad61)"))
    (pad 59 connect rect (at -5.08 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 23 "Net-(P1-Pad59)"))
    (pad 57 connect rect (at -7.62 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 24 "Net-(P1-Pad57)"))
    (pad 55 connect rect (at -10.16 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 25 "Net-(P1-Pad55)"))
    (pad 53 connect rect (at -12.7 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 26 "Net-(P1-Pad53)"))
    (pad 51 connect rect (at -15.24 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 27 "Net-(P1-Pad51)"))
    (pad 49 connect rect (at -17.78 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 28 "Net-(P1-Pad49)"))
    (pad 47 connect rect (at -20.32 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 29 "Net-(P1-Pad47)"))
    (pad 45 connect rect (at -22.86 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 30 "Net-(P1-Pad45)"))
    (pad 43 connect rect (at -25.4 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 31 "Net-(P1-Pad43)"))
    (pad 41 connect rect (at -27.94 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 32 "Net-(P1-Pad41)"))
    (pad 39 connect rect (at -30.48 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 33 "Net-(P1-Pad39)"))
    (pad 37 connect rect (at -33.02 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 34 "Net-(P1-Pad37)"))
    (pad 24 connect rect (at -50.8 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 35 "Net-(P1-Pad24)"))
    (pad 22 connect rect (at -53.34 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 36 "Net-(P1-Pad22)"))
    (pad 20 connect rect (at -55.88 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 37 "Net-(P1-Pad20)"))
    (pad 18 connect rect (at -58.42 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 38 "Net-(P1-Pad18)"))
    (pad 16 connect rect (at -60.96 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 39 "Net-(P1-Pad16)"))
    (pad 14 connect rect (at -63.5 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 40 "Net-(P1-Pad14)"))
    (pad 12 connect rect (at -66.04 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 41 "Net-(P1-Pad12)"))
    (pad 10 connect rect (at -68.58 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 42 "Net-(P1-Pad10)"))
    (pad 8 connect rect (at -71.12 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 43 "Net-(P1-Pad8)"))
    (pad 6 connect rect (at -73.66 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 44 "Net-(P1-Pad6)"))
    (pad 4 connect rect (at -76.2 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 45 "Net-(P1-Pad4)"))
    (pad 2 connect rect (at -78.74 0) (size 1.54 7.62) (layers B.Cu B.Mask)
      (net 46 "Net-(P1-Pad2)"))
    (pad 35 connect rect (at -35.56 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 47 "Net-(P1-Pad35)"))
    (pad 33 connect rect (at -38.1 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 48 "Net-(P1-Pad33)"))
    (pad 31 connect rect (at -40.64 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 49 "Net-(P1-Pad31)"))
    (pad 29 connect rect (at -43.18 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 50 "Net-(P1-Pad29)"))
    (pad 27 connect rect (at -45.72 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 51 "Net-(P1-Pad27)"))
    (pad 25 connect rect (at -48.26 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 52 "Net-(P1-Pad25)"))
    (pad 23 connect rect (at -50.8 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 53 "Net-(P1-Pad23)"))
    (pad 21 connect rect (at -53.34 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 54 "Net-(P1-Pad21)"))
    (pad 19 connect rect (at -55.88 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 55 "Net-(P1-Pad19)"))
    (pad 17 connect rect (at -58.42 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 56 "Net-(P1-Pad17)"))
    (pad 15 connect rect (at -60.96 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 57 "Net-(P1-Pad15)"))
    (pad 13 connect rect (at -63.5 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 58 "Net-(P1-Pad13)"))
    (pad 11 connect rect (at -66.04 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 59 "Net-(P1-Pad11)"))
    (pad 9 connect rect (at -68.58 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 60 "Net-(P1-Pad9)"))
    (pad 7 connect rect (at -71.12 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 61 "Net-(P1-Pad7)"))
    (pad 5 connect rect (at -73.66 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 62 "Net-(P1-Pad5)"))
    (pad 3 connect rect (at -76.2 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 63 "Net-(P1-Pad3)"))
    (pad 1 connect rect (at -78.74 0) (size 1.54 7.62) (layers F.Cu F.Mask)
      (net 64 "Net-(P1-Pad1)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x32_Pitch2.54mm (layer F.Cu) (tedit 5A9944F7)
    (at 69.85 95.885 90)
    (descr "Through hole straight socket strip, 2x32, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x32 2.54mm double row")
    (fp_text reference "" (at -1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "" (at -1.27 81.07 90) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at -2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P1-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(P1-Pad21)"))
    (pad 22 thru_hole oval (at -2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P1-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at -2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P1-Pad25)"))
    (pad 26 thru_hole oval (at -2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad27)"))
    (pad 28 thru_hole oval (at -2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at -2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at -2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P1-Pad33)"))
    (pad 34 thru_hole oval (at -2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P1-Pad35)"))
    (pad 36 thru_hole oval (at -2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P1-Pad37)"))
    (pad 38 thru_hole oval (at -2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P1-Pad39)"))
    (pad 40 thru_hole oval (at -2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P1-Pad41)"))
    (pad 42 thru_hole oval (at -2.54 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad43)"))
    (pad 44 thru_hole oval (at -2.54 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad44)"))
    (pad 45 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P1-Pad45)"))
    (pad 46 thru_hole oval (at -2.54 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad46)"))
    (pad 47 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P1-Pad47)"))
    (pad 48 thru_hole oval (at -2.54 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad48)"))
    (pad 49 thru_hole oval (at 0 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P1-Pad49)"))
    (pad 50 thru_hole oval (at -2.54 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad50)"))
    (pad 51 thru_hole oval (at 0 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P1-Pad51)"))
    (pad 52 thru_hole oval (at -2.54 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad52)"))
    (pad 53 thru_hole oval (at 0 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P1-Pad53)"))
    (pad 54 thru_hole oval (at -2.54 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad54)"))
    (pad 55 thru_hole oval (at 0 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P1-Pad55)"))
    (pad 56 thru_hole oval (at -2.54 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad56)"))
    (pad 57 thru_hole oval (at 0 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P1-Pad57)"))
    (pad 58 thru_hole oval (at -2.54 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad58)"))
    (pad 59 thru_hole oval (at 0 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P1-Pad59)"))
    (pad 60 thru_hole oval (at -2.54 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad60)"))
    (pad 61 thru_hole oval (at 0 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P1-Pad61)"))
    (pad 62 thru_hole oval (at -2.54 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad62)"))
    (pad 63 thru_hole oval (at 0 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P1-Pad63)"))
    (pad 64 thru_hole oval (at -2.54 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad64)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x32_Pitch2.54mm.wrl
      (at (xyz -0.05 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 146.05 98.7)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 72.39 98.806 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x32_Pitch2.54mm (layer F.Cu) (tedit 5A997764)
    (at 69.85 92.71 90)
    (descr "Through hole straight socket strip, 1x32, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x32 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 81.07 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 0 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 0 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 0 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 0 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x32_Pitch2.54mm.wrl
      (at (xyz 0 -1.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_line (start 68.05 100.75) (end 68.05 90.7796) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 68.6 101.3) (end 68.05 100.75) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 68.6 109.45) (end 68.6 101.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114 109.45) (end 68.6 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114 101.4) (end 114 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.6 101.4) (end 114 101.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.6 109.45) (end 114.6 101.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.35 109.45) (end 114.6 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.35 101.4) (end 134.35 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.95 101.4) (end 134.35 101.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.95 109.45) (end 134.95 101.4) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.75 109.45) (end 134.95 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.75 101) (end 149.75 109.45) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.45 100.3) (end 149.75 101) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.45 90.7796) (end 150.45 100.3) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 68.05 90.7861) (end 150.45 90.7861) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text snw.lonningdal.no (at 103.9 100.55) (layer F.SilkS))
)
