(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 0)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.9972 49.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5D1267F5)
    (at 120 71.2)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS))
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2.9972 49.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 5D12670F)
    (at 178 71.2)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS))
    (fp_text value SolderWirePad_single_SMD_5x10mm (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2.9972 49.8) (layers F.Cu F.Paste F.Mask))
  )
  (gr_line (start 94.9 90.2) (end 203.1 90.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.9 51.7) (end 94.9 90.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.1 51.7) (end 203.1 90.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.9 51.7) (end 203.1 51.7) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.9 51.7) (xy 203 51.5) (xy 203.1 90.3) (xy 95.1 90.1)
      )
    )
  )
)
