(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 785)
    (zones 0)
    (modules 47)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 165 71)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 LA)
  (net 2 D4)
  (net 3 LB)
  (net 4 LC)
  (net 5 LD)
  (net 6 LE)
  (net 7 LF)
  (net 8 D3)
  (net 9 D2)
  (net 10 GND)
  (net 11 5V)
  (net 12 VCC)
  (net 13 SRCLK)
  (net 14 RCLK)
  (net 15 OE)
  (net 16 SER)
  (net 17 6)
  (net 18 7)
  (net 19 22)
  (net 20 "Net-(R1-Pad2)")
  (net 21 "Net-(R2-Pad2)")
  (net 22 "Net-(R3-Pad2)")
  (net 23 "Net-(R4-Pad2)")
  (net 24 "Net-(R5-Pad2)")
  (net 25 "Net-(R6-Pad2)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 LG)
  (net 28 LH)
  (net 29 "Net-(R8-Pad2)")
  (net 30 D1)
  (net 31 BA)
  (net 32 BB)
  (net 33 D0)
  (net 34 BC)
  (net 35 BD)
  (net 36 BE)
  (net 37 BF)
  (net 38 BG)
  (net 39 BH)
  (net 40 "Net-(U1-Pad9)")
  (net 41 "Net-(U2-Pad9)")
  (net 42 "Net-(U3-Pad1)")
  (net 43 D5)
  (net 44 D6)
  (net 45 D7)
  (net 46 "Net-(U3-Pad18)")
  (net 47 "Net-(U3-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 22)
    (add_net 5V)
    (add_net 6)
    (add_net 7)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net LA)
    (add_net LB)
    (add_net LC)
    (add_net LD)
    (add_net LE)
    (add_net LF)
    (add_net LG)
    (add_net LH)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad20)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 188.114 85.732 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C6CDAB0)
    (at 187.86 106.56)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C6CDAB0)
    (at 142.14 106.56)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C6CDAB0)
    (at 187.86 13.215)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 141.505 0.92)
    (fp_text reference D1 (at -3.035 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 LA))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 150.903 0.92)
    (fp_text reference D2 (at -2.685 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 160.301 0.92)
    (fp_text reference D3 (at -2.843 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 169.699 0.92)
    (fp_text reference D4 (at -2.747 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 179.097 0.92)
    (fp_text reference D5 (at -2.905 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 LE))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 188.495 0.92)
    (fp_text reference D6 (at -2.809 2.516) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 D4))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 LF))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 141.505 6.89)
    (fp_text reference D7 (at -2.781 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 LA))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 150.903 6.89)
    (fp_text reference D8 (at -2.685 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 160.301 6.89)
    (fp_text reference D9 (at -2.589 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 169.699 6.89)
    (fp_text reference D10 (at -2.239 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 179.097 6.89)
    (fp_text reference D11 (at -2.143 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 LE))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 188.495 6.89)
    (fp_text reference D12 (at -2.301 2.388) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 LF))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 D3))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 141.525 23.62)
    (fp_text reference D13 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 LA))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 148.275 23.62)
    (fp_text reference D14 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LB))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 160.625 23.62)
    (fp_text reference D15 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 LC))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 170.705 23.62)
    (fp_text reference D16 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LD))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 182.165 23.62)
    (fp_text reference D17 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 LE))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 188.905 23.62)
    (fp_text reference D18 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 LF))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 D2))
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59DE0611)
    (at 142.14 68.46)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 1.27 6.604) (layer B.SilkS))
    (fp_text value Conn_01x10 (at 1.27 -16.764) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 OE))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 6))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 7))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 22))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C25944D)
    (at 140.235 79.255 270)
    (fp_text reference J2 (at 3.175 -0.127 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 270) (layer F.Fab))
    (fp_text user %R (at 3.175 -0.127 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 5V))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.015 40.015 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 LA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 159.92 46.105 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 LB))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 161.825 40.015 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 LC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 163.73 46.105 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 LD))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 165.635 40.015 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 LE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.54 46.105 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 LF))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.445 40.015 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 26 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 LG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 171.35 46.105 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 LH))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 150 45.5)
    (fp_text reference SW1 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 18 7) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 LA))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 D1))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 31 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 180 45.5)
    (fp_text reference SW2 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 32 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 D1))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 LB))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 18 7) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 165 71)
    (fp_text reference SW3 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 LB))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 32 BB) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 150 86)
    (fp_text reference SW4 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 31 BA) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 LA))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 165 86)
    (fp_text reference SW5 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 34 BC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 LC))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 179.92 86)
    (fp_text reference SW6 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 LD))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 35 BD) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 165 101)
    (fp_text reference SW7 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 LE))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 36 BE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 150 116)
    (fp_text reference SW8 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 37 BF) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 LF))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 165 116)
    (fp_text reference SW9 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 38 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 LG))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 180 116)
    (fp_text reference SW10 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 17 6) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 LH))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 D0))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 39 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 155.475 56.395 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 15 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 BA))
    (pad 14 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 SER))
    (pad 13 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 OE))
    (pad 12 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 RCLK))
    (pad 11 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 SRCLK))
    (pad 10 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 9 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 7 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 BH))
    (pad 6 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 BG))
    (pad 5 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 BF))
    (pad 4 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 BE))
    (pad 3 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 BD))
    (pad 2 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 BC))
    (pad 1 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 BB))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 165 32.265 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R8-Pad2)"))
    (pad 8 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 9 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 11 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 SRCLK))
    (pad 12 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 RCLK))
    (pad 13 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 OE))
    (pad 14 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R1-Pad2)"))
    (pad 16 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 182.145 70.365 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 180) (layer F.SilkS))
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad9)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 D0))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 D1))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 D2))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 D3))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 VCC))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 OE))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 RCLK))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 SRCLK))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 D4))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 D5))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 D6))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 D7))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U3-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U3-Pad20)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C6CDAB0)
    (at 142.14 13.215)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 174.906 100.972 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text BLUE (at 188.622 26.804) (layer F.SilkS))
  (gr_text BLUE (at 141.632 26.804) (layer F.SilkS))
  (gr_text RED (at 182.018 26.804) (layer F.SilkS))
  (gr_text RED (at 148.49 26.804) (layer F.SilkS))
  (gr_text RED (at 165.508 23.756) (layer F.SilkS))
  (gr_text RED (at 183.542 3.944 90) (layer F.SilkS))
  (gr_text AMBER (at 165 4.198 90) (layer F.SilkS))
  (gr_text GREEN (at 146.204 4.452 90) (layer F.SilkS))
  (gr_text "ACP3-X-SRS-PCB\nREV. A, 2-20-2019" (at 188.368 45.6 90) (layer F.SilkS))
  (gr_text "ACP3-X-SRS-PCB\nREV. A, 2-20-2019" (at 175.16 84.716 90) (layer B.SilkS))
  (gr_text 5V (at 142.394 80.652) (layer B.SilkS))
  (gr_text 5V (at 142.394 80.652) (layer F.SilkS))
  (gr_text GND (at 142.902 78.112) (layer B.SilkS))
  (gr_text GND (at 142.902 78.112) (layer F.SilkS))
  (gr_line (start 138.33 -1.39) (end 191.67 -1.39) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.33 121.8) (end 191.67 121.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.33 -1.39) (end 138.33 121.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.67 -1.39) (end 191.67 121.8) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.33 -1.39) (xy 191.67 -1.39) (xy 191.67 121.8) (xy 138.33 121.8)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.33 -1.39) (xy 191.67 -1.39) (xy 191.67 121.8) (xy 138.33 121.8)
      )
    )
  )
)
