(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 135.124999 101.7565 176.872725 110.5979)
    (thickness 1.6)
    (drawings 12)
    (tracks 144)
    (zones 0)
    (modules 27)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "ground pad" (layer B.Cu) (tedit 579002BD)
    (at 172.2882 107.8738)
    (fp_text reference REF** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value "ground pad" (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS))
  )
  (module "ground pad" (layer B.Cu) (tedit 579002C2)
    (at 172.1104 104.1654)
    (fp_text reference REF** (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value "ground pad" (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask B.SilkS))
  )
  (module fh26footprints:FH26W-17S-0.3SHW (layer B.Cu) (tedit 578E6D32)
    (at 137.55 106.4 270)
    (fp_text reference "" (at 0 -0.5 270) (layer B.SilkS))
    (fp_text value XF3B (at 0 -2.6416 270) (layer B.Fab))
    (pad 1 connect rect (at -0.6 -1.7875 270) (size 0.3 0.8) (layers B.Cu B.Mask))
    (pad 2 connect rect (at 0 -1.7875 270) (size 0.3 0.8) (layers B.Cu B.Mask))
    (pad 3 connect rect (at 0.6 -1.7875 270) (size 0.3 0.8) (layers B.Cu B.Mask))
    (pad 4 connect rect (at 1.2 -1.7875 270) (size 0.3 0.8) (layers B.Cu B.Mask))
    (pad 5 connect rect (at -0.9 1.7875 270) (size 0.3 0.65) (layers B.Cu B.Mask))
    (pad 6 connect rect (at -0.3 1.7875 270) (size 0.3 0.65) (layers B.Cu B.Mask))
    (pad 7 connect rect (at 0.3 1.7875 270) (size 0.3 0.65) (layers B.Cu B.Mask))
    (pad 8 connect rect (at 0.9 1.7875 270) (size 0.3 0.65) (layers B.Cu B.Mask))
  )
  (module pins (layer F.Cu) (tedit 578E7564)
    (at 153.4 106.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75B5)
    (at 153.4 103.35)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7585)
    (at 153.45 108.75 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7590)
    (at 149.7 108.75 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75AD)
    (at 149.65 103.35)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E755F)
    (at 149.65 106.05)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E7554)
    (at 142.15 106.1)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E759E)
    (at 142.15 103.4)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7589)
    (at 142.2 108.8 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E758C)
    (at 145.95 108.8 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75A4)
    (at 145.9 103.4)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E755D)
    (at 145.9 106.1)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E7572)
    (at 168.5 106)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75D9)
    (at 168.5 103.3)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7575)
    (at 168.55 108.7 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E757E)
    (at 161.05 108.65 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75C9)
    (at 161 103.25)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E756B)
    (at 161 105.95)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module pins (layer F.Cu) (tedit 578E7568)
    (at 157.15 105.95)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75C2)
    (at 157.15 103.25)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E7581)
    (at 157.2 108.65 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeR_EIA-2012 (layer F.Cu) (tedit 578E757A)
    (at 164.8 108.7 180)
    (descr "Tantal Cap. , Size C, EIA-2012")
    (fp_text reference "" (at 0.0254 -1.2954 180) (layer F.SilkS))
    (fp_text value "NP0 capacitor(1.25x2mm, ceramic, SM)" (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at 0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.8 0 180) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.55 1.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm (layer F.Cu) (tedit 578E75D1)
    (at 164.75 103.3)
    (descr "Resistor, Ceramic, Horizontal")
    (tags "Resistor, Ceramic, Horizontal")
    (fp_text reference "" (at 0 -1.016) (layer F.SilkS))
    (fp_text value "metal film resistor(2x1.25mm, 7.5kohm, SM)" (at 0 1.016) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
    (model Resistors_ThroughHole.3dshapes/Resistor_Ceramic_Horizontal_L19mm-W8mm-H8mm-p25mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 1.1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pins (layer F.Cu) (tedit 578E756E)
    (at 164.75 106)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value pins (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "R3\n\n" (at 168.5798 104.521) (layer B.SilkS))
  (gr_text "R4\n" (at 164.719 103.3272) (layer B.SilkS))
  (gr_text R6 (at 160.8328 103.4288) (layer B.SilkS))
  (gr_text "R8\n" (at 156.972 103.4034) (layer B.SilkS))
  (gr_text R2 (at 153.4414 103.4288) (layer B.SilkS))
  (gr_text "R1\n" (at 149.5298 103.3018) (layer B.SilkS))
  (gr_text "R7\n\n" (at 145.8468 104.7496) (layer B.SilkS))
  (gr_text "R5\n" (at 142.1384 103.632) (layer B.SilkS))
  (gr_line (start 135.2 102.15) (end 135.2 110.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 102.15) (end 135.2 102.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 110.15) (end 174.3 102.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.3 110.15) (end 135.2 110.15) (angle 90) (layer Edge.Cuts) (width 0.15))
)
