(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 8)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (title_block
    (title NiCad-2-2032-13)
    (date 2020-08-02)
    (rev 1.0)
    (comment 4 "Author: James Powell")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (edge_width 0.05)
    (segment_width 0.7)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.17 2.17)
    (pad_drill 1.17)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BAT1-PadPos)")
  (net 2 "Net-(BAT1-PadNeg)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net "Net-(BAT1-PadNeg)")
    (add_net "Net-(BAT1-PadPos)")
  )
  (module digikey-footprints:Battery_Holder_Coin_2032_BS-7 (layer F.Cu) (tedit 5FCD9398)
    (at 134.6708 113.0108 205)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 11.3284 5.3848 25) (layer F.SilkS))
    (fp_text value BS-7 (at 7.4676 5.588 25) (layer F.Fab))
    (fp_text user %R (at 7.366 7.874 25) (layer F.Fab))
    (pad Neg thru_hole rect (at 0 0 180) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 2 "Net-(BAT1-PadNeg)"))
    (pad Pos thru_hole circle (at 20 0 205) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(BAT1-PadPos)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 112.75 116.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at -0.0756 0.1016) (layer B.SilkS))
    (fp_text value + (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -45) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(BAT1-PadPos)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 142.25 116.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at -0.01 0.127) (layer B.SilkS))
    (fp_text value - (at 0 -2.33) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(BAT1-PadNeg)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 114.7826 116.4844) (layer B.SilkS))
  (gr_text - (at 139.573 116.4844) (layer B.SilkS))
  (gr_text + (at 114.6556 116.4844) (layer F.SilkS))
  (gr_text - (at 130.9624 112.395) (layer F.SilkS))
  (gr_text + (at 120.7516 122.8852) (layer F.SilkS))
  (gr_text - (at 139.8016 115.4176) (layer F.SilkS))
  (gr_arc (start 143.5014 124) (end 145 124) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 143.5014 109) (end 145 109) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 145 124) (end 145 109) (layer Edge.Cuts) (width 0.0254))
  (gr_text "1/2 AA\nto\n2032\n" (at 110.4646 111.1758) (layer F.SilkS))
  (gr_arc (start 111.4986 124) (end 110 124) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 111.4986 109) (end 110 109) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 111.4986 125.5) (end 143.5014 125.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 111.4986 107.5) (end 143.5014 107.5) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 110 124) (end 110 109) (layer Edge.Cuts) (width 0.0254))
  (gr_text "1/2 AA to 2032\n" (at 136.3472 123.698) (layer B.SilkS))
)
