(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 15)
    (no_connects 0)
    (area 135.839999 86.309999 179.120001 111.810001)
    (thickness 1.6)
    (drawings 18)
    (tracks 47)
    (zones 0)
    (modules 13)
    (nets 11)
  )
  (page A4)
  (title_block
    (title "ZX Spectrum +2A/3 Composite Video PCB")
    (date 2016-10-23)
    (rev 0.9)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4572)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 142.24 83.185)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C301-Pad1)")
  (net 2 "Net-(C301-Pad2)")
  (net 3 "Net-(D301-Pad2)")
  (net 4 "Net-(D301-Pad1)")
  (net 5 "Net-(D302-Pad1)")
  (net 6 "Net-(D303-Pad1)")
  (net 7 "Net-(L301-Pad1)")
  (net 8 "Net-(P301-Pad4)")
  (net 9 "Net-(P302-Pad1)")
  (net 10 "Net-(Q301-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.4572)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C301-Pad2)")
    (add_net "Net-(D301-Pad1)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D302-Pad1)")
    (add_net "Net-(D303-Pad1)")
    (add_net "Net-(L301-Pad1)")
  )
  (net_class +12 ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P301-Pad4)")
  )
  (net_class COVO ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P302-Pad1)")
    (add_net "Net-(Q301-Pad1)")
  )
  (net_class GND ""
    (clearance 0.1524)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C301-Pad1)")
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 58112246)
    (at 147.955 90.17 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D301 (at 5.08 1.905 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D301-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D301-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5811225A)
    (at 161.29 109.22 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C301 (at 4.445 0 270) (layer F.SilkS))
    (fp_text value 39p (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C301-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 582DFF53)
    (at 161.29 104.775 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C302 (at 4.445 0 450) (layer F.SilkS))
    (fp_text value 47p (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C301-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 58112249)
    (at 151.765 90.17 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D302 (at 5.08 1.905 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D301-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D302-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 5811224B)
    (at 155.575 90.17 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D303 (at 5.08 1.905 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D302-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D303-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58112256)
    (at 144.145 106.68)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference L301 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text value 15m (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(L301-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C301-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58112287)
    (at 139.065 105.41 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P301 (at -2.54 3.81 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(L301-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D301-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P301-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5811239E)
    (at 175.26 93.345)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P302 (at 0 -2.54) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P302-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 582E013D)
    (at 165.1 95.25 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q301 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value 2N3904 (at 0 3 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D303-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P301-Pad4)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(Q301-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 58112238)
    (at 160.02 90.17 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R301 (at 5.08 2.54 270) (layer F.SilkS))
    (fp_text value 1.5k (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D303-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C301-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 582E013B)
    (at 169.545 100.33 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R302 (at 5.08 2.54 90) (layer F.SilkS))
    (fp_text value 75 (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(P302-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(Q301-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 582DFFAF)
    (at 140.97 91.44)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 582DFFA5)
    (at 174.625 107.315)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.4 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.4) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.697056 -1.697056) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_text "P302:\n1. Video OUT\n2. GND" (at 172.085 100.33) (layer F.SilkS))
  (dimension 43.18 (width 0.3) (layer Dwgs.User)
    (gr_text "1.7000 in" (at 157.48 116.92) (layer Dwgs.User))
    (feature1 (pts (xy 179.07 111.76) (xy 179.07 118.27)))
    (feature2 (pts (xy 135.89 111.76) (xy 135.89 118.27)))
    (crossbar (pts (xy 135.89 115.57) (xy 179.07 115.57)))
    (arrow1a (pts (xy 179.07 115.57) (xy 177.943496 116.156421)))
    (arrow1b (pts (xy 179.07 115.57) (xy 177.943496 114.983579)))
    (arrow2a (pts (xy 135.89 115.57) (xy 137.016504 116.156421)))
    (arrow2b (pts (xy 135.89 115.57) (xy 137.016504 114.983579)))
  )
  (gr_line (start 177.8 86.36) (end 137.16 86.36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.07 87.63) (end 177.8 86.36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.07 110.49) (end 179.07 87.63) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.8 111.76) (end 179.07 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 111.76) (end 177.8 111.76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "ver. 0.95" (at 177.8 94.615 90) (layer F.SilkS))
  (gr_text "P301:\n1. TEA2000 / LUMI (8)\n2. GND\n3. TEA2000 / COVO (6)\n4. +12V" (at 165.1 111.125 90) (layer F.SilkS))
  (gr_text "ZX Spectrum +2/3\nComposite Video" (at 147.955 109.855) (layer F.SilkS))
  (gr_line (start 135.89 87.63) (end 137.16 86.36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.89 110.49) (end 135.89 87.63) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 111.76) (end 135.89 110.49) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 25.4 (width 0.3) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 130.73 99.06 90) (layer Dwgs.User))
    (feature1 (pts (xy 135.89 86.36) (xy 129.38 86.36)))
    (feature2 (pts (xy 135.89 111.76) (xy 129.38 111.76)))
    (crossbar (pts (xy 132.08 111.76) (xy 132.08 86.36)))
    (arrow1a (pts (xy 132.08 86.36) (xy 132.666421 87.486504)))
    (arrow1b (pts (xy 132.08 86.36) (xy 131.493579 87.486504)))
    (arrow2a (pts (xy 132.08 111.76) (xy 132.666421 110.633496)))
    (arrow2b (pts (xy 132.08 111.76) (xy 131.493579 110.633496)))
  )
)
