(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 57)
    (no_connects 0)
    (area -0.100001 -0.100001 279.500001 216.000001)
    (thickness 1.6)
    (drawings 64)
    (tracks 186)
    (zones 0)
    (modules 27)
    (nets 36)
  )
  (page A)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.8128)
    (zone_clearance 0.4064)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1.6256)
    (via_drill 0.8128)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 7 7)
    (pad_drill 3.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x01000_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +24V)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 /DI1)
  (net 5 "Net-(D2-Pad1)")
  (net 6 /DI2)
  (net 7 "Net-(D3-Pad1)")
  (net 8 /DI3)
  (net 9 "Net-(D4-Pad1)")
  (net 10 /DI4)
  (net 11 "Net-(D5-Pad1)")
  (net 12 /DI5)
  (net 13 "Net-(D6-Pad1)")
  (net 14 /DI6)
  (net 15 +5V)
  (net 16 /IN)
  (net 17 /OUT)
  (net 18 VEE)
  (net 19 "Net-(Q1-Pad1)")
  (net 20 "Net-(U2-Pad10)")
  (net 21 "Net-(U2-Pad12)")
  (net 22 "Net-(U2-Pad14)")
  (net 23 "Net-(D1-Pad2)")
  (net 24 "Net-(D2-Pad2)")
  (net 25 "Net-(D3-Pad2)")
  (net 26 "Net-(D4-Pad2)")
  (net 27 "Net-(D5-Pad2)")
  (net 28 "Net-(D6-Pad2)")
  (net 29 "Net-(U2-Pad7)")
  (net 30 "Net-(U1-Pad10)")
  (net 31 "Net-(U1-Pad12)")
  (net 32 "Net-(U1-Pad14)")
  (net 33 "Net-(J1-Pad1)")
  (net 34 "Net-(R7-Pad2)")
  (net 35 "Net-(R8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.8128)
    (trace_width 0.635)
    (via_dia 1.6256)
    (via_drill 0.8128)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +5V)
    (add_net /DI1)
    (add_net /DI2)
    (add_net /DI3)
    (add_net /DI4)
    (add_net /DI5)
    (add_net /DI6)
    (add_net /IN)
    (add_net /OUT)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad7)")
    (add_net VEE)
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 5AFD809E)
    (at 107.95 104.14 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 4.445 270) (layer B.SilkS))
    (fp_text value Q_PMOS_GDS (at 0 -4.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 540) (layer B.Fab))
    (pad 2 smd rect (at 3.15 0 270) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.48) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 3 smd rect (at -3.15 -2.3 270) (size 2 1.48) (layers B.Cu B.Paste B.Mask)
      (net 1 +24V))
    (pad 1 smd rect (at -3.15 2.3 270) (size 2 1.48) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 5AFC6C67)
    (at 173.6852 146.4437)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 5AFC6C67)
    (at 105.7148 146.4437)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 5AFC6C67)
    (at 173.6852 69.4563)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad locked (layer F.Cu) (tedit 5AFC6C67)
    (at 105.7148 69.4563)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.4) (layers *.Cu *.Mask))
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EE1)
    (at 109.22 123.19 180)
    (fp_text reference D1 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EE4)
    (at 124.46 123.19 180)
    (fp_text reference D2 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EE9)
    (at 139.7 123.19 180)
    (fp_text reference D3 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5AFD8097)
    (at 107.95 110.49)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -3.175 0 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5AFD80B8)
    (at 107.95 113.03 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 3.175 0 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD8089)
    (at 109.22 134.62 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.445 0 90) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /DI1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD808B)
    (at 124.46 134.62 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -4.445 0 90) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /DI2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD808E)
    (at 139.7 134.62 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.445 0 90) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 /DI3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD8085)
    (at 139.7 81.28 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -4.445 0 270) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /DI4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EED)
    (at 139.7 92.71 180)
    (fp_text reference D4 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EF1)
    (at 124.46 92.71 180)
    (fp_text reference D5 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module My_Modules:LED-3mm-0.1 (layer F.Cu) (tedit 5AFD7EF5)
    (at 109.22 92.71 180)
    (fp_text reference D6 (at 3.175 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.7 2.3) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD8082)
    (at 124.46 81.28 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.445 0 270) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 /DI5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD807F)
    (at 109.22 81.28 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.445 0 270) (layer B.SilkS))
    (fp_text value 1.1K (at 0 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 /DI6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 5AFD81CD)
    (at 153.67 97.79 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 2.54 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 +24V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5AFD7EF9)
    (at 115.57 118.11 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.81 -2.54 90) (layer F.SilkS))
    (fp_text value LTV-847 (at 3.81 20.11 90) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(R7-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /IN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 VEE))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 5AFD7F00)
    (at 133.35 97.79 270)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U2 (at 3.81 20.32 270) (layer F.SilkS))
    (fp_text value LTV-847 (at 3.81 20.11 270) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 7.62 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D5-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad14)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 7.62 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad12)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D6-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad14)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad7)"))
    (pad 15 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad14)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /OUT))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5AFD80B2)
    (at 107.95 118.11)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -3.175 0 90) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module My_Modules:OSTTC092162 (layer F.Cu) (tedit 5AFD7F09)
    (at 124.46 129.54)
    (fp_text reference J1 (at 24.765 0 90) (layer F.SilkS))
    (fp_text value "Left Sensors" (at 0 -2.54) (layer F.Fab))
    (pad 9 thru_hole circle (at 20.32 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 15.24 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 /DI3))
    (pad 1 thru_hole circle (at -20.32 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -15.24 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 /DI1))
    (pad 3 thru_hole circle (at -10.16 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -5.08 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 5 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 /DI2))
    (pad 6 thru_hole circle (at 5.08 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 10.16 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
  )
  (module My_Modules:OSTTC092162 (layer F.Cu) (tedit 5AFD7F10)
    (at 124.46 86.36 180)
    (fp_text reference J2 (at -24.765 0 270) (layer F.SilkS))
    (fp_text value "Right Sensors" (at 0 -2.54 180) (layer F.Fab))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 15.24 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 /DI6))
    (pad 1 thru_hole circle (at -20.32 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -15.24 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 /DI4))
    (pad 3 thru_hole circle (at -10.16 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -5.08 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 5 thru_hole circle (at 0 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 /DI5))
    (pad 6 thru_hole circle (at 5.08 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 10.16 0 180) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad1)"))
  )
  (module My_Modules:OSTTC062162 (layer F.Cu) (tedit 5AFD7F12)
    (at 148.59 107.95 90)
    (fp_text reference J3 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value "Cart Interface" (at 0 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -12.7 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 15 +5V))
    (pad 2 thru_hole circle (at -7.62 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 /IN))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 /OUT))
    (pad 4 thru_hole circle (at 2.54 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 VEE))
    (pad 5 thru_hole circle (at 7.62 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module My_Modules:Android-Logo (layer F.Cu) (tedit 0)
    (at 168.91 107.95 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text EX20010-000-E (at 175.26 107.95 90) (layer F.SilkS))
  (gr_text DI6 (at 109.22 81.28 180) (layer F.SilkS))
  (gr_text DI5 (at 124.46 81.28 180) (layer F.SilkS))
  (gr_text DI4 (at 139.7 81.28 180) (layer F.SilkS))
  (gr_text GND (at 104.14 81.28 180) (layer F.SilkS))
  (gr_text GND (at 119.38 81.28 180) (layer F.SilkS))
  (gr_text GND (at 134.62 81.28 180) (layer F.SilkS))
  (gr_text 24V (at 144.78 81.28 180) (layer F.SilkS))
  (gr_text 24V (at 129.54 81.28 180) (layer F.SilkS))
  (gr_text 24V (at 114.3 81.28 180) (layer F.SilkS))
  (gr_text DI3 (at 139.7 134.62) (layer F.SilkS))
  (gr_text DI2 (at 124.46 134.62) (layer F.SilkS))
  (gr_text DI1 (at 109.22 134.62) (layer F.SilkS))
  (gr_text GND (at 144.78 134.62) (layer F.SilkS))
  (gr_text GND (at 129.54 134.62) (layer F.SilkS))
  (gr_text GND (at 114.3 134.62) (layer F.SilkS))
  (gr_text 24V (at 134.62 134.62) (layer F.SilkS))
  (gr_text 24V (at 119.38 134.62) (layer F.SilkS))
  (gr_text 24V (at 104.14 134.62) (layer F.SilkS))
  (gr_text ISOLATED (at 160.02 113.03 90) (layer F.SilkS))
  (gr_text GND (at 153.67 105.41 90) (layer F.SilkS))
  (gr_text OUT (at 153.67 110.49 90) (layer F.SilkS))
  (gr_text IN (at 153.67 115.57 90) (layer F.SilkS))
  (gr_text 5V (at 153.67 120.65 90) (layer F.SilkS))
  (gr_text 24V (at 153.67 100.33 90) (layer F.SilkS))
  (gr_text GND (at 153.67 95.25 90) (layer F.SilkS))
  (gr_line (start 100.9523 146.4437) (end 100.9523 69.4563) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 173.6852 151.2062) (end 105.7148 151.2062) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.4477 69.4563) (end 178.4477 146.4437) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.7148 64.6938) (end 173.6852 64.6938) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.7148 146.4437) (end 105.7148 151.2062) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 173.6852 146.4437) (end 178.4477 146.4437) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 173.6852 69.4563) (end 173.6852 64.6938) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 105.7148 69.4563) (end 100.9523 69.4563) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.8128) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 179.07 152.4) (xy 100.33 152.4) (xy 100.33 63.5) (xy 179.07 63.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.8128) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 179.07 152.4) (xy 100.33 152.4) (xy 100.33 63.5) (xy 179.07 63.5)
      )
    )
  )
)
