(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 111)
    (no_connects 2)
    (area 99.949999 99.949999 142.800001 141.900001)
    (thickness 1.6)
    (drawings 25)
    (tracks 491)
    (zones 0)
    (modules 40)
    (nets 49)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.7 0.5)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 +3V3)
  (net 7 +1V8)
  (net 8 "Net-(D1-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D2-Pad1)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 "Net-(D3-Pad1)")
  (net 13 "Net-(D3-Pad2)")
  (net 14 /NINT)
  (net 15 "Net-(P2-Pad7)")
  (net 16 "Net-(P2-Pad10)")
  (net 17 "Net-(P2-Pad8)")
  (net 18 "Net-(P2-Pad6)")
  (net 19 "Net-(P2-Pad4)")
  (net 20 "Net-(P2-Pad2)")
  (net 21 "Net-(P3-Pad1)")
  (net 22 "Net-(P3-Pad2)")
  (net 23 "Net-(P3-Pad3)")
  (net 24 "Net-(P3-Pad4)")
  (net 25 "Net-(P3-Pad5)")
  (net 26 "Net-(P3-Pad6)")
  (net 27 "Net-(P3-Pad7)")
  (net 28 "Net-(P4-Pad2)")
  (net 29 +5V)
  (net 30 "Net-(P5-Pad2)")
  (net 31 "Net-(P5-Pad3)")
  (net 32 "Net-(P5-Pad4)")
  (net 33 +BATT)
  (net 34 "Net-(R4-Pad1)")
  (net 35 "Net-(R5-Pad1)")
  (net 36 "Net-(U1-Pad1)")
  (net 37 "Net-(U1-Pad5)")
  (net 38 "Net-(U1-Pad6)")
  (net 39 "Net-(U1-Pad7)")
  (net 40 "Net-(U1-Pad8)")
  (net 41 "Net-(U1-Pad14)")
  (net 42 "Net-(U2-Pad11)")
  (net 43 "Net-(U2-Pad12)")
  (net 44 "Net-(U2-Pad13)")
  (net 45 "Net-(U2-Pad18)")
  (net 46 /SCL)
  (net 47 /SDA)
  (net 48 "Net-(P5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net /NINT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad6)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad4)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad18)")
    (add_net VCC)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 129.45 110.05 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 0)
    (at 111.15 117.65114 270)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at 8.59886 -0.1 270) (layer F.SilkS))
    (fp_text value Crystal (at 2.54 5.08 270) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 270) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 4.84886 0 270) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 131.4 137.3)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0.05 2.5) (layer F.SilkS))
    (fp_text value TLV70018DDC (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 123.7 122.95)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 10.1 0.05 90) (layer F.SilkS))
    (fp_text value TLV70033DDC (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 120.15 115.3)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U2 (at -5.15 -5.85) (layer F.SilkS))
    (fp_text value STM32F042K6T6 (at 0 5.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad10)"))
    (pad 5 smd rect (at -4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 6 smd rect (at -4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 7 smd rect (at -4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P4-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P3-Pad1)"))
    (pad 15 smd rect (at 2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P3-Pad2)"))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 18 smd rect (at 4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /SCL))
    (pad 20 smd rect (at 4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /SDA))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P5-Pad2)"))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P5-Pad3)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad4)"))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /NINT))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P3-Pad3)"))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P3-Pad4)"))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P3-Pad5)"))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P3-Pad6)"))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P3-Pad7)"))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R4-Pad1)"))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:14_OESIP (layer F.Cu) (tedit 586B0FB1)
    (at 136.75 136.35 180)
    (fp_text reference U1 (at -1 -3.75 180) (layer F.SilkS))
    (fp_text value MAX30105 (at 0.125 -3.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.2 -2.4 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -1.2 -1.6 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 46 /SCL))
    (pad 3 smd rect (at -1.2 -0.8 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 47 /SDA))
    (pad 4 smd rect (at -1.2 0 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.2 0.8 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -1.2 1.6 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -1.2 2.4 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 1.2 2.4 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 1.2 1.6 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 10 smd rect (at 1.2 0.8 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 11 smd rect (at 1.2 0 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 12 smd rect (at 1.2 -0.8 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 1.2 -1.6 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 /NINT))
    (pad 14 smd rect (at 1.2 -2.4 180) (size 0.75 0.35) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad14)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 119.5 122.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -11.6 270) (layer F.SilkS))
    (fp_text value DNI (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 117.9 122.6 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -11.9 270) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 +BATT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 103.8 113.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0.05 -2.65 270) (layer F.SilkS))
    (fp_text value 140R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 103.9 117.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.1 -2.8 270) (layer F.SilkS))
    (fp_text value 140R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 103.8 122.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.05 -2.65 270) (layer F.SilkS))
    (fp_text value 140R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 136.5 112.05 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.3 -0.05 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 locked (layer F.Cu) (tedit 58307A47)
    (at 132.9 112.7 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P5-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 115.95 125.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0.15 -1.5 90) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 116.3 122.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.45 12.15 90) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 126.85 110.05 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 126.55 119.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.9 0.05) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /NINT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 126.05 117.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.35 0.1 90) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 127.65 116.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.35 0.25 90) (layer F.SilkS))
    (fp_text value 2K2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 /SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 112.08 131.1)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 7.97 2.3) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +BATT))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +3V3))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 +1V8))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 118.61 126.5)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 5.24 1.2) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 +BATT))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5543E447)
    (at 140.15 114.1 90)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P5 (at -3.65 -3.8 90) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 4.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3009 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at -0.6509 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P5-Pad2)"))
    (pad 3 smd rect (at -0.0009 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P5-Pad3)"))
    (pad 4 smd rect (at 0.6491 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P5-Pad4)"))
    (pad 5 smd rect (at 1.2991 -1.56254 180) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.5009 -1.56254 180) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 6 thru_hole oval (at 2.4991 -1.56254 180) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 6 thru_hole oval (at -3.5009 1.13746 180) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 6 thru_hole oval (at 3.4991 1.13746 180) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 54E9F429)
    (at 108.14 126.75 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at -2.86 -1.65 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(P4-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module parts:CONN_JTAG_10 (layer F.Cu) (tedit 586B0481)
    (at 134 104.3 270)
    (fp_text reference P2 (at 1.7 -7.7 270) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -7.375 270) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 3 smd rect (at -1.95 -1.27 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.95 0 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -1.95 1.27 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P2-Pad7)"))
    (pad 9 smd rect (at -1.95 2.54 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 1.95 2.54 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad10)"))
    (pad 8 smd rect (at 1.95 1.27 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad8)"))
    (pad 6 smd rect (at 1.95 0 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P2-Pad6)"))
    (pad 4 smd rect (at 1.95 -1.27 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad4)"))
    (pad 2 smd rect (at 1.95 -2.54 270) (size 2.4 0.76) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad2)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05 (layer F.Cu) (tedit 0)
    (at 139.02 131.1 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.13 -2.95 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /SCL))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 /SDA))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /NINT))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 134.05 136.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 3.25 -0.1 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 128.75 136.95 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.1 1.45 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 126.35 122.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.4 -8.75 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 121.05 122.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0.45 -11.4 270) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 134.95 112.05 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.3 -0.05 270) (layer F.SilkS))
    (fp_text value C (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 107.8 122.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.45 0.15 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 107.8 113.2 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -2.6 -0.1 270) (layer F.SilkS))
    (fp_text value C (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 133.35 134.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.25 -0.15 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:LED_2.1X1.6_RA (layer F.Cu) (tedit 586AFB56)
    (at 102.1 122.1 90)
    (fp_text reference D1 (at -1.1 3.1 90) (layer F.SilkS))
    (fp_text value LED (at 0 -2.475 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
  )
  (module parts:LED_2.1X1.6_RA (layer F.Cu) (tedit 586AFB56)
    (at 102.2 117.4 90)
    (fp_text reference D2 (at -1.1 3.2 90) (layer F.SilkS))
    (fp_text value LED (at 0 -2.475 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
  )
  (module parts:LED_2.1X1.6_RA (layer F.Cu) (tedit 586AFB56)
    (at 102.1 112.7 90)
    (fp_text reference D3 (at -1.05 3.15 90) (layer F.SilkS))
    (fp_text value LED (at 0 -2.475 90) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.3 0 90) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad2)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05 (layer F.Cu) (tedit 0)
    (at 139.03 126.85 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at -0.87 2.7 180) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 /SCL))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 /SDA))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /NINT))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x05.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 125.59 105.2 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(P3-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(P3-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 54E9F429)
    (at 104.3 102.26 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P9 (at -0.56 -2.65 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 134.15 116.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "hackhat v0.1\n2017-01-05\nPatrick Yeon" (at 132.55 120.35) (layer B.SilkS))
  (gr_line (start 100 141.85) (end 142.75 141.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 100) (end 100 141.85) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.75 100) (end 100 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.75 141.85) (end 142.75 100) (layer Edge.Cuts) (width 0.1))
)
