(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 60)
    (tracks 323)
    (zones 0)
    (modules 14)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC_IO2)
  (net 3 +3V3)
  (net 4 /VCC_IO1)
  (net 5 VCC)
  (net 6 +1V8)
  (net 7 /TCK)
  (net 8 /TDO)
  (net 9 /TDI)
  (net 10 /TMS)
  (net 11 "Net-(U2-Pad6)")
  (net 12 "Net-(U2-Pad3)")
  (net 13 /INPUT)
  (net 14 /FB1_16)
  (net 15 /FB1_15)
  (net 16 /FB1_14)
  (net 17 /FB1_13)
  (net 18 /FB1_12)
  (net 19 /FB1_11)
  (net 20 /FB1_10)
  (net 21 /FB1_9)
  (net 22 /FB1_8)
  (net 23 /FB1_7)
  (net 24 /FB1_6)
  (net 25 /FB1_5)
  (net 26 /FB1_4)
  (net 27 /FB1_3)
  (net 28 /FB1_2)
  (net 29 /FB1_1)
  (net 30 /FB2_16)
  (net 31 /FB2_15)
  (net 32 /FB2_14)
  (net 33 /FB2_13)
  (net 34 /FB2_12)
  (net 35 /FB2_11)
  (net 36 /FB2_10)
  (net 37 /FB2_9)
  (net 38 /FB2_8)
  (net 39 /FB2_7)
  (net 40 /FB2_6)
  (net 41 /FB2_5)
  (net 42 /FB2_4)
  (net 43 /FB2_3)
  (net 44 /FB2_2)
  (net 45 /FB2_1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /FB1_1)
    (add_net /FB1_10)
    (add_net /FB1_11)
    (add_net /FB1_12)
    (add_net /FB1_13)
    (add_net /FB1_14)
    (add_net /FB1_15)
    (add_net /FB1_16)
    (add_net /FB1_2)
    (add_net /FB1_3)
    (add_net /FB1_4)
    (add_net /FB1_5)
    (add_net /FB1_6)
    (add_net /FB1_7)
    (add_net /FB1_8)
    (add_net /FB1_9)
    (add_net /FB2_1)
    (add_net /FB2_10)
    (add_net /FB2_11)
    (add_net /FB2_12)
    (add_net /FB2_13)
    (add_net /FB2_14)
    (add_net /FB2_15)
    (add_net /FB2_16)
    (add_net /FB2_2)
    (add_net /FB2_3)
    (add_net /FB2_4)
    (add_net /FB2_5)
    (add_net /FB2_6)
    (add_net /FB2_7)
    (add_net /FB2_8)
    (add_net /FB2_9)
    (add_net /INPUT)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad6)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net /VCC_IO1)
    (add_net /VCC_IO2)
    (add_net GND)
    (add_net VCC)
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 113.538 114.173 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.032 1.524 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias (layer F.Cu) (tedit 5DC5FE75)
    (at 107.823 114.149 180)
    (descr "MSOP, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf#page=15), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U2 (at 0 2.516) (layer F.SilkS))
    (fp_text value MIC5355-SGYMME (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.43 0.59 180) (size 0.72 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.43 -0.59 180) (size 0.72 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 0.59 180) (size 0.72 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 -0.59 180) (size 0.72 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 9 smd rect (at 0 0 180) (size 1.5 1.5) (layers B.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.5 0.5 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.5 0.5 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.5 -0.5 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.5 -0.5 180) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 9 smd rect (at 0 0 180) (size 2.5 3) (layers F.Cu)
      (net 1 GND))
    (pad "" smd rect (at 0 0 180) (size 1.73 2.36) (layers F.Mask))
    (pad 8 smd roundrect (at 2.175 -0.975 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 7 smd roundrect (at 2.175 -0.325 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +1V8))
    (pad 6 smd roundrect (at 2.175 0.325 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U2-Pad6)"))
    (pad 5 smd roundrect (at 2.175 0.975 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (pad 4 smd roundrect (at -2.175 0.975 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (pad 3 smd roundrect (at -2.175 0.325 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U2-Pad3)"))
    (pad 2 smd roundrect (at -2.175 -0.325 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.175 -0.975 180) (size 1.35 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-44_10x10mm_P0.8mm (layer F.Cu) (tedit 5D9F72AF)
    (at 107.85 91.44)
    (descr "LQFP, 44 Pin (https://www.nxp.com/files-static/shared/doc/package_info/98ASS23225W.pdf?&fsrch=1), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U1 (at -0.027 -7.493) (layer F.SilkS))
    (fp_text value XC2C32A-VQ44 (at 0 7.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 44 smd roundrect (at -4 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /FB2_6))
    (pad 43 smd roundrect (at -3.2 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /FB2_5))
    (pad 42 smd roundrect (at -2.4 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /FB2_4))
    (pad 41 smd roundrect (at -1.6 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /FB2_3))
    (pad 40 smd roundrect (at -0.8 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /FB2_2))
    (pad 39 smd roundrect (at 0 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /FB2_1))
    (pad 38 smd roundrect (at 0.8 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /FB1_1))
    (pad 37 smd roundrect (at 1.6 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /FB1_2))
    (pad 36 smd roundrect (at 2.4 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /FB1_3))
    (pad 35 smd roundrect (at 3.2 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 34 smd roundrect (at 4 -5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /FB1_4))
    (pad 33 smd roundrect (at 5.6625 -4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /FB1_5))
    (pad 32 smd roundrect (at 5.6625 -3.2) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /FB1_6))
    (pad 31 smd roundrect (at 5.6625 -2.4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /FB1_7))
    (pad 30 smd roundrect (at 5.6625 -1.6) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /FB1_8))
    (pad 29 smd roundrect (at 5.6625 -0.8) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /FB1_9))
    (pad 28 smd roundrect (at 5.6625 0) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /FB1_10))
    (pad 27 smd roundrect (at 5.6625 0.8) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /FB1_11))
    (pad 26 smd roundrect (at 5.6625 1.6) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC_IO2))
    (pad 25 smd roundrect (at 5.6625 2.4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 24 smd roundrect (at 5.6625 3.2) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /TDO))
    (pad 23 smd roundrect (at 5.6625 4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /FB1_12))
    (pad 22 smd roundrect (at 4 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /FB1_13))
    (pad 21 smd roundrect (at 3.2 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /FB1_14))
    (pad 20 smd roundrect (at 2.4 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /FB1_15))
    (pad 19 smd roundrect (at 1.6 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /FB1_16))
    (pad 18 smd roundrect (at 0.8 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /INPUT))
    (pad 17 smd roundrect (at 0 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at -0.8 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /FB2_16))
    (pad 15 smd roundrect (at -1.6 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 14 smd roundrect (at -2.4 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /FB2_15))
    (pad 13 smd roundrect (at -3.2 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /FB2_14))
    (pad 12 smd roundrect (at -4 5.6625) (size 0.55 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /FB2_13))
    (pad 11 smd roundrect (at -5.6625 4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /TCK))
    (pad 10 smd roundrect (at -5.6625 3.2) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /TMS))
    (pad 9 smd roundrect (at -5.6625 2.4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /TDI))
    (pad 8 smd roundrect (at -5.6625 1.6) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /FB2_12))
    (pad 7 smd roundrect (at -5.6625 0.8) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /VCC_IO1))
    (pad 6 smd roundrect (at -5.6625 0) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /FB2_11))
    (pad 5 smd roundrect (at -5.6625 -0.8) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /FB2_10))
    (pad 4 smd roundrect (at -5.6625 -1.6) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -5.6625 -2.4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /FB2_9))
    (pad 2 smd roundrect (at -5.6625 -3.2) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /FB2_8))
    (pad 1 smd roundrect (at -5.6625 -4) (size 1.475 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /FB2_7))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 105.41 109.22 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at 0.127 -3.048 180) (layer F.SilkS) hide)
    (fp_text value Jumper_3_Open (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +1V8))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC_IO1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110.49 105.41 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP1 (at 0 8.0645 180) (layer F.SilkS) hide)
    (fp_text value Jumper_3_Open (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC_IO2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +1V8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 101.6 67.31 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Male (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /TCK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /TDO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /TDI))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /TMS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 97.79 67.31 180)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x20_Male (at 0 -50.59) (layer B.Fab))
    (fp_text user %R (at 0 -24.13 -90) (layer B.Fab))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +1V8))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VCC_IO1))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /FB2_16))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /FB2_15))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /FB2_14))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /FB2_13))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /FB2_12))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /FB2_11))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /FB2_10))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /FB2_9))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /FB2_8))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /FB2_7))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /FB2_6))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /FB2_5))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /FB2_4))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /FB2_3))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /FB2_2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /FB2_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 118.11 67.4 180)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value Conn_01x20_Male (at 0 -50.59) (layer B.Fab))
    (fp_text user %R (at 0 -24.13 270) (layer B.Fab))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VCC_IO2))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /INPUT))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /FB1_16))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /FB1_15))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /FB1_14))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /FB1_13))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /FB1_12))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /FB1_11))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /FB1_10))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /FB1_9))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /FB1_8))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /FB1_7))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /FB1_6))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /FB1_5))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /FB1_4))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /FB1_3))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /FB1_2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /FB1_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 100.838 114.046 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.159 -2.159 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 103.251 114.046 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.159 2.54 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 +1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 111.0996 82.9564 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.9906 1.8034 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 100.2411 92.5449 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.5019 0.5461 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0.05 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /VCC_IO1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 107.061 100.457)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.5065 93.98 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 3.302 1.5875) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /VCC_IO2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1.8 (at 110.49 102.997) (layer F.SilkS))
  (gr_text 3.3 (at 105.41 103.124) (layer F.SilkS))
  (gr_text FB2 (at 101.473 101.727 270) (layer F.SilkS))
  (gr_text 16 (at 99.441 105.41 270) (layer F.SilkS))
  (gr_text 15 (at 99.441 102.743 270) (layer F.SilkS))
  (gr_text 14 (at 99.441 100.203 270) (layer F.SilkS))
  (gr_text 13 (at 99.441 97.79 270) (layer F.SilkS))
  (gr_text 12 (at 99.441 95.25 270) (layer F.SilkS))
  (gr_text 9 (at 99.441 87.503 270) (layer F.SilkS))
  (gr_text 8 (at 99.441 85.09 270) (layer F.SilkS))
  (gr_text "7\n" (at 99.441 82.55 270) (layer F.SilkS))
  (gr_text 6 (at 99.441 80.01 270) (layer F.SilkS))
  (gr_text 5 (at 99.441 77.47 270) (layer F.SilkS))
  (gr_text 4 (at 99.441 74.93 270) (layer F.SilkS))
  (gr_text 3 (at 99.441 72.517 270) (layer F.SilkS))
  (gr_text 2 (at 99.441 69.85 270) (layer F.SilkS))
  (gr_text 1 (at 99.441 67.31 270) (layer F.SilkS))
  (gr_text "XC2C32A-VQ44\nBREAKOUT\nBOARD" (at 107.823 76.962) (layer F.SilkS))
  (gr_text 15 (at 116.459 102.87 90) (layer F.SilkS))
  (gr_text 14 (at 116.459 100.457 90) (layer F.SilkS))
  (gr_text 13 (at 116.459 97.917 90) (layer F.SilkS))
  (gr_text 12 (at 116.459 95.25 90) (layer F.SilkS))
  (gr_text 11 (at 116.459 92.456 90) (layer F.SilkS))
  (gr_text 10 (at 116.459 90.297 90) (layer F.SilkS))
  (gr_text 9 (at 116.332 87.757 90) (layer F.SilkS))
  (gr_text 8 (at 116.332 85.217 90) (layer F.SilkS))
  (gr_text "7\n" (at 116.332 82.677 90) (layer F.SilkS))
  (gr_text 6 (at 116.332 80.137 90) (layer F.SilkS))
  (gr_text 5 (at 116.332 77.597 90) (layer F.SilkS))
  (gr_text 4 (at 116.332 75.057 90) (layer F.SilkS))
  (gr_text 3 (at 116.332 72.517 90) (layer F.SilkS))
  (gr_text 1 (at 116.332 67.437 90) (layer F.SilkS))
  (gr_text 2 (at 116.332 69.977 90) (layer F.SilkS))
  (gr_text 16 (at 116.459 105.41 90) (layer F.SilkS))
  (gr_text FB1 (at 114.046 101.6 90) (layer F.SilkS))
  (gr_text 3.3V (at 100.584 112.014) (layer F.SilkS))
  (gr_text 1.8V (at 100.584 110.236) (layer F.SilkS))
  (gr_text VCCIO1 (at 100.965 108.077) (layer F.SilkS))
  (gr_text GND (at 115.824 115.697) (layer F.SilkS))
  (gr_text VIN (at 115.951 113.157) (layer F.SilkS))
  (gr_text VCCIO2 (at 114.935 110.49) (layer F.SilkS))
  (gr_text INP (at 115.316 107.95) (layer F.SilkS))
  (gr_text 3V3 (at 113.792 72.517 90) (layer F.SilkS))
  (gr_text GND (at 111.633 72.644 90) (layer F.SilkS))
  (gr_text TCK (at 109.22 72.39 90) (layer F.SilkS))
  (gr_text TDO (at 106.68 72.39 90) (layer F.SilkS))
  (gr_text TDI (at 104.267 72.39 90) (layer F.SilkS))
  (gr_text TMS (at 101.854 72.39 90) (layer F.SilkS))
  (gr_line (start 96.52 116.84) (end 96.52 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 116.84) (end 96.52 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.38 66.04) (end 119.38 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.52 66.04) (end 119.38 66.04) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.888 117.348) (xy 96.012 117.348) (xy 96.012 65.532) (xy 119.888 65.532)
      )
    )
  )
)
