(kicad_pcb (version 4) (host pcbnew 0.201601191446+6495~42~ubuntu15.10.1-product)
  (general
    (links 43)
    (no_connects 0)
    (area 48.115999 32.857999 98.216001 82.958001)
    (thickness 1.6)
    (drawings 83)
    (tracks 150)
    (zones 0)
    (modules 26)
    (nets 19)
  )
  (page User 140.005 150.012)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5VD)
  (net 2 GND_D)
  (net 3 GND_A)
  (net 4 -5V)
  (net 5 +5V)
  (net 6 VIN_R)
  (net 7 VOUT_R)
  (net 8 VIN_L)
  (net 9 VOUT_L)
  (net 10 ZCEN)
  (net 11 SDI)
  (net 12 CS)
  (net 13 SCLK)
  (net 14 MUTE)
  (net 15 SDO)
  (net 16 "Net-(D1-Pad2)")
  (net 17 "Net-(D2-Pad2)")
  (net 18 "Net-(D3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +5VD)
    (add_net -5V)
    (add_net CS)
    (add_net GND_A)
    (add_net GND_D)
    (add_net MUTE)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net SCLK)
    (add_net SDI)
    (add_net SDO)
    (add_net VIN_L)
    (add_net VIN_R)
    (add_net VOUT_L)
    (add_net VOUT_R)
    (add_net ZCEN)
  )
  (module w_conn_jst-ph:b5b-ph-kl (layer F.Cu) (tedit 56A52F1B)
    (at 50.2 58.2 90)
    (descr "JST PH series connector, B5B-PH-KL")
    (fp_text reference P5 (at 0 -2.99974 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 4.20116 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -4.00304 0 90) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 10 ZCEN))
    (pad 3 thru_hole oval (at 0 0 90) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 11 SDI))
    (pad 2 thru_hole oval (at -2.00152 0 90) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 12 CS))
    (pad 4 thru_hole oval (at 1.99898 0 90) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCLK))
    (pad 5 thru_hole oval (at 4.0005 0 90) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 14 MUTE))
    (model walter/conn_jst-ph/b5b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:soic-16 (layer F.Cu) (tedit 4F1AAE16)
    (at 67 58.6 270)
    (descr "SOIC Wide, 16 pins")
    (fp_text reference U1 (at 0 -1.016 270) (layer F.SilkS))
    (fp_text value PGA2311 (at 0 1.016 270) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 10 ZCEN))
    (pad 2 smd rect (at -3.175 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 12 CS))
    (pad 3 smd rect (at -1.905 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 11 SDI))
    (pad 4 smd rect (at -0.635 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 1 +5VD))
    (pad 5 smd rect (at 0.635 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_D))
    (pad 6 smd rect (at 1.905 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 13 SCLK))
    (pad 7 smd rect (at 3.175 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 15 SDO))
    (pad 8 smd rect (at 4.445 4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 14 MUTE))
    (pad 9 smd rect (at 4.445 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 6 VIN_R))
    (pad 10 smd rect (at 3.175 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 11 smd rect (at 1.905 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 7 VOUT_R))
    (pad 12 smd rect (at 0.635 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 13 smd rect (at -0.635 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 4 -5V))
    (pad 14 smd rect (at -1.905 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 9 VOUT_L))
    (pad 15 smd rect (at -3.175 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 16 smd rect (at -4.445 -4.81076 270) (size 0.55118 1.43002) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN_L))
    (model walter/smd_dil/soic-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 56A52F29)
    (at 74.5 38)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference P1 (at 0 -5.842) (layer F.SilkS) hide)
    (fp_text value VIN_R (at 0 5.842) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 6 VIN_R))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 56A52F08)
    (at 85.5 78 180)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference P2 (at 0 -5.842 180) (layer F.SilkS) hide)
    (fp_text value VOUT_R (at 0 5.842 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 7 VOUT_R))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 56A52F2C)
    (at 85.5 38)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference P3 (at 0 -5.842) (layer F.SilkS) hide)
    (fp_text value VIN_L (at 0 5.842) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 8 VIN_L))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 56A52F06)
    (at 74.5 78 180)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference P4 (at 0 -5.842 180) (layer F.SilkS) hide)
    (fp_text value VOUT_L (at 0 5.842 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 9 VOUT_L))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 56A52F18)
    (at 53 45.5 90)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference P8 (at 0 -5.842 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 5.842 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5VD))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND_D))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 49047394)
    (at 60 59 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C2 (at 0 -0.9906 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 +5VD))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_D))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 49047394)
    (at 74.2 56.7 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C3 (at 0 -0.9906 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 4 -5V))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_tant_C (layer F.Cu) (tedit 4D5D91B9)
    (at 79.3 56.9)
    (descr "SMT capacitor, tantalum size C")
    (fp_text reference C4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.0955) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 2 smd rect (at -2.52476 0) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 4 -5V))
    (model walter/smd_cap/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 49047394)
    (at 74.2 60.9 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C5 (at 0 -0.9906 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_tant_C (layer F.Cu) (tedit 4D5D91B9)
    (at 79.3 60.9 180)
    (descr "SMT capacitor, tantalum size C")
    (fp_text reference C6 (at 0 -2.159 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.0955 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at -2.52476 0 180) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (model walter/smd_cap/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_1206 (layer F.Cu) (tedit 50CDAAE4)
    (at 51 74.5 180)
    (descr "SMD LED, 1206")
    (fp_text reference D1 (at 0.0222 -1.6746 180) (layer F.SilkS))
    (fp_text value LED (at -0.054 1.602 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_D))
    (pad 2 smd rect (at 1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (model walter/smd_leds/led_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_1206 (layer F.Cu) (tedit 50CDAAE4)
    (at 95.1 70.3 180)
    (descr "SMD LED, 1206")
    (fp_text reference D2 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value LED (at -0.023 1.7962 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 2 smd rect (at 1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model walter/smd_leds/led_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_1206 (layer F.Cu) (tedit 50CDAAE4)
    (at 95 66.8 180)
    (descr "SMD LED, 1206")
    (fp_text reference D3 (at 0 -1.651 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.80086 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 4 -5V))
    (pad 2 smd rect (at 1.74752 0 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad2)"))
    (model walter/smd_leds/led_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_1 (layer F.Cu) (tedit 4B90E035)
    (at 50.5 66)
    (descr "Pin strip 1pin")
    (tags "CONN DEV")
    (fp_text reference P6 (at 0 -2.159) (layer F.SilkS))
    (fp_text value SDO_TO_OTHER_PGA2311 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 SDO))
    (model walter/pin_strip/pin_strip_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_1210 (layer F.Cu) (tedit 49047434)
    (at 51 70.5 180)
    (descr "SMT resistor, 1210")
    (fp_text reference R1 (at -0.0286 -0.0612 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.7018 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 +5VD))
    (model walter/smd_resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_1210 (layer F.Cu) (tedit 49047434)
    (at 88.8 70.6 180)
    (descr "SMT resistor, 1210")
    (fp_text reference R2 (at -0.0238 0.0134 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.7018 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model walter/smd_resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_1210 (layer F.Cu) (tedit 49047434)
    (at 88.9 67.3 180)
    (descr "SMT resistor, 1210")
    (fp_text reference R3 (at 0.0762 -0.0608 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.7018 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 3 GND_A))
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad2)"))
    (model walter/smd_resistors/r_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mechanical:3.5mm_m3 (layer F.Cu) (tedit 56A52F24)
    (at 51 80)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value 3.5mmM3 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.1) (size 5 5) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module mechanical:3.5mm_m3 (layer F.Cu) (tedit 56A52F0D)
    (at 95 80)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value 3.5mmM3 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.1) (size 5 5) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module mechanical:3.5mm_m3 (layer F.Cu) (tedit 56A52F10)
    (at 95 36)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value 3.5mmM3 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.1) (size 5 5) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module mechanical:3.5mm_m3 (layer F.Cu) (tedit 56A52F15)
    (at 51 36)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value 3.5mmM3 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.1) (size 5 5) (drill 3.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module w_smd_cap:c_tant_C (layer F.Cu) (tedit 4D5D91B9)
    (at 57 59 90)
    (descr "SMT capacitor, tantalum size C")
    (fp_text reference C1 (at 0 -2.159 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.0955 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 2.52476 0 90) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 1 +5VD))
    (pad 2 smd rect (at -2.52476 0 90) (size 2.55016 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 2 GND_D))
    (model walter/smd_cap/c_tant_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Connections_Bridges:WireConnection_0-8mmDrill (layer F.Cu) (tedit 56A52F20)
    (at 72 69 180)
    (descr "WireConnection with 0.8mm drill")
    (fp_text reference "" (at 4.8514 0.2032 180) (layer F.SilkS))
    (fp_text value JUMPER (at 5.08 3.81 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND_D))
  )
  (module mechanical:mors_3p_inv_pins (layer F.Cu) (tedit 56A52F2F)
    (at 93.6 57.7 270)
    (descr "Terminal block 3 pins")
    (tags DEV)
    (fp_text reference P7 (at 0 -5.842 270) (layer F.SilkS) hide)
    (fp_text value "" (at 0 5.842 270) (layer F.SilkS))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 4 -5V))
    (pad 2 thru_hole circle (at 0 0 270) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND_A))
    (pad 1 thru_hole circle (at 5.08 0 270) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model walter/conn_screw/mors_3p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text R (at 88.165 81.4872) (layer B.SilkS))
  (gr_text G (at 72.1136 81.3102) (layer B.SilkS))
  (gr_text L (at 76.8418 81.08) (layer B.SilkS))
  (gr_text G (at 82.878 81.4094) (layer B.SilkS))
  (gr_text +5V (at 60.35 47.95) (layer B.SilkS))
  (gr_text GND (at 60.45 42.475) (layer B.SilkS))
  (gr_text GND (at 60.45 42.475) (layer F.SilkS))
  (gr_text +5V (at 60.35 47.95) (layer F.SilkS))
  (gr_text +5V (at 85.625 62.925) (layer B.SilkS))
  (gr_text GND (at 86 57.875) (layer B.SilkS))
  (gr_text -5V (at 86.2 52.75) (layer B.SilkS))
  (gr_text G (at 68.075 73.325) (layer F.SilkS))
  (gr_text G (at 81.1 70) (layer F.SilkS))
  (gr_text L (at 78.95 70.05) (layer F.SilkS))
  (gr_text R (at 91.975 73.275) (layer F.SilkS))
  (gr_text L (at 81.875 45.95) (layer F.SilkS))
  (gr_text R (at 70.525 45.925) (layer F.SilkS))
  (gr_text G (at 78.025 45.975) (layer F.SilkS))
  (gr_text G (at 89.45 45.825) (layer F.SilkS))
  (gr_text GND (at 86 57.85) (layer F.SilkS))
  (gr_text +5V (at 85.65 62.9) (layer F.SilkS))
  (gr_text -5V (at 86.2 52.75) (layer F.SilkS))
  (gr_text "Ground plane connect" (at 67 67.4) (layer B.SilkS))
  (gr_text "Ground plane connect" (at 67 67.4) (layer F.SilkS))
  (gr_text MUTE (at 54.4 54.2 180) (layer F.SilkS))
  (gr_text SCLK (at 54.6 56 180) (layer F.SilkS))
  (gr_text SDI (at 54.2 58.2 180) (layer B.SilkS))
  (gr_text CS (at 54 60.2 180) (layer F.SilkS))
  (gr_text zcen (at 54.4 62.2 180) (layer F.SilkS))
  (gr_text SDO (at 53.25 66.75 180) (layer B.SilkS))
  (gr_text SDO (at 53.25 66.75 180) (layer F.SilkS))
  (gr_text MUTE (at 54.4 54.2 180) (layer B.SilkS))
  (gr_text SCLK (at 54.6 56 180) (layer B.SilkS))
  (gr_text SDI (at 54.2 58.2 180) (layer F.SilkS))
  (gr_text CS (at 54 60.2 180) (layer B.SilkS))
  (gr_text zcen (at 54.4 62.2 180) (layer B.SilkS))
  (gr_line (start 48.166 32.908) (end 48.166 82.908) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.166 32.908) (end 98.166 32.908) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.166 82.908) (end 98.166 82.908) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.166 32.908) (end 98.166 82.908) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND_D) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.625 33.075) (xy 66.475 82.75) (xy 48.325 82.75) (xy 48.425 33.35) (xy 66.575 33.2)
        (xy 66.575 33.2)
      )
    )
  )
  (zone (net 3) (net_name GND_A) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.975 33.275) (xy 67.8 82.625) (xy 97.675 82.425) (xy 97.675 33.175) (xy 67.875 33.375)
      )
    )
  )
  (zone (net 2) (net_name GND_D) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.625 33.4) (xy 66.45 82.45) (xy 48.225 82.7) (xy 48.45 33.525) (xy 66.775 33.225)
        (xy 66.55 33.225)
      )
    )
  )
  (zone (net 3) (net_name GND_A) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.925 82.6) (xy 67.825 33.1) (xy 97.875 33.1) (xy 97.875 82.55) (xy 67.825 82.6)
      )
    )
  )
)
