(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "+3V3")
  (net 5 "Net-(C6-Pad2)")
  (net 6 "RESET")
  (net 7 "CLK")
  (net 8 "MOSI")
  (net 9 "MISO")
  (net 10 "unconnected-(IC1-Pad9)")
  (net 11 "+5V")
  (net 12 "+BATT")
  (net 13 "VBUS")
  (net 14 "TX_LED")
  (net 15 "Net-(D1-Pad2)")
  (net 16 "RX_LED")
  (net 17 "Net-(D2-Pad2)")
  (net 18 "Net-(D4-Pad2)")
  (net 19 "Net-(F1-Pad1)")
  (net 20 "D+")
  (net 21 "D-")
  (net 22 "unconnected-(IC1-Pad10)")
  (net 23 "unconnected-(IC2-Pad5)")
  (net 24 "unconnected-(J1-Pad1)")
  (net 25 "unconnected-(J1-Pad8)")
  (net 26 "3.3V_SD_CS")
  (net 27 "3.3V_MOSI")
  (net 28 "3.3V_CLK")
  (net 29 "unconnected-(J1-Pad9)")
  (net 30 "MotorInputThree")
  (net 31 "Net-(J6-PadA5)")
  (net 32 "unconnected-(J6-PadA8)")
  (net 33 "Net-(J6-PadB5)")
  (net 34 "unconnected-(IC1-Pad11)")
  (net 35 "unconnected-(IC1-Pad12)")
  (net 36 "unconnected-(IC1-Pad13)")
  (net 37 "unconnected-(IC1-Pad14)")
  (net 38 "unconnected-(IC1-Pad15)")
  (net 39 "unconnected-(IC1-Pad16)")
  (net 40 "unconnected-(IC2-Pad4)")
  (net 41 "unconnected-(PS1-Pad4)")
  (net 42 "unconnected-(J6-PadB8)")
  (net 43 "unconnected-(J6-PadS1)")
  (net 44 "unconnected-(J6-PadS2)")
  (net 45 "SD_CS")
  (net 46 "CarBatt")
  (net 47 "unconnected-(J6-PadS3)")
  (net 48 "unconnected-(U1-Pad32)")
  (net 49 "unconnected-(U1-Pad31)")
  (net 50 "unconnected-(U1-Pad30)")
  (net 51 "unconnected-(U1-Pad29)")
  (net 52 "unconnected-(U1-Pad27)")
  (net 53 "unconnected-(U1-Pad26)")
  (net 54 "unconnected-(U1-Pad25)")
  (net 55 "unconnected-(U1-Pad21)")
  (net 56 "unconnected-(U1-Pad20)")
  (net 57 "unconnected-(U1-Pad41)")
  (net 58 "unconnected-(U1-Pad40)")
  (net 59 "Net-(R4-Pad1)")
  (net 60 "unconnected-(J6-PadS4)")
  (net 61 "Net-(R2-Pad1)")
  (net 62 "Net-(R3-Pad1)")
  (net 63 "Net-(R12-Pad1)")
  (net 64 "Net-(R15-Pad1)")
  (net 65 "Net-(C3-Pad2)")
  (net 66 "unconnected-(U1-Pad1)")
  (net 67 "MotorInputOne")
  (net 68 "MotorInputTwo")
  (net 69 "SDA")
  (net 70 "SCL")
  (net 71 "unconnected-(D5-Pad2)")
  (net 72 "Net-(D5-Pad4)")
  (net 73 "NeoPixel")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.4 73.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "SCL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.4 54.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5.1k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(J6-PadA5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.6 73.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 104.1 74.1)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 104.1 50.1)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.2 63.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-642CDAA2" (layer "F.Cu")
    (tedit 642CDAA2)
    (at 65.7 54.5)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjEuMjUiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiUFAgMS41XHJcbiIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI1IiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICI1IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNSIsICJQYWRkaW5nVG9wQ3RybCI6ICI1IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-642CDAA2" (at 0 -4.139665) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.139665) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6 64.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.4 56.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "5.1k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(J6-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 85.9 68.44 -90)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2.45 90) (layer "F.SilkS") hide)
    (fp_text value "Crystal_GND24" (at 0 2.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 -0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85 270) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.3 73.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.3 69.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.6 71 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm" (layer "F.Cu")
    (tedit 63F6A688)
    (at 78.9 71.2 180)
    (descr "TSSOP, 16 Pin (Allegro A4954 https://www.allegromicro.com/-/media/Files/Datasheets/A4954-Datasheet.ashx), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Arrow Part Number" "CD74HC4050PW")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/cd74hc4050pw/texas-instruments?region=nac")
    (property "Description" "High Speed CMOS Logic Hex Non-Inverting Buffers")
    (property "Height" "1.2")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_Part_Number" "CD74HC4050PW")
    (property "Mouser Part Number" "595-CD74HC4050PW")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/CD74HC4050PW?qs=ZA235jQDfbrcxB7kYB6RDA%3D%3D")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC1" (at 0 -3.45) (layer "F.SilkS") hide)
    (fp_text value "CD74HC4050PW" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.875 -2.275 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pinfunction "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at -2.875 -1.625 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "3.3V_SD_CS") (pinfunction "1Y") (pintype "passive"))
    (pad "3" smd roundrect (at -2.875 -0.975 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "SD_CS") (pinfunction "1A") (pintype "passive"))
    (pad "4" smd roundrect (at -2.875 -0.325 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "3.3V_MOSI") (pinfunction "2Y") (pintype "passive"))
    (pad "5" smd roundrect (at -2.875 0.325 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "MOSI") (pinfunction "2A") (pintype "passive"))
    (pad "6" smd roundrect (at -2.875 0.975 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "3.3V_CLK") (pinfunction "3Y") (pintype "passive"))
    (pad "7" smd roundrect (at -2.875 1.625 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "CLK") (pinfunction "3A") (pintype "passive"))
    (pad "8" smd roundrect (at -2.875 2.275 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "9" smd roundrect (at 2.875 2.275 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "unconnected-(IC1-Pad9)") (pinfunction "4A") (pintype "passive+no_connect"))
    (pad "10" smd roundrect (at 2.875 1.625 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(IC1-Pad10)") (pinfunction "4Y") (pintype "passive+no_connect"))
    (pad "11" smd roundrect (at 2.875 0.975 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "unconnected-(IC1-Pad11)") (pinfunction "5A") (pintype "passive+no_connect"))
    (pad "12" smd roundrect (at 2.875 0.325 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "unconnected-(IC1-Pad12)") (pinfunction "5Y") (pintype "passive+no_connect"))
    (pad "13" smd roundrect (at 2.875 -0.325 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(IC1-Pad13)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "14" smd roundrect (at 2.875 -0.975 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "unconnected-(IC1-Pad14)") (pinfunction "6A") (pintype "passive+no_connect"))
    (pad "15" smd roundrect (at 2.875 -1.625 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "unconnected-(IC1-Pad15)") (pinfunction "6Y") (pintype "passive+no_connect"))
    (pad "16" smd roundrect (at 2.875 -2.275 180) (size 1.55 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "unconnected-(IC1-Pad16)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-8" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.1 61.1 -90)
    (descr "SOT, 8 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "INA219AxDCN" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.975 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "MotorInputTwo") (pinfunction "IN+") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 -0.325 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "MotorInputOne") (pinfunction "IN-") (pintype "input"))
    (pad "3" smd roundrect (at -1.1375 0.325 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.1375 0.975 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "VS") (pintype "power_in"))
    (pad "5" smd roundrect (at 1.1375 0.975 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "SCL") (pinfunction "SCL") (pintype "input"))
    (pad "6" smd roundrect (at 1.1375 0.325 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 1.1375 -0.325 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R12-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "8" smd roundrect (at 1.1375 -0.975 270) (size 1.325 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R15-Pad1)") (pinfunction "A1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 65.1 74.1)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.9 61.1 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 72.1 71.061424 180)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Arrow Part Number" "NCP161ASN330T1G")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/ncp161asn330t1g/on-semiconductor?region=nac")
    (property "Description" "ON SEMICONDUCTOR - NCP161ASN330T1G - Fixed LDO Voltage Regulator, 1.9V to 5.5V, 225mV drop, 3.3V/450mA out, SOT-23-5")
    (property "Height" "1.45")
    (property "Manufacturer_Name" "onsemi")
    (property "Manufacturer_Part_Number" "NCP161ASN330T1G")
    (property "Mouser Part Number" "863-NCP161ASN330T1G")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/onsemi/NCP161ASN330T1G?qs=vLWxofP3U2ze5zA%252BHmAd3w%3D%3D")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "PS1" (at 0 -2.4 180) (layer "F.SilkS") hide)
    (fp_text value "NCP161ASN330T1G" (at 0 2.4 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "IN") (pintype "input"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "unconnected-(PS1-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pinfunction "OUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.3 57.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "0" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(D5-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "NeoPixel") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.6 73.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm" (layer "F.Cu")
    (tedit 63F68EDA)
    (at 93.46 68.55 -90)
    (descr "QFN, 44 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/2512S.pdf#page=17), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.82 90) (layer "F.SilkS") hide)
    (fp_text value "ATmega32U4-MU" (at 0 4.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at 1 -1 270) (size 1.5 1.5) (layers "F.Paste") (roundrect_rratio 0.2380953333))
    (pad "" smd roundrect (at -1 1 270) (size 1.5 1.5) (layers "F.Paste") (roundrect_rratio 0.2380953333))
    (pad "" smd roundrect (at -1 -1 270) (size 1.5 1.5) (layers "F.Paste") (roundrect_rratio 0.2380953333))
    (pad "" smd roundrect (at 1 1 270) (size 1.5 1.5) (layers "F.Paste") (roundrect_rratio 0.2380953333))
    (pad "1" smd roundrect (at -3.3375 -2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "unconnected-(U1-Pad1)") (pinfunction "PE6") (pintype "bidirectional+no_connect"))
    (pad "2" smd roundrect (at -3.3375 -2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "UVCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -3.3375 -1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(R3-Pad1)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.3375 -1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R2-Pad1)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.3375 -0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "UGND") (pintype "passive"))
    (pad "6" smd roundrect (at -3.3375 0 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad2)") (pinfunction "UCAP") (pintype "passive"))
    (pad "7" smd roundrect (at -3.3375 0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "VBUS") (pinfunction "VBUS") (pintype "input"))
    (pad "8" smd roundrect (at -3.3375 1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "RX_LED") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.3375 1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "CLK") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.3375 2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "MOSI") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -3.3375 2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "MISO") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "NeoPixel") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "RESET") (pinfunction "~{RESET}") (pintype "input"))
    (pad "14" smd roundrect (at -1.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" smd roundrect (at -1 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" smd roundrect (at -0.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pinfunction "XTAL2") (pintype "output"))
    (pad "17" smd roundrect (at 0 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)") (pinfunction "XTAL1") (pintype "input"))
    (pad "18" smd roundrect (at 0.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "SCL") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 1 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "SDA") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 1.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "unconnected-(U1-Pad20)") (pinfunction "PD2") (pintype "bidirectional+no_connect"))
    (pad "21" smd roundrect (at 2 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "unconnected-(U1-Pad21)") (pinfunction "PD3") (pintype "bidirectional+no_connect"))
    (pad "22" smd roundrect (at 2.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "TX_LED") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 3.3375 2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "24" smd roundrect (at 3.3375 2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "AVCC") (pintype "power_in"))
    (pad "25" smd roundrect (at 3.3375 1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "unconnected-(U1-Pad25)") (pinfunction "PD4") (pintype "bidirectional+no_connect"))
    (pad "26" smd roundrect (at 3.3375 1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "unconnected-(U1-Pad26)") (pinfunction "PD6") (pintype "bidirectional+no_connect"))
    (pad "27" smd roundrect (at 3.3375 0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "unconnected-(U1-Pad27)") (pinfunction "PD7") (pintype "bidirectional+no_connect"))
    (pad "28" smd roundrect (at 3.3375 0 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "SD_CS") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.3375 -0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "unconnected-(U1-Pad29)") (pinfunction "PB5") (pintype "bidirectional+no_connect"))
    (pad "30" smd roundrect (at 3.3375 -1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "unconnected-(U1-Pad30)") (pinfunction "PB6") (pintype "bidirectional+no_connect"))
    (pad "31" smd roundrect (at 3.3375 -1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "unconnected-(U1-Pad31)") (pinfunction "PC6") (pintype "bidirectional+no_connect"))
    (pad "32" smd roundrect (at 3.3375 -2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U1-Pad32)") (pinfunction "PC7") (pintype "bidirectional+no_connect"))
    (pad "33" smd roundrect (at 3.3375 -2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R4-Pad1)") (pinfunction "~{HWB}/PE2") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 2.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "VCC") (pintype "passive"))
    (pad "35" smd roundrect (at 2 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "36" smd roundrect (at 1.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "MotorInputThree") (pinfunction "PF7") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 1 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "MotorInputTwo") (pinfunction "PF6") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 0.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "MotorInputOne") (pinfunction "PF5") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 0 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "CarBatt") (pinfunction "PF4") (pintype "bidirectional"))
    (pad "40" smd roundrect (at -0.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "unconnected-(U1-Pad40)") (pinfunction "PF1") (pintype "bidirectional+no_connect"))
    (pad "41" smd roundrect (at -1 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "unconnected-(U1-Pad41)") (pinfunction "PF0") (pintype "bidirectional+no_connect"))
    (pad "42" smd roundrect (at -1.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(C3-Pad2)") (pinfunction "AREF") (pintype "passive"))
    (pad "43" smd roundrect (at -2 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "44" smd roundrect (at -2.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "AVCC") (pintype "passive"))
    (pad "45" smd rect (at 0 0 270) (size 3.8 3.8) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6 61.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "22" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "D+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 98.675 75.5 -90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x12_Male" (at 0 30.27 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 13.97) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "+BATT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "MotorInputThree") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "MotorInputTwo") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "SCL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "SDA") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "RESET") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "SD_CS") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "MISO") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "MOSI") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "CLK") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3V3") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-63FD119E" (layer "F.Cu")
    (tedit 63FD119F)
    (at 103.9 68.8 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjAuNiIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJwd3IiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMTQiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjUiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICI1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjE0IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63FD119E" (at 0 -3.929187 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.929187 90) (layer "F.SilkS") hide)
  )
  (footprint "Connector_Card:microSD_HC_Hirose_DM3D-SF" (layer "F.Cu")
    (tedit 61D4C10C)
    (at 68.03 62.32 -90)
    (descr "Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)")
    (tags "Micro SD")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -0.025 -7.625 90) (layer "F.SilkS") hide)
    (fp_text value "Micro_SD_Card" (at -0.025 6.975 90) (layer "F.Fab"))
    (fp_text user "KEEPOUT" (at -0.725 -4.8 90) (layer "Cmts.User"))
    (fp_text user "KEEPOUT" (at -0.275 -0.525 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at -0.025 1.475 90) (layer "F.Fab"))
    (pad "1" smd rect (at 3.175 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "unconnected-(J1-Pad1)") (pinfunction "DAT2") (pintype "bidirectional+no_connect"))
    (pad "2" smd rect (at 2.075 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "3.3V_SD_CS") (pinfunction "DAT3/CD") (pintype "bidirectional"))
    (pad "3" smd rect (at 0.975 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "3.3V_MOSI") (pinfunction "CMD") (pintype "input"))
    (pad "4" smd rect (at -0.125 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd rect (at -1.225 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "3.3V_CLK") (pinfunction "CLK") (pintype "input"))
    (pad "6" smd rect (at -2.325 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "7" smd rect (at -3.425 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "MISO") (pinfunction "DAT0") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.525 5.35 270) (size 0.7 1.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "unconnected-(J1-Pad8)") (pinfunction "DAT1") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect (at -5.65 -3.875 270) (size 1.45 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(J1-Pad9)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "10" smd rect (at 5.575 -5.45 270) (size 1 1.55) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd rect (at 5.625 5.225 270) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd rect (at -5.975 -2.375 270) (size 0.8 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd rect (at -5.725 5.225 270) (size 1.3 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "11" smd rect (at 5.975 -3.025 270) (size 0.8 1.4) (layers "F.Cu" "F.Paste" "F.Mask"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 69.555 57.395)
          (xy 69.555 65.895)
          (xy 67.555 65.895)
          (xy 67.555 57.395)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 71.905 60.345)
          (xy 71.905 62.845)
          (xy 73.755 62.845)
          (xy 73.755 60.345)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98 72.7 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.1 61.8 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCad:Terminal_Block" (layer "F.Cu")
    (tedit 0)
    (at 92.06 50.91)
    (descr "5441537-3")
    (tags "Connector")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Female" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 2.475 -0.025) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "MotorInputThree") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "+BATT") (pinfunction "Pin_2") (pintype "passive"))
    (model "Z:/Uni/EE4951W/PCB Design/PowerProber V1.5/KiCad Library/Terminal Block/3D/TB002-500-02BE.stp"
      (offset (xyz -2.5 -4.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.3 73.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-63F8F3C2" (layer "F.Cu")
    (tedit 63F8F3C2)
    (at 88.6 70.8 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjAuNiIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJUWCIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIxNCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjc1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjE0IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63F8F3C2" (at 0 -3.929187 -90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.929187 -90) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.7 65.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm" (layer "F.Cu")
    (tedit 5AA4B285)
    (at 76.9 62.3 90)
    (descr "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
    (tags "LED RGB NeoPixel")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -3.5 90) (layer "F.SilkS") hide)
    (fp_text value "WS2812B" (at 0 4 90) (layer "F.Fab"))
    (fp_text user "1" (at -4.15 -1.6 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.45 -1.6 90) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd rect (at -2.45 1.6 90) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "unconnected-(D5-Pad2)") (pinfunction "DOUT") (pintype "output+no_connect"))
    (pad "3" smd rect (at 2.45 1.6 90) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "4" smd rect (at 2.45 -1.6 90) (size 1.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(D5-Pad4)") (pinfunction "DIN") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-63F8F2BE" (layer "F.Cu")
    (tedit 63F8F2BE)
    (at 82.6 65.6 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjAuNiIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJSWCIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI0MCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiMjAiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICIyMCIsICJQYWRkaW5nVG9wQ3RybCI6ICIxMCIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63F8F2BE" (at 0 -4.365749 -90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.365749 -90) (layer "F.SilkS") hide)
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 65.1 50.1)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 63FD0D3F)
    (at 101.5 69.3)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.2 67.74)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.3 70.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6 62.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "22" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "D-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.5 57.8)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "CarBatt") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "USB4105-GF-A:GCT_USB4105-GF-A" (layer "F.Cu")
    (tedit 63F67F13)
    (at 104.980489 62.1625 90)
    (property "MANUFACTURER" "GCT")
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm")
    (property "PARTREV" "A3")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J6" (at -1.825 -8.135 90) (layer "F.SilkS") hide)
    (fp_text value "USB4105-GF-A" (at 5.16 -6.635 90) (layer "F.Fab"))
    (fp_text user "PCB EDGE" (at 5.4 2.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -2.89 -3.68 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 2.89 -3.68 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "A1_B12" smd rect locked (at -3.2 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "A4_B9" smd rect locked (at -2.4 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(F1-Pad1)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "A5" smd rect locked (at -1.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(J6-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect locked (at -0.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "D+") (pinfunction "DP1") (pintype "bidirectional"))
    (pad "A7" smd rect locked (at 0.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "D-") (pinfunction "DN1") (pintype "bidirectional"))
    (pad "A8" smd rect locked (at 1.25 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(J6-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "B1_A12" smd rect locked (at 3.2 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "B4_A9" smd rect locked (at 2.4 -4.755 90) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(F1-Pad1)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "B5" smd rect locked (at 1.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(J6-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect locked (at 0.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "D+") (pinfunction "DP2") (pintype "bidirectional"))
    (pad "B7" smd rect locked (at -0.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "D-") (pinfunction "DN2") (pintype "bidirectional"))
    (pad "B8" smd rect locked (at -1.75 -4.755 90) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(J6-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "S1" thru_hole oval locked (at -4.32 -4.18 90) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J6-PadS1)") (pinfunction "SHELL_GND") (pintype "power_in+no_connect"))
    (pad "S2" thru_hole oval locked (at -4.32 0 90) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J6-PadS2)") (pinfunction "SHELL_GND") (pintype "power_in+no_connect"))
    (pad "S3" thru_hole oval locked (at 4.32 0 90) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J6-PadS3)") (pinfunction "SHELL_GND") (pintype "power_in+no_connect"))
    (pad "S4" thru_hole oval locked (at 4.32 -4.18 90) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 60 "unconnected-(J6-PadS4)") (pinfunction "SHELL_GND") (pintype "power_in+no_connect"))
    (model "Z:/Uni/EE4951W/PCB Design/PowerProber V1.5/KiCad Library/USB4105-GF-A/USB4105-GF-A.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7)
    (at 95.5 57.8 90)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "20V/0.5A/385Vf" (at 0 2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.65 0 90) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "VBUS") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.2 73.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.8 57.3 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "1M" (at 0 2.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.9625 0 180) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 68 "MotorInputTwo") (pintype "passive"))
    (pad "2" smd roundrect (at 2.9625 0 180) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 67 "MotorInputOne") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 63F8F323)
    (at 82 65.6125 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "RX_LED") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.5 60.9 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 86.2 60.9 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 97.9 59.4625 180)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "500mA" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "VBUS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.6 66.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.9 58.1)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 91.8 59.1 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Arrow Part Number" "KF50BD-TR")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/kf50bd-tr/stmicroelectronics?region=nac")
    (property "Description" "KF50BD-TR, Low Dropout Voltage Regulator, 500mA, 5.2 V +/-2%, -0.5  20 Vin, 8-Pin SOIC")
    (property "Height" "1.75")
    (property "Manufacturer_Name" "STMicroelectronics")
    (property "Manufacturer_Part_Number" "KF50BD-TR")
    (property "Mouser Part Number" "511-KF50BD-TR")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/KF50BD-TR?qs=FPrINEQeLwG6VKFjrTzTpg%3D%3D")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC2" (at 0 -3.4 90) (layer "F.SilkS") hide)
    (fp_text value "KF50BD-TR" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pinfunction "VOUT") (pintype "passive"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "unconnected-(IC2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "unconnected-(IC2-Pad5)") (pinfunction "INHIBIT") (pintype "passive+no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND_3") (pintype "passive"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND_4") (pintype "passive"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "+BATT") (pinfunction "VIN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 63F8F10C)
    (at 88.5 71.5875 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "TX_LED") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.5 68)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCad:Terminal_Block" (layer "F.Cu")
    (tedit 0)
    (at 72.15 50.9)
    (descr "5441537-3")
    (tags "Connector")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Female" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 2.475 -0.025) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 46 "CarBatt") (pinfunction "Pin_2") (pintype "passive"))
    (model "Z:/Uni/EE4951W/PCB Design/PowerProber V1.5/KiCad Library/Terminal Block/3D/TB002-500-02BE.stp"
      (offset (xyz -2.5 -4.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.8 60.9 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10uf" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.4 66.7 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 -270) (layer "F.SilkS") hide)
    (fp_text value "0.1uf" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCad:Terminal_Block" (layer "F.Cu")
    (tedit 0)
    (at 82.1 50.9)
    (descr "5441537-3")
    (tags "Connector")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Female" (at 2.475 -0.025) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 2.475 -0.025) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 67 "MotorInputOne") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.95 1.95) (drill 1.3) (layers *.Cu *.Mask)
      (net 68 "MotorInputTwo") (pinfunction "Pin_2") (pintype "passive"))
    (model "Z:/Uni/EE4951W/PCB Design/PowerProber V1.5/KiCad Library/Terminal Block/3D/TB002-500-02BE.stp"
      (offset (xyz -2.5 -4.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.6 72.2)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.9 66.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "0.1uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 80.6 61.1 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.9 56.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Senior_Design.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-642EFDC9" (layer "B.Cu")
    (tedit 642EFDC9)
    (at 84.7 70.6 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiTGVmdCIsICJDYXBMZWZ0Q2hvaWNlIjogIlsiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiXSIsICJGb250Q29tYm9Cb3giOiAiUXVpY2tzaWx2ZXJJdGFsaWMtT1Y5WjQiLCAiSGVpZ2h0Q3RybCI6ICIxLjI3IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlZJTlxyXG5HTkRcclxuTSBJTiAxXHJcbk0gSU4gMlxyXG5TQ0xcclxuU0RBXHJcblJFU0VUXHJcblNEX0NTXHJcbk1JU09cclxuTU9TSVxyXG5DTEtcclxuMy4zViIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI1IiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICI1IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNSIsICJQYWRkaW5nVG9wQ3RybCI6ICI1IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-642EFDC9" (at 0 18.017991 270) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -18.017991 270) (layer "B.SilkS") hide)
  )
  (footprint "kibuzzard-642CEEEC" (layer "B.Cu")
    (tedit 642CEEEC)
    (at 102.9 62.1 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjEuIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlBPV0VSUFJPQkVSIFYxLjUiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiNSIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiNSIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-642CEEEC" (at 0 3.921332 270) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -3.921332 270) (layer "B.SilkS") hide)
  )
  (footprint "kibuzzard-642EFC61" (layer "B.Cu")
    (tedit 642EFC61)
    (at 84.8 55.8 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiWyIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJRdWlja3NpbHZlckl0YWxpYy1PVjlaNCIsICJIZWlnaHRDdHJsIjogIjEuMjUiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiVklOXHJcblxyXG5NIElOIDFcclxuXHJcbk0gSU4gMlxyXG5cclxuTSBPVVRcclxuXHJcblZTWVNcclxuXHJcbkdORCIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIyMiIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiMjIiLCAiV2lkdGhDdHJsIjogIiJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-642EFC61" (at 0 17.947607 270) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -17.947607 270) (layer "B.SilkS") hide)
  )
  (footprint "LOGO" (layer "B.Cu")
    (tedit 0)
    (at 65.7 62.4 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "B.SilkS") hide)
  )
  (gr_arc (start 107.6 74.6) (mid 106.721321 76.721321) (end 104.6 77.6) (layer "Edge.Cuts") (width 0.5))
  (gr_line (start 104.6 46.6) (end 64.6 46.6) (layer "Edge.Cuts") (width 0.5))
  (gr_arc (start 61.6 49.6) (mid 62.478679 47.478679) (end 64.6 46.6) (layer "Edge.Cuts") (width 0.5))
  (gr_circle (center 65.1 74.1) (end 66.6 74.1) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_circle (center 104.1 50.1) (end 105.6 50.1) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_line (start 107.6 74.6) (end 107.6 49.6) (layer "Edge.Cuts") (width 0.5))
  (gr_arc (start 64.6 77.6) (mid 62.478679 76.721321) (end 61.6 74.6) (layer "Edge.Cuts") (width 0.5))
  (gr_circle (center 65.1 50.1) (end 66.6 50.1) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_line (start 64.6 77.6) (end 104.6 77.6) (layer "Edge.Cuts") (width 0.5))
  (gr_arc (start 104.6 46.6) (mid 106.72132 47.47868) (end 107.6 49.6) (layer "Edge.Cuts") (width 0.5))
  (gr_circle (center 104.1 74.1) (end 105.6 74.1) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_line (start 61.6 49.6) (end 61.6 74.6) (layer "Edge.Cuts") (width 0.5))
  (zone (net 67) (net_name "MotorInputOne") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.4 58.8)
        (xy 81.8 56.2)
        (xy 84.4 56)
      )
    )
  )
  (zone (net 68) (net_name "MotorInputTwo") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.8 58.8)
        (xy 87.2 58.8)
        (xy 85.3 56.3)
        (xy 87.8 55.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.6 53.8)
        (xy 88.1 54.9)
        (xy 81.3 54.9)
        (xy 79.6 53.8)
        (xy 79.6 46.8)
        (xy 89.6 46.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.49 43.67)
        (xy 108.88 79.5)
        (xy 60.42 80.26)
        (xy 57.83 43.29)
      )
    )
  )
)
