(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "HEMT Amplifier 300K Filter Box")
		(date "2024-05-23")
		(rev "V4.3.1")
		(company "SPLENDOR Collaboration")
		(comment 1 "Jadyn Anczarski | 2024")
		(comment 2 "KIPAC at Stanford and SLAC")
	)
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 50.810662 0)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND-D")
	(net 2 "unconnected-(J2-Pad2)")
	(net 3 "unconnected-(J2-Pad3)")
	(net 4 "unconnected-(J2-Pad6)")
	(net 5 "unconnected-(J2-Pad7)")
	(net 6 "Net-(J2-Pad5)")
	(net 7 "unconnected-(J3-Pad2)")
	(net 8 "unconnected-(J3-Pad11)")
	(net 9 "unconnected-(J3-Pad13)")
	(net 10 "unconnected-(J3-P15-Pad15)")
	(net 11 "unconnected-(J3-P24-Pad24)")
	(net 12 "unconnected-(J5-Pad2)")
	(net 13 "unconnected-(J5-Pad3)")
	(net 14 "unconnected-(J5-Pad6)")
	(net 15 "unconnected-(J5-Pad7)")
	(net 16 "/Vdd1+(2)")
	(net 17 "/GND-S")
	(net 18 "/INJ (2)")
	(net 19 "/Vdd1+(1)")
	(net 20 "/INJ (1)")
	(net 21 "/OUT-(2)")
	(net 22 "/OUT+(2)")
	(net 23 "/DETBIAS-(2)")
	(net 24 "/DETBIAS+(2)")
	(net 25 "/Vgg2+(2)")
	(net 26 "/OUT-(1)")
	(net 27 "/DETBIAS-(1)")
	(net 28 "/OUT+(1)")
	(net 29 "/DETBIAS+(1)")
	(net 30 "/Vgg2+(1)")
	(net 31 "/Vdd2+(1)")
	(net 32 "/Vdd1+(2) ")
	(net 33 "/Vgg1+(2)")
	(net 34 "/Vdd1-(1) ")
	(net 35 "/Vgg2+(1) ")
	(net 36 "/Vdd1+(1) ")
	(net 37 "/Vdd1-(2) ")
	(net 38 "/Vgg2+(2) ")
	(net 39 "/Vgg1+(1)")
	(net 40 "/DETBIAS+(1) ")
	(net 41 "/OUT+(2) ")
	(net 42 "/DETBIAS+(2) ")
	(net 43 "/Vgg1+(1) ")
	(net 44 "/DETBIAS-(1) ")
	(net 45 "/DETBIAS-(2) ")
	(net 46 "/Vdd2-(2) ")
	(net 47 "/OUT+(1) ")
	(net 48 "/Vdd2-(1) ")
	(net 49 "/Vdd2+(1) ")
	(net 50 "/Vdd2+(2) ")
	(net 51 "/Vgg1+(2) ")
	(net 52 "/OUT-(2) ")
	(net 53 "/OUT-(1) ")
	(net 54 "Net-(C67-Pad2)")
	(net 55 "Net-(C61-Pad1)")
	(net 56 "Net-(C61-Pad2)")
	(net 57 "Net-(C55-Pad1)")
	(net 58 "Net-(C55-Pad2)")
	(net 59 "Net-(C53-Pad2)")
	(net 60 "Net-(C49-Pad2)")
	(net 61 "Net-(C15-Pad2)")
	(net 62 "Net-(C13-Pad2)")
	(net 63 "Net-(C11-Pad2)")
	(net 64 "Net-(C10-Pad2)")
	(net 65 "Net-(C33-Pad2)")
	(net 66 "Net-(C33-Pad1)")
	(net 67 "Net-(C7-Pad1)")
	(net 68 "Net-(C3-Pad1)")
	(net 69 "Net-(C1-Pad1)")
	(net 70 "Net-(C31-Pad2)")
	(net 71 "Net-(C5-Pad1)")
	(net 72 "Net-(C27-Pad2)")
	(net 73 "Net-(C1-Pad2)")
	(net 74 "Net-(C3-Pad2)")
	(net 75 "Net-(C5-Pad2)")
	(net 76 "Net-(C7-Pad2)")
	(net 77 "Net-(C67-Pad1)")
	(net 78 "Net-(C10-Pad1)")
	(net 79 "Net-(C15-Pad1)")
	(net 80 "Net-(C13-Pad1)")
	(net 81 "Net-(C11-Pad1)")
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 203.635662 101.95 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 48 "/Vdd2-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 159.723162 104.5 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 55 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 56 "Net-(C61-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 170.398162 114.65 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 57 "Net-(C55-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 58 "Net-(C55-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 217.635662 113.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 181.073162 78.5 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C70"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 41 "/OUT+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 182.135662 118.05 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 40 "/DETBIAS+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 217.635662 103.525 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 79 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 61 "Net-(C15-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 213.135662 113.55 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 60 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.310662 76.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 68 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 72 "Net-(C27-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 198.310662 83.475 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 50 "/Vdd2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 208.635662 112.55 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 60 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 234.723162 117.95 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 36 "/Vdd1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 230.810662 76.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 69 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 37 "/Vdd1-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 222.898162 74.6 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 69 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 73 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 208.310662 72.5 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 51 "/Vgg1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 213.310662 78.5 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 72 "Net-(C27-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 200.135662 114.55 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 81 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 63 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 239.723162 113 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 34 "/Vdd1-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 176.223162 108 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C65"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 47 "/OUT+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 217.810662 76.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 69 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 234.898162 78.1 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 37 "/Vdd1-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 202.810662 83.975 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 50 "/Vdd2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 153.073162 84.975)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 23 "/DETBIAS-(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 65 "Net-(C33-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 181.310662 83.975)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 6 "Net-(J2-Pad5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 75 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 217.635662 116.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 19 "/Vdd1+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 64 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 191.223162 76.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 68 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 167.723162 103)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 56 "Net-(C61-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 53 "/OUT-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 224.810662 89.5 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 38 "/Vgg2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 212.810662 73 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 51 "/Vgg1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 181.573162 73 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C71"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 52 "/OUT-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 239.723162 118.5 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 36 "/Vdd1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 220.810662 84.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 67 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 70 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 163.985662 73.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 21 "/OUT-(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 54 "Net-(C67-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 239.398162 78.55 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 37 "/Vdd1-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 239.398162 73.05 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 32 "/Vdd1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 154.985662 106.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 28 "/OUT+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 55 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 203.898162 120)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 20 "/INJ (1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 43 "/Vgg1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 216.310662 85 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 67 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 76 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 162.485662 85.975 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 66 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 65 "Net-(C33-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 178.048162 116.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 57 "Net-(C55-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 40 "/DETBIAS+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 227.398162 74.55 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 69 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 73 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 220.810662 88)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 76 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 38 "/Vgg2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 212.635662 119.05 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 43 "/Vgg1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 191.548162 116.575)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 39 "/Vgg1+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 63 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 207.810662 87)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 25 "/Vgg2+(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 76 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 173.573162 75 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C67"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 77 "Net-(C67-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 54 "Net-(C67-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 169.985662 89.475 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 42 "/DETBIAS+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 176.723162 102.5 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C64"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 53 "/OUT-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 217.810662 73.1)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 16 "/Vdd1+(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 73 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 207.810662 83.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 67 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 208.135662 118.05 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 43 "/Vgg1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 185.573162 79 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C69"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "/OUT+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 190.135662 104.45 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 80 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 62 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.310662 116.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 29 "/DETBIAS+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 57 "Net-(C55-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 213.135662 103.525 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 79 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 61 "Net-(C15-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 169.073162 75 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C68"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 77 "Net-(C67-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 54 "Net-(C67-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 185.635662 104.45 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 80 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 62 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 220.635662 105.525)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 79 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 59 "Net-(C53-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 195.635662 114.55 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 81 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 63 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 199.135662 101.45 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 48 "/Vdd2-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 186.310662 85.475 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 71 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 75 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 229.635662 101.525 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 35 "/Vgg2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 158.073162 85.975 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 66 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 65 "Net-(C33-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.310662 113.15)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 27 "/DETBIAS-(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 58 "Net-(C55-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 176.985662 77.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 77 "Net-(C67-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 41 "/OUT+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 181.223162 87.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 71 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:MILL-MAX_830-10-006-10-005000"
		(layer "F.Cu")
		(at 135.310662 79.5 90)
		(property "Reference" "J6"
			(at -3.075 -2.885 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BNC_IN_1"
			(at -2.429 2.286 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Library:MILL-MAX_830-10-006-10-005000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 202.810662 89.475 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 46 "/Vdd2-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.985662 84.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 65 "Net-(C33-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 45 "/DETBIAS-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 167.723162 106.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 55 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 47 "/OUT+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 152.985662 88.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 24 "/DETBIAS+(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 66 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 194.548162 102.45)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 80 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 48 "/Vdd2-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lib:MILL-MAX_830-10-006-10-005000"
		(layer "F.Cu")
		(at 145.810662 79.5 90)
		(property "Reference" "J1"
			(at -3.075 -2.885 90)
			(layer "F.SilkS")
		)
		(property "Value" "BNC_IN_2"
			(at -2.413 2.286 90)
			(layer "F.Fab")
		)
		(property "Footprint" "lib:MILL-MAX_830-10-006-10-005000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/DETBIAS+(2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/DETBIAS-(2)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/OUT+(2)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/OUT-(2)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/INJ (2)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 174.985662 84.475 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 45 "/DETBIAS-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 172.223162 102 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C63"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 53 "/OUT-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 182.635662 112.55 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 44 "/DETBIAS-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 163.985662 77.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 22 "/OUT+(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 77 "Net-(C67-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 194.548162 105.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 62 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 49 "/Vdd2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 155.810662 73.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 18 "/INJ (2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 51 "/Vgg1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.048162 116.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 63 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 43 "/Vgg1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 181.635662 102.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 80 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 229.135662 107.025 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 59 "Net-(C53-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 196.310662 74.5 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 68 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 74 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 194.223162 83.975)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 75 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 50 "/Vdd2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 230.635662 113.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 34 "/Vdd1-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.223162 73)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 74 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 51 "/Vgg1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 175.135662 114.65 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 57 "Net-(C55-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 58 "Net-(C55-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 186.635662 118.55 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 40 "/DETBIAS+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 164.223162 104.5 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 55 "Net-(C61-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 56 "Net-(C61-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 171.723162 107.5 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C66"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 47 "/OUT+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 174.485662 89.975 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 42 "/DETBIAS+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 208.048162 105.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 79 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 154.985662 103)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 26 "/OUT-(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 56 "Net-(C61-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 198.635662 106.95 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 49 "/Vdd2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 176.985662 74)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 54 "Net-(C67-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 52 "/OUT-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 187.135662 113.05 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 44 "/DETBIAS-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 229.810662 84.5 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 70 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 220.548162 102.025)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 61 "Net-(C15-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 35 "/Vgg2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lib:MILL-MAX_830-10-006-10-005000"
		(layer "F.Cu")
		(at 146.310662 112 90)
		(property "Reference" "J4"
			(at -3.075 -2.885 -90)
			(layer "F.SilkS")
		)
		(property "Value" "BNC_IN_1"
			(at -2.429 2.286 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "lib:MILL-MAX_830-10-006-10-005000"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND-D")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/DETBIAS+(1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/DETBIAS-(1)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 1 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/OUT+(1)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 3 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/OUT-(1)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 5 0 90)
			(size 1.218 1.218)
			(drill 0.71)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/INJ (1)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 225.135662 101.025 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 35 "/Vgg2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 186.073162 73.5 90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C72"
			(at 0 -2.65 -90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 90)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 52 "/OUT-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 235.223162 112.5 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 34 "/Vdd1-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 226.223162 115 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 78 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 64 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 225.310662 84 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 70 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 190.810662 85.475 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 71 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 75 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 191.635662 113.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 17 "/GND-S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 81 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 165.898162 87.975)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 66 "Net-(C33-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 42 "/DETBIAS+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 194.223162 87.475)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 71 "Net-(C5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 46 "/Vdd2-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 178.135662 113.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 58 "Net-(C55-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 44 "/DETBIAS-(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 234.898162 72.55 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 32 "/Vdd1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 204.135662 113.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 81 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 60 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 221.723162 115 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 78 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 64 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 224.635662 106.55 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 59 "Net-(C53-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 211.810662 85 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 67 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 76 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 181.635662 106.45)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 31 "/Vdd2+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 62 "Net-(C13-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 170.485662 83.975 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 45 "/DETBIAS-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 200.810662 74.5 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 68 "Net-(C3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 74 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 191.223162 73.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 33 "/Vgg1+(2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 74 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 203.135662 107.475 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 49 "/Vdd2+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 208.310662 78 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 72 "Net-(C27-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 208.135662 102.025)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 30 "/Vgg2+(1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 61 "Net-(C15-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 229.310662 90 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 38 "/Vgg2+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 230.723162 117)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 64 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 36 "/Vdd1+(1) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 230.810662 73)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 73 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 32 "/Vdd1+(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1812_4532Metric"
		(layer "F.Cu")
		(at 198.310662 88.975 -90)
		(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -2.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 0 2.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_1812_4532Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 1 "GND-D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.05 0 270)
			(size 1.4 3.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.178571)
			(net 46 "/Vdd2-(2) ")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm"
		(layer "B.Cu")
		(at 58.810662 76 90)
		(descr "15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm")
		(property "Reference" "J2"
			(at -9.695 5.89 -90)
			(layer "B.SilkS")
		)
		(property "Value" "HARVARD_PS_2"
			(at -9.695 -8.73 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Female*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -9.695 -1.42 -90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Vdd1+(2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(J2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J2-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/Vgg1+(2)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pad5)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(J2-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J2-Pad7)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/Vgg2+(2)")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -1.385 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -4.155 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -6.925 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P111")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -9.695 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -12.465 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -15.235 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -18.005 -2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P15")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Vertical_P2.77x2.84mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lib:CONN_5747846-4_TYC"
		(layer "B.Cu")
		(at 265.159931 95 90)
		(tags "5747846-4 ")
		(property "Reference" "J3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DB25_F_Fridge"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "lib:CONN_5747846-4_TYC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Female*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at -16.6116 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/DETBIAS+(1) ")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -13.843 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J3-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -11.0744 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/Vdd1+(1) ")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.3058 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/Vgg1+(1) ")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -5.5372 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/Vdd2+(1) ")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -2.7686 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/OUT+(1) ")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/OUT+(2) ")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.7686 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/Vdd2+(2) ")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 5.5372 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/Vgg1+(2) ")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 8.3058 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/Vdd1+(2) ")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 11.0744 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J3-Pad11)")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 13.843 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/DETBIAS+(2) ")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 16.6116 -10.922 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(J3-Pad13)")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -15.2273 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/DETBIAS-(1) ")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -12.4587 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(J3-P15-Pad15)")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -9.6901 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/Vdd1-(1) ")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -6.9215 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/Vgg2+(1) ")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -4.1529 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/Vdd2-(1) ")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -1.3843 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/OUT-(1) ")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 1.3843 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/OUT-(2) ")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 4.1529 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/Vdd2-(2) ")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 6.9215 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/Vgg2+(2) ")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 9.6901 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/Vdd1-(2) ")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 12.4587 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J3-P24-Pad24)")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 15.2273 -8.0772 90)
			(size 1.651 1.651)
			(drill 1.143)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/DETBIAS-(2) ")
			(pinfunction "P25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at -23.6474 -9.4996 90)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole circle
			(at 23.6474 -9.4996 90)
			(size 3.302 3.302)
			(drill 3.302)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm"
		(layer "B.Cu")
		(at 93.310662 113.89 -90)
		(descr "15-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 33.3mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "15-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 33.3mm")
		(property "Reference" "J5"
			(at -9.695 5.89 90)
			(layer "B.SilkS")
		)
		(property "Value" "HARVARD_PS_1"
			(at -9.695 -8.73 90)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_Dsub:DSUB-15_Female_Vertical_P2.77x2.84mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Female*")
		(sheetname "Root")
		(sheetfile "hemt_board_filter_V4.3.1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -9.695 -1.42 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Vdd1+(1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J5-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/Vgg1+(1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/Vdd2+(1)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J5-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J5-Pad7)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/Vgg2+(1)")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -1.385 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -4.155 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -6.925 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P111")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -9.695 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P12")
			(pintype "passive")
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -12.465 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -15.235 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -18.005 -2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/GND-S")
			(pinfunction "P15")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Vertical_P2.77x2.84mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 42.810662 65)
		(end 42.810662 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 42.810662 125)
		(end 259 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259 125)
		(end 259 65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 259 65)
		(end 42.810662 65)
		(layer "Edge.Cuts")
	)
	(gr_text "KIPAC at STANFORD and SLAC\nSPLENDOR COLLABORATION\nHEMT AMPLIFIER 300K FILTER BOARD V4.3.1\nJADYN ANCZARSKI, MAY 2024"
		(at 43.317662 124.841 0)
		(layer "F.SilkS")
	)
	(gr_text "CHANNEL 1"
		(at 119.310662 119.5 90)
		(layer "F.SilkS")
	)
	(gr_text "CHANNEL 2"
		(at 118.810662 85 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND-D")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 40.810662 57) (xy 37.310662 129.5) (xy 272.810662 132.5) (xy 272.310662 67.5) (xy 271.810662 56.5)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/GND-S")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 33.030662 53.34) (xy 276.870662 53.34) (xy 276.870662 127) (xy 33.030662 127)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND-D")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 46.310662 42) (xy 33.810662 43) (xy 30.310662 133) (xy 278.310662 138) (xy 277.810662 45)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND-D")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 28.810662 34.5) (xy 281.810662 35.5) (xy 282.310662 145.5) (xy 24.310662 144.5)
			)
		)
	)
)
